IEEE P802.11
Wireless LANs

|  |
| --- |
| CC28 CR VHTz Protocol Clean Up |
| Date: 2018-09-10 |
| Author(s): |
| Name | Company | Address | Phone | Email |
| Christian Berger  | Marvell |  |  | crberger@marvell.com  |
|  |  |  |  |  |

**Abstract**

This submission proposes resolutions of comments received from TGaz CC28.

(The proposed change is based on TGaz Draft 0.4.1)

* CIDs: 405, 406, 407, 408, 413, 47, 48, 176, 409, 410, 411, 493, 415, 417, 414, 177, 49, 50, 178, 422, 423, 424, 426, 418, 419, 420, 421, 416, 179, 430, 428, 431, 432 (33 CIDs)

| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| --- | --- | --- | --- | --- | --- |
| 405 | 58 | 11.22.6.4.4.4 | "equalt to nonzero" | "nonzero" | Accepted |
| 406 | 58 | 11.22.6.4.4.4 | "protocoloperates" | Add space after "l" | Accepted |
| 407 | 59 | 11.22.6.4.4.1 | " the MaxToAAvailable value " -- where is this value defined? The field is the MaxToAAvailableExp | Clarify | RevisedAdded explanation that the MaxToaAvailableExp indicates a time marked MaxToaAvailable in Fig. |
| 408 | 59 | 11.22.6.4.4.1 | "for which the responder retains the computed ToA value. " -- what does this mean? | Clarify | RevisedRemoved sentence, kept normative behavior |
| 413 | 59 | 11.22.6.4.4.1 | Figure 11-xx is not referred to anywhere | Refer to figure in text | Accepted |
| 47 | 59 | 11.22.6.4.4.2 | NPDA and NDP PPDU format is defined in the previous and the paragraph after this statement. Should we define the LMR PDDU as SU PPDU (not ER SU PPDU?) explicitly or it's implicit anyway | As per comment | RevisedPPDU format defintions have been removed |
| 48 | 59 | 11.22.6.4.4.2 | Remove the phrase "operating at 2.4GHz and 5GHz bands" as VHTz is applicable to these bands anyway | As per comment | RevisedPPDU format defintions have been removed |
| 176 | 59 | 11.22.6.4.4.2 | Shouldn't the text here be mandatory behavior? | Change "use" to "shall use". | Revisedparagraph has been removed |
| 409 | 59 | 11.22.6.4.4.2 | Non-break space before units | Needed before GHz and us (which should be <micro>s), etc. | Revisedparagraph has been removed |
| 410 | 59 | 11.22.6.4.4.2 | This is a big lump of text | Split into bullets for the three (?) cases | Revisedparagraph has been removed |
| 411 | 59 | 11.22.6.4.4.2 | What happens for VHTz mode in other bands? | Clarify | Revisedparagraph has been removed |
| 493 | 59 | 11.22.6.4.4.2 | GI=0.8us is incorrect | change GI=0.8us to GI=1.6us everywhere | Revisedparagraph has been removed |
| 415 | 60 | 11.22.6.4.4.3 | This Figure 11-xx has a MinProcessingTime but this is not defined anywhere. Further, if the time to the next sounding sequence is more than this processing time, why can't the LMR be provided immediately after the first sounding sequence, as in the Figure 11-xx above? | Clarify | RevisedFigure 11-xx now uses “MinTimeBetweenMeasurements”, which is defined.The LMR can only be provided if the ISTA is available (could be off channel), the only way for the ISTA to signal availability is to initiate another measurement. |
| 417 | 60 | 11.22.6.4.4.3 | This Figure 11-xx refers to an "Empty LMR" but this is not defined anywhere. What does an Empty LMR consist of? | Clarify | AcceptedAdded clarification |
| 414 | 60 | 11.22.6.4.4.3 | There are 4 Figure 11-xxs in this subclause, but only one reference (to one of them) | Refer to all the figures in the text | AcceptedAdded reference to Figures in relevant places |
| 177 | 60 | 11.22.6.4.4.3 | This should be in other subcaluse | Move the sentence to the general part of VHTz ranging description | AcceptedMoved paragraph as requested |
| 49 | 60 | 11.22.6.4.4.3 | Change "field in an initial Fine Timing Measurement frame has expired"  | As per comment:to "field in the most recent initial Fine Timing Measurement frame has elapsed".' | AcceptedChanged wording |
| 50 | 60 | 11.22.6.4.4.3 | Change "an initial Fine Timing Measurement frame with the MinToAReady field value equal to a nonzero"  | As per comment:to "the most recent transmitted initial Fine Timing Measurement frame with the MinToAReady field value equal to a nonzero" | RevisedRewrote paragraph |
| 178 | 60 | 11.22.6.4.4.3 | The valid result may not be available, e.g. when the UL NDP is not received. | Fix the issue mentioned in the comment. | RevisedChanged wording to reflect the case where no valid ToA available |
| 422 | 60 | 11.22.6.4.4.3 | Again "equal to a nonzero" | "nonzero" | RevisedRewrote paragraph |
| 423 | 60 | 11.22.6.4.4.3 | "may not" is ambiguous | Change to "is not required to" | RevisedRewrote paragraph |
| 424 | 60 | 11.22.6.4.4.3 | What is a "valid" measurement result? How is it distinguished from an invalid one? Or does nothing get transmitted at all? | Clarify. Also at line 29 | RevisedRewrote paragraph |
| 426 | 60 | 11.22.6.4.4.3 | "is negotiated and agreed on during negotiation" -- these are the same thing, in baseline conventions | Delete "and agreed on during negotiation" throughout | AcceptedChanged wording accordingly |
| 418 | 60 | 11.22.6.4.4.3 | "The direction(s) of LMR feedback(s) is(are) negotiated at service establishment." -- so can be ISTA-to-RSTA only (unlike HEz)? | Clarify | RevisedRewrote/removed paragraph |
| 419 | 60 | 11.22.6.4.4.3 | "In both directions, LMR feedback is neither acknowledged" -- this follows from it being in Action No Ack frames | Delete, or change to a NOTE, referring to the use of Action No Ack frames | AcceptedNow refer to Acktion No Ack frame format |
| 420 | 60 | 11.22.6.4.4.3 | "LMR feedback is reported in the next sounding sequence. " but the Figures 11-xx indicate the LMR feedback is after the sounding sequence, not part of it | As it says in the comment | AcceptedReplaced sounding sequence with measurement exchange |
| 421 | 60 | 11.22.6.4.4.3 | What is the "sounding sequence" for VHTz? Is it the NDPA NDP NDP from Figure 11-xx in 11.22.6.4.4.2? | Clarify | AcceptedAdded language that defines “Sounding sequence”  |
| 416 | 60 | 11.22.6.4.4.3 | What is the point of having units "[ms]" if there are no numbers or other marks on the axis? | Delete in all cases | RevisedRemoved units |
| 179 | 61 | 11.22.6.4.4.3 | This is not IEEE language. | Fix the issue mentioned in the comment. | RevisedRewrote/removed paragraph |
| 430 | 61 | 11.22.6.4.4.3 | Spurious full stop | Delete one of them | AcceptedFixed typo |
| 428 | 61 | 11.22.6.4.4.3 | "TOA and TOD format " -- what is this? | Change "format" to "reporting". Ditto line 14 | RevisedRewrote/removed paragraph |
| 431 | 61 | 11.22.6.4.4.3 | Same comments re secured wording as for 11.22.6.4.3.4 | See comments on that subclause | AcceptedChanged wording accordingly |
| 432 | 61 | 11.22.6.4.4.3 | Same comments re secured wording as for 11.22.6.4.3.4 | See comments on that subclause | AcceptedChanged wording accordingly |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

***TGaz Editor: replace Section 11.22.6.4.4 with the following revised text, changes relative to draft 0.4.1***

* + - * 1. 11.22.6.4.4 Measurement Exchange in VHTz Mode

11.22.6.4.4.1 General

In VHTz mode, the protocol operates in an ISTA centric scheduling FTM mode (); whenever the medium is available, an ISTA may initiate the measurement exchange procedure. The RSTA can only limit the frequency with which the ISTA can initiate the measurement exchange, by setting a minimum time interval between subsequent range mesasurements.



Figure 11-xx VHTz Measurement Exchange Sequence

11.22.6.4.4.2 Measurement Exchange Sequence

The measurement exchange in VHTz mode shall follow the sequence illustrated in Figure 11-xx. The frame format of NDP-A, NDP, and LMR are defined in 9.3.1.20, 28.3.17a and 9.6.7.37, respectively.

For immediate feedback the LMR carries measurement results of this round, while for delayed feedback the LMR carries measurement results of previous round (see 11.22.6.4.4.3).

An ISTA shall not initiate a new measurement exchange sequence until the minimum time interval between subsequent range measurements, specified in the MinTimeBetweenMeasurements field in the VHTz Specific subelement subfield in the Ranging Parameters field in an initial Fine Timing Measurement frame, has elapsed (see Figure 11-xy).

In the VHTz mesurement exchange sequence, the ISTA shall transmit the NDP-A frame with the same bandwidth as the UL NDP to reserve the medium; the RSTA shall transmit the DL NDP with the same bandwidth as the NDP-A and UL NDP, while the LMR can be transmitted at any bandwidth not exceeding the bandwidth of the NDP-A, UL NPD and DL NDP. The allowed bandwidths are specified in the Format and Bandwidth subfield of the Ranging Parameters field (see 9.4.2.246).

Accordingly:

* An ISTA transmitting a Ranging NDP-A frame shall not use a bandwidth wider than that indicated by an RSTA in the Ranging Parameters element, in the initial Fine Timing Measurement frame. The TA field of the Ranging NDP Announcement frame is a bandwidth signalling TA when the Ranging NDP Announcement frame is sent in a non-HT duplicate PPDU (see 10.7.6.6)
* An ISTA transmitting an UL NDP shall set the TXVECTOR parameter CH\_BANDWIDTH to the same value as the TXVECTOR parameter CH\_BANDWIDTH in the preceding Ranging NDP-A frame.
* An RSTA transmitting a DL NDP shall set the TXVECTOR parameter CH\_BANDWIDTH to the bandwidth of the Ranging NDP-A frame and/or the UL NDP frame; which are obtained from the RXVECTOR parameter CH\_BANDWIDTH of the Ranging NDP-A frame or UL NDP frame respectively. For the NDP-A frame, when not received in an HE/VHT/HT PPDU from the RXVECTOR parameter CH\_BANDWIDTH\_IN\_NON\_HT when the Ranging NDP–A frame is received in a non-HT duplicate PPDU and is 20 MHz when the Ranging NDP-A frame is received in a non-HT PPDU.

11.22.6.4.4.3 Measurement Report

In VHTz mode, the ranging protocol supports both immediate and delayed reporting. In delayed reporting, the TOA feedback corresponding to the current sounding sequence is reported in the next measurement exchange, see Figures 11-xy and 11-xz, where “sounding sequence” refers to the NDP-A and UL/DL NDP frames. Delayed reporting is meant to give the RSTA enough processing time, in case some RSTA implementations cannot have the TOA measurements of the UL NDP ready in time to be included in the LMR of the same measurement exchange sequence. In this case, the LMR following the very first sounding sequence has no valid TOA to include, which in Figure 11-xy is termed and “Empty LMR” for illustrative purposes.

 

Figure 11-xy VHTz Immediate Reporting

 

Figure 11-xz VHTz Delayed Reporting

An RSTA indicates delayed reporting by setting the MinToaReady parameter in the VHTz Specific subelement in the Ranging Parameters field to a non-zero value. The RSTA then shall also set the MinTimeBetweenMeasurements to the same value as the MinToaReady parameter and set the MaxToaAvailableExp parameter in the VHTz Specific subelement to indicate a time value larger than MinToaReady.

An RSTA that indicated delayed reporting shall provide TOA feedback to the ISTA, if the ISTA initiates another measurement sequence after MinToaReady, but before MaxToaAvailable - the time indicated by the MaxToaAvailableExp parameter in the VHTz Specific subelement, see Figure 11-yx. This TOA feedback is carried in the LMR frame of this new measurement sequence and can be either valid or invalid as indicated by the invalid Measurement field in the LMR frame.



Figure 11-yx Illustration of MinToaReady and MaxToaAvailable for delayed reporting

If ISTA-to-RSTA LMR feedback is negotiated, the VHTz measurement exchange shall follow the sequence shown in Figure 11-yy. After SIFS time of receiving the RSTA-to-ISTA LMR frame, the ISTA shall transmit the ISTA-to-RSTA LMR frame to the RSTA. The feedback type of ISTA-to-RSTA LMR could be either immediate or delayed.

LMR feedback is carried in Action No Ack frames (see 9.6.7.37), and are therefore neither acknowledged nor retransmitted.



Figure 11-yy VHTz Measurement Exchange Sequence with Bidirectional LMR Feedbacks

The data rate or MCS used for transmitting the LMR frame is solely decided by the transmitter of the corresponding LMR frame. The bandwidth used to transmit the LMR frame shall not be wider than the bandwidth of the soliciting NDP-A.

In the secured mode of VHTz, if an RSTA receives the PHY-RXEND.indication(*IntegrityCheckError*) primitive, the RSTA shall set the Invalid Measurement field in the RSTA-to-ISTA LMR frame carrying the TOA measured from the UL NDP to 1. Correspondingly, if ISTA-to-RSTA LMR was negotiated between the ISTA and RSTA and the ISTA receives the PHY-RXEND.indication(*IntegrityCheckError*) primitive, the ISTA shall set the Invalid Measurement field in the ISTA-to-RSTA LMR carrying the TOA measured from the DL NDP to 1.

If the Invalid Measurement field in RSTA-to-ISTA LMR or ISTA-to-RSTA LMR is set to 1, the RSTA or ISTA receiving the LMR should discard the TOA carried in the LMR.