IEEE P802.11
Wireless LANs

|  |
| --- |
| OCV CIDs 2329, 2330 |
| Date: 2019-03-11 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Thomas Derham | Broadcom | 16340 W Bernardo Dr, San Diego CA 92127 |  | thomas.derham@broadcom.com |

Abstract

Addresses CIDs 2329 and 2330 on OCV.

CIDs:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed change** | **Resolution** |
| 2329 | 12.7.6.3 | 2628 | This list is an exclusive list, i.e. in any given situation only one of the bullets applies. Therefore this new OCI KDE bullet could cause conflicts with the other bullets | Change to "Additionally contains an OCI KDE at the end when [...]" | Accept |
| 2330 | 12.7.6.4 | 2630 | This list is an exclusive list, i.e. in any given situation only one of the bullets applies. Therefore this new OCI KDE bullet could cause conflicts with the other bullets | Change to "Additionally contains an OCI KDE at the end when [...]" | Accept |

**Discussion**

Commenter is correct that the existing bullets in Key Data description for 4-way messages 2 and 3 form an exclusive list, whereas the OCI is intended to be additionally added to KeyData when certain conditions are true. Therefore prefixing with “Additionally…” is a useful clarification.

**Instructions to the editor**

***Instruct the editor to modify Section 12.7.6.3 as follows:***

* Additionally, contains OCI KDE when dot11RSNAOperatingChannelValidationActivated on the Supplicant.(M58)

***Instruct the editor to modify Section 12.7.6.4 as follows:***

* Additionally, contains OCI KDE when dot11RSNAOperatingChannelValidationActivated on the Authenticator.(M58)