IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution for CID 20012 | | | | |
| Date: March 12, 2019 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Abhishek Patil | Qualcomm Inc. |  |  | appatil@qti.qualcomm.com |
| Alfred Asterjadhi | Qualcomm Inc. |  |  | aasterja@qti.qualcomm.com |
| George Cherian | Qualcomm Inc. |  |  | gcherian@qti.qualcomm.com |

Abstract

This submission proposes resolutions for CID 20012 received for TGax LB238

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Section** | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
| 20012 | Abhishek Patil | 9.4.1.9 | 123 | 28 | Status code 18 (REFUSED\_BASIC\_RATES\_MISMATCH) should be updated to include Basic HE MCS and NSS Set. | As in comment | **Revised**  Agree with the comment.  **TGax editor, please make changes as showing in 11-19/0479r0 with the tag CID 20012** |

* Status Code field

***TGax Editor: Please update entry corresponding to Status Code 18 as shown below***

Insert the following row in Table 9-52 (Status codes) maintaining numeric order and updating the reserved range:

|  |  |  |
| --- | --- | --- |
| * Status codes | | |
| Status code | Name | Meaning |
| 18 | REFUSED\_BASIC\_RATES\_MISMATCH | Association denied due to requesting STA not supporting all of the data rates in the BSSBasicRateSet parameter, the Basic HT-MCS Set field of the HT Operation parameter, or the Basic VHT-MCS and NSS Set field in the VHT Operation parameter[20012], or the Basic HE-MCS and NSS Set field in the HE Operation parameter. |
| 124(#ANA) | DENIED\_HE\_NOT\_SUPPORTED | Association denied because the requesting STA does not support HE features. |