### **IEEE P802.11Wireless LANs**

|  |
| --- |
| Comment Resolutions on Some BPSK-Mark Comments |
| Date: 2019-03-12 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Steve Shellhammer | Qualcomm |  |  | shellhammer@ieee.org |
|  |  |  |  |  |

**Abstract**

The document provides comment resolutions for CIDs: 2085 and 2669.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page/Line** | **Comment** | **Proposed Change** | **Resolution** |
| 2085 | 31.2.1 | 86.51 | Since 'BPSK-Mark' field is actually the repeat of L-SIG and it's identified by 11ax devices as 'RL-SIG' field, it's better to change 'BPSK-Mark' to 'RL-SIG'. | Change 'BPSK-Mark' to 'RL-SIG' in the whole standard | **Reject**The term RL-SIG is used in High Efficiency (HE) where there are four additional populated subcarriers. To avoid confusion with the term used in HE it makes sense to use a different term here. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page/Line** | **Comment** | **Proposed Change** | **Resolution** |
| 2669 | 31.2.5.5 | 95.8 | Multiple frequency segments not supported. Replace "Apply CSD for each transmit chain and frequency segment" with "Apply CSD for each transmit chain" | As shown in the comment | **Accept** |