IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for CID 3109 and 3145 | | | | |
| Date: 2019-07-10 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 2 Huntington Quad,  Melville, NY 11747  USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Joseph Levy |  |  |
| Rui Yang |  |  |

Abstract

This submission proposes resolutions for the following CIDs: 3109 and 3145.The baseline for this comment resolution document is 802.11ba Draft 3.0.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
| 3109 | Jeongki Kim | 9.4.2.298 | 65 | 27 | Recommended WUR Parameters Present subfield is used only by WUR non-AP STA and reserved in WUR AP. | Add the following text at the end of the indicated text: "The Recommended WUR Parameters Present subfield is reserved when the WUR Mode element is transmitted by a WUR AP." | Revised—  Agree in principle with the comment.  TGba editor, please add the following text at the end of the paragraph at page 65 line 29 “The Recommended WUR Parameters Present subfield is set to 0 when the WUR Mode element is transmitted by a WUR AP.” |
| 3145 | Joseph Levy | 9.4.2.297 | 63 | 33 | The description of the Counter subfield is vague and not specific. If the intent is to set the Counter subfield to be equal to the Counter subfield received in the last received WUR Wake-up frame, it should state so. The use of the word current is not clear. | Replace: "The Counter subfield indicates the current value of the Counter subfield included in the broadcast WUR Wake-up frames (see 29.5.3 (Transmitter ID))." With: "The Counter subfield is set to the Counter subfield in the last received WUR Wake-up frame (see 29.5.3 (Transmitter ID))." | Revised—  Agree with the comment that more clarification is needed to make clear that the counter field in the WUR Operation element is transmitted by the same AP that is transmitting the broadcast WUR frames.  TGba editor, please replace the following sentence at 63.33 “The Counter subfield indicates the current value of the Counter subfield included in the broadcast WUR Wake-up frames (see 29.5.3 (Transmitter ID))." with the following sentence “The Counter subfield indicates the current value of the Counter subfield included in the broadcast WUR Wake-up frames (see 29.5.3 (Transmitter ID)) that are transmitted by the same AP." |