IEEE P802.11
Wireless LANs

|  |
| --- |
| CRs on MCS Tables |
| Date: 2019-11-11 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Bin Tian | Qualcomm |  |  | btian@qti.qualcomm.com |

Abstract

This submission shows

* Resolution for a comment received from TGax comment collection (TGax Draft D5.0)
* The proposed changes are based on 11ax D5.0.

The submission provides resolutions to following

* 22291, 22292

Revisions:

* Rev 0: Initial version of the document.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 22291 | 705.36 | In Table 27-97--HE-MCSs for 996-tone RU and non-OFDMA 80 MHz, NSS = 2 the "1 134.3" should be "1 134.2" (cf. Table 27-104--HE-MCSs for non-OFDMA 160 MHz and 80+80 MHz, NSS = 1). The actual rate is 1134236111 bps | As it says in the comment | Reject10The data rate listed in the table is correct. Please see the following computation of the data rateNdpbs=10\*5/6\*2\*980=16333.3316333.33Actual data rate= Ndbps/(12.8+1.6)us=1134.259 which is round to 1134.3 in the table. |
| 22292 | 693.51 | In Table 27-79--HE-MCSs for 106-tone RU, NSS = 8, "225.0" should be "255.0". This is the exact rate | As it says in the comment | AcceptThis is a typo. The data rate should be 255 instead of 225 |