IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Draft Spec Text for Definition of tone rotation | | | | |
| Date: 2020-01-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Yujin Noh | NEWRACOM |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission contains spec text for 33.3.7.3 Definition of tone rotation in P802.11bd D0.1. The text reflects the related straw polls and motions passed in 11/19/1864 and 11-19/0514.

Revisions:

* Rev 0: Initial version of the document.

Discussion

After the decision by 11bd group, one among Equation (33-x5) and Equation (33-x6) will remain with revision 1.

***To TGbd Editor:*** *replace the current text with the proposed changes below.*

***------------- Begin Text Changes ---------------***

33.3.7.3 Definition of tone rotation

The function is used to represent a rotation of the tones. BW in is determined by the TXVECTOR parameter CH\_BANDWIDTH as defined in Table 33-xx (CH\_BANDWIDTH).

|  |  |
| --- | --- |
| Table 33-x4 CH\_BANDWIDTH and | |
| CH\_BANDWIDTH |  |
| CBW10 |   *k*  10   |
| CBW20 |   *k*  20   |

For a 10 MHz NGV PPDU transmission,

(33-x4)

For a 20 MHz NGV PPDU transmission, ~~tone rotation values are TBD.~~

(33-x5)

(33-x6)

***------------- End Text Changes ------------------***