IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolutions to 32.3.8.10 Midambles |
| Date: 2020-06-15 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Yujin Noh | Newracom |  |  | yujin.noh at newracom.com |
|  |  |  |  |  |

Abstract

This submission shows

* Resolutions for comments from TGbd draft 0.3
* 7 CIDs: 19, 122, 152, 153, 154, 202 and 341

Revisions:

* Rev 0: Initial version of the document.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 152 | 56.26 | "An NGV STA may include midambles ..". As Midamble is mandatory for NGV PPDU, need to change "may" to "shall". | change "An NGV STA may include midambles .." to "An NGV STA shall include midambles ... " | Revised.I agree that Midamble is a mandatory feature in 11bd. However, the spec still allows no midamble field in the PPDU depending on the number of data symbol and the Midamble Periodicity.TGbd Editor: make changes according to this document 11-20-0721-00-00bd Resolutions to 32.3.8.10 Midambles.  |
| 19 | 56.30 | We defined the three value for midamle peridicity and it is indicated by NGV-SIG field. | modify the following sentence like as" where M is either 4 or8 or 16 as indicated by the Midamble Periodicity field in NGV-SIG field." | Revised.TGbd Editor: make changes according to this document 11-20-0721-00-00bd Resolutions to 32.3.8.10 Midambles. |
| 122 | 56.30 | "Midambles are present in the Data field of the NGV PPDU every M OFDM symbols, where M is either 4 or <TBD> as indicated by the Midamble Periodicity field in <TBD>" Update "<TBD>" and rephrase. | Midambles are present in the Data field of the NGV PPDU after every M Data symbols, where M is 4, 8 or 16 as indicated by the Midamble Periodicity field in NGV-SIG. | Revised.The same resolution to CID19 is applied to CID122. |
| 153 | 56.31 | "where M is either 4 or<TBD> as indicated by the Midamble Periodicity field in <TBD>." Need to update the <TBD> based on the latest motion on Midamble periodicity. | As in the comment. | Revised.The same resolution to CID19 is applied to CID153. |
| 341 | 56.31 | remove TBD and correct the setence properly. M is 4, 8, or 16 as indicated by the Midamble Periodicity field in Table 32-10 | as in comment | Revised.The same resolution to CID19 is applied to CID341. |
| 154 | 56.34 | "Each midamble is the same format as the NGV-LTF field(s) in the preamble of the same PPDU as defined inClause 32.3.7.3.6 (NGV-LTF definition), as shown", the description can be improved to make it more clear. | change "Each midamble is the same format as the NGV-LTF field(s) in the preamble of the same PPDU as defined inClause 32.3.7.3.6 (NGV-LTF definition), as shown" to "Eahc midamble field uses the same format as the NGV-LTF field of the same PPDU, which format is signaled in NGV-SIG. The Midamble OFDM symbol modulation is defined the same as Section 32.3.7.3.6 (NGV-LTF definition). The Midamble in a NGV PPDU is shown". | Revised.TGbd Editor: make changes according to this document 11-20-0721-00-00bd Resolutions to 32.3.8.10 Midambles. |
| 202 | 56.32 | Add an equation after Line 32 that maps the Midamble Periodicity Field to M. | Add the following line after Line 32:M= 4 \* 2^(Midamble Periodicity Field), where the value of Midamble Periodicity Field is defined in Table Table 32-10 (Fields in the NGV-SIG field). | RejectedMidambles are present in the Data field of the NGV PPDU every M OFDM symbols, where M is directly mapped to value among 4, 8, or 16 based on the values from Midamble Periodicity field (see Table 32-10) as below* Set to 0 for **4** symbols
* Set to 1 for **8** symbols
* Set to 2 for **16** symbols
* Value 3 is reserved.

The suggested equation seems redundant.  |

***To TGbd Editor:*** ***P56L23*** *update the description as below.*

***------------- Begin Text Changes ---------------***

**32.3.8.10 Midambles**

An NGV STA ~~may~~shall include midambles in an NGV PPDU transmission to facilitate channel estimation update during the PPDU when *NMA*is set to nonzero value as shown in Equation (32-42). (#152)

 The recipient might use the midambles to compensate the channel estimation.

Midambles are present in the Data field of the NGV PPDU every M OFDM symbols, where M is either 4, 8 or 16 ~~<TBD>~~ as indicated by the Midamble Periodicity field in NGV-SIG field (see Table 32-10 (Fields in the NGV-SIG field))~~<TBD>~~.(#19, #122, #153, #341)

~~Each midamble is the same format as the NGV-LTF field(s) in the preamble of the same PPDU as defined in~~

~~Clause 32.3.7.3.6 (NGV-LTF definition), as~~ Each midamble field uses the same format as the NGV-LTF field of the same PPDU, which format is signaled in NGV-SIG field. The generation of midamble is defined the same as subclause 32.3.7.3.6 (NGV-LTF definition). The midamble in a NGV PPDU is shown in Figure 32-11 (NGV PPDU with midamble). (#154)

***------------- End Text Changes ------------------***