IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposal for TWT Wide Range Parameters |
| Date: 2019-09-01 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Laurent Cariou | Intel |  |  |  |
| Alfred Asterjadhi | QC |  |  |  |
| George Cherian | QC |  |  |  |
| Matt Fischer | BRCM |  |  |  |

Abstract

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: constraint applicable to STA side as well

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TG Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TG Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TG Editor: Editing instructions preceded by “TG Editor” are instructions to the TG editor to modify existing material in the TG draft. As a result of adopting the changes, the TG editor will execute the instructions rather than copy them to the TG Draft.***

### Providing range of TWT parameters within TWT Setup

***Discussion Item:*** *Current a TWT request can provide only a value for each TWT parameter. Seems to be desirable to specify that the TWT request can also provide a range of values from which the peer STA can chose to select the TWT parameters.*

**TG Editor: *change section 9.3.3.3 as follows***

9.3.3.3 Beacon frame format

….

|  |
| --- |
| * Beacon frame body
 |
| **Order** | **Information** | **Notes** |
| 19 | EDCA Parameter Set | The EDCA Parameter Set element is present if dot11QosOptionImplemented is true, ~~and~~ dot11MeshActivated is false, and the QoS Capability element is not present; otherwise it is not present. |
| 20 | QoS Capability | The QoS Capability element is present if dot11QosOptionImplemented is true, ~~and~~ dot11MeshActivated is false, and neither the EDCA Parameter Set element nor the MU EDCA Parameter Set element are ~~is not~~ present; otherwise it is not present. |
| 57 | VHT Operation | The VHT Operation element is present when dot11VHTOptionImplemented is true and is optionally present if dot11HEOptionImplemented is true; otherwise, it is not present. |
| 63 | Reduced Neighbor Report | The Reduced Neighbor Report element is optionally present ifdot11TVHTOptionImplemented or dot11FILSActivated(11ai) or dot11ColocatedRNRImplemented(#20668) istrue; otherwise not present.(11ai) |
| 73 | Multiple BSSID Configuration | The Multiple BSSID Configuration element is optionally present if dot11MultiBSSIDImplemented is true.(M125) |
| 76 | HE Capabilities | The HE Capabilities element is present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 77 | HE Operation | The HE Operation element is present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 78 | TWT | The TWT element is optionally present if dot11TWTOptionActivated is true; otherwise it is not present. |
| 79 | UORA Parameter Set | The UORA Parameter Set element is optionally present if dot11OFDMARandomAccessOptionImplemented is true; otherwise it is not present. |
| 80 | BSS Color Change Announcement | The BSS Color Change Announcement element is optionally present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 81 | Spatial Reuse Parameter Set | The Spatial Reuse Parameter Set element is optionally present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 82 | MU EDCA Parameter Set | The MU EDCA Parameter Set element is optionally present if dot11HEOptionImplemented is true and dot11MUEDCAParametersActivated is true; otherwise, it is not present.(#20603) |
| 83 | ESS Report | The ESS Report element is optionally present.(#20638) |
| 84 | NDP Feedback Report Parameter Set | The NDP Feedback Report Parameter Set element is optionally present if dot11HEOptionImplemented is true; otherwise, it is not present. |
| 85 | HE BSS Load | The HE BSS Load element is optionally present if dot11QBSSLoadImplemented and dot11HEOptionImplemented are true. |
| 86 | HE 6 GHz Band Capabilities(#21158) | The HE 6 GHz Band Capabilities element is present if dot11HEOptionImplemented and dot11HE6GOptionImplemented(#20458) are true. |
| <ANA> | TWT Constraint Parameters element | The TWT Constraint Parameters element is optionally present if dot11TWTOptionActivated is true; otherwise it is not present. |

**TG Editor: *change section 9.3.3.7 as follows***

9.3.3.7 Association Response frame format

|  |
| --- |
| * Association Response frame body
 |
| **Order** | **Information** | **Notes** |
| 6 | EDCA Parameter Set | The EDCA Parameter Set element(#2479) is optionally(#20624) present ifdot11QosOptionImplemented is true; otherwise not present. |
| 29 | VHT Operation | The VHT Operation element is present when dot11VHTOptionImplemented is true and is optionally present if dot11HEOptionImplemented is true; otherwise, it is not present. |
| 39 | TWT | The TWT element is present if dot11TWTOptionActivated is true and the TWT element is present in the Association Request frame that elicited the Association Response frame.The TWT element is optionally present if dot11TWTOptionActivated is true, dot11HEOptionImplemented is true, and the TWT Requester Support field in the HE Capabilities element in the Association Request frame that elicited this Association Response frame is 1.Otherwise, the TWT element is not present.If the TWT element is present in the Association Request frame that solicits the Association Response frame but the TWT element is not present in the Association Response frame then the STA can transmit another TWT request frame after association. |
| 54 | HE Capabilities | The HE Capabilities element is present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 55 | HE Operation | The HE Operation element is present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 56 | BSS Color Change Announcement | The BSS Color Change Announcement element is optionally present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 57 | Spatial Reuse Parameter Set | The Spatial Reuse Parameter Set element is optionally present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 58 | MU EDCA Parameter Set | The MU EDCA Parameter Set element is present if dot11HEOptionImplemented is true and dot11MUEDCAParametersActivated is true; otherwise, it is not present.(#20603) |
| 59 | UORA Parameter Set | The UORA Parameter Set element is optionally present if dot11HEOptionImplemented is true; otherwise, it is not present. |
| 60 | ESS Report | The ESS Report element is optionally present.(#20638) |
| 61 | NDP Feedback Report Parameter Set | The NDP Feedback Report Parameter Set element is optionally present if dot11HEOptionImplemented is true; otherwise, it is not present. |
| 62 | HE 6 GHz Band Capabilities(#21158) | The HE 6 GHz Band Capabilities element is present if dot11HEOptionImplemented and dot11HE6GOptionImplemented(#20458) are true. |
| <ANA> | TWT Constraint Parameters element | The TWT Constraint Parameters element is optionally present if dot11TWTOptionActivated is true; otherwise it is not present. |

**TG Editor: *Insert the following paragraph after secion 9.3.3.11***

9.3.3.11 Probe Response frame format

|  |
| --- |
| * Probe Response frame body
 |
| **Order** | Information | Notes |
| 18 | EDCA Parameter Set | The EDCA Parameter Set element is optionally present ifdot11QosOptionImplemented is true and dot11MeshActivated isfalse.(#20624) |
| 59 | VHT Operation | The VHT Operation element is present when dot11VHTOptionImplemented is true and is optionally present if dot11HEOptionImplemented is true; otherwise, it is not present. |
| 65 | Reduced Neighbor Report  | The Reduced Neighbor Report element is optionally present ifdot11TVHTOptionImplemented (11ai)or dot11FILSActivated or dot11ColocatedRNRImplemented(#20668) istrue; otherwise not present. (11ai) |
| 92 | Multiple BSSID Configuration | The Multiple BSSID Configuration element is optionally present if dot11MultiBSSIDImplemented is true.(M125) |
| 93 | HE Capabilities | The HE Capabilities element is present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 94 | HE Operation | The HE Operation element is present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 95 | TWT | The TWT element is optionally present within broadcast Probe Response frames if dot11TWTOptionActivated, dot11HEOptionImplemented and dot11FILSOmitReplicateProbeResponses are true; otherwise it is not present. If the TWT element is present, then the Negotiation Type subfield(#20589) of the TWT element is 2. |
| 96 | UORA Parameter Set | The UORA Parameter Set element is optionally present if dot11OFDMARandomAccessOptionImplemented is true; otherwise it is not present. |
| 97 | BSS Color Change Announcement | The BSS Color Change Announcement element is optionally present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 98 | Spatial Reuse Parameter Set | The Spatial Reuse Parameter Set element is optionally present if dot11HEOptionImplemented is true; otherwise it is not present. |
| 99 | MU EDCA Parameter Set | The MU EDCA Parameter Set element is present if dot11HEOptionImplemented is true and dot11MUEDCAParametersActivated is true; otherwise, it is not present.(#20603) |
| 100 | ESS Report | The ESS Report element is optionally present.(#20638) |
| 101 | NDP Feedback Report Parameter Set | The NDP Feedback Report Parameter Set element is optionally present if dot11HEOptionImplemented is true; otherwise, it is not present. |
| 102 | HE BSS Load | The HE BSS Load element is optionally present if dot11QBSSLoadImplemented and dot11HEOptionImplemented are true. |
| 103 | HE 6 GHz Band Capabilities(#21158) | The HE 6 GHz Band Capabilities element is present if dot11HEOptionImplemented and dot11HE6GOptionImplemented(#20458) are true. |
| <ANA> | TWT Constraint Parameters element | The TWT Constraint Parameters element is optionally present if dot11TWTOptionActivated is true; otherwise it is not present. |

**TG Editor: *Insert the following paragraph after secion 9.3.3.11***

* + - 1. Association Request frame format

|  |
| --- |
| Table 9-36 - Association Request frame body  |
| **Order** | Information | Notes |
| <ANA> | TWT Constraint Parameters element | The TWT Constraint Parameters element is optionally present if dot11TWTOptionActivated is true; otherwise it is not present. |

**TG Editor: *Insert the following paragraph after secion 9.3.3.11***

* + - 1. Probe Request frame format

|  |
| --- |
| Table 9-40 - Probe Request frame body  |
| **Order** | Information | Notes |
| <ANA> | TWT Constraint Parameters element | The TWT Constraint Parameters element is optionally present if dot11TWTOptionActivated is true; otherwise it is not present. |

**TG Editor: *Insert the following subclause after 9.4.2.257***

9.4.2.xxx TWT Constraint Parameters element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  | Element ID | Length | TWT Constraint Parameters |
| Octets:  | 1 | 1 | 1 |
| Figure 9-xxx TWT Constraint Parameters element format |
|  |  |  |  |  |  |
|  | Starting Target Wake Time Alignment | Number of TWT Sessions |
| Octets:  | 1 | 1 |
| Figure 9-xxx TWT Constraint Parameter Set field format |

The Starting Target Wake Time Alignment field contains a positive integer number *n* to indicate a recommended time for the start of the first TWT SP of a TWT agreements. A value of *n* indicates that the recommended first start time should be an integer multiple of 2*n*\*TUs (i.e. (Target Wake Time) % (2*n*\*TUs) = 0 ).

The Number of TWT Sessions field contains the maximum number of TWT sessions that an AP is capable of establishing with an associated peer =STA.

**TG Editor: *Insert a new capability bit in the Extended Capabilities element named “Multiple Choice TWT Parameters Support” defined as follows:***

Multiple Choice TWT Parameters Support Set to 1 to indicate support for reception of a TWT Setup frame that contains two TWT elements (see 10.48.9 (Multiple choice TWT parameters); otherwise set to 0.

* TWT Setup frame format

The TWT Setup frame is an Action frame of category Unprotected S1G. It is sent by a STA to request the setup of a TWT SP and it is sent by a responding STA to indicate the status of a requested TWT SP. The Action field of the TWT Setup frame contains the information shown in Table 9-500 (TWT Setup frame Action field format(11ah)).

**TG Editor: *Change the table below as follows:***

|  |
| --- |
| * TWT Setup frame Action field format
 |
| Order | Information |
| 1 | Category  |
| 2 | Unprotected S1G Action |
| 3 | Dialog Token |
| 4 | One or more TWTs (9.4.2.199 (TWT element(11ah))) |

The Category field is defined in 9.4.1.11 (Action field).

The Unprotected S1G Action field is defined in 9.6.24.1 (Unprotected S1G Action field).

In a TWT Setup frame with a TWT Request field that is equal to 1, the Dialog Token field is set to a nonzero value chosen by the transmitting STA to identify the request/response transaction. In a TWT Setup frame with a TWT Request field equal to 0 that is sent in response to a TWT Setup frame with a TWT Request field that is equal to 1, the Dialog Token field is set to the value copied from the corresponding received TWT Setup frame with a TWT Request field equal to 1. In a TWT Setup frame with a TWT Request field set to 0 that is not sent in response to a TWT Setup frame with a TWT Request field equal to 1, the Dialog Token field is set to 0.

**TG Editor: *Insert a new paragraph as follows:***

The TWT element is defined in 9.4.2.199 (TWT element). A TWT Setup frame contains only one TWT element unless the Multiple Choice TWT Parameter Support field is equal to 1 in the Extended Capabilities element sent by the receiving STA, in which case two TWT elements are present (see 10.48.9 (Multiple choice TWT parameters) and those elements represent a request for the establishment of a single TWT agreement with a range of TWT parameter values.

**TG Editor: *Insert two new paragraphs as follows:***

**10.48.1 TWT overview**

A STA should not initiate a new TWT agreement with another STA if the number of TWT sessions between the two STAs would exceed the value of the Number of TWT Sessions field in the TWT Constraint Parameters elements (if any) exchanged between the two STAs .

A STA that includes the Target Wake Time field in a TWT element transmitted within a TWT request should include a value in the Target Wake Time field that is an integer multiple of 2*n*\*TUs (i.e. (Target Wake Time) % (2*n*\*TUs) = 0) where *n* is the value from the Starting Wake Time Alignment subfield the most recent TWT Constraint Parameters element received from the TWT responding STA. If no TWT Constraint Parameters element has been received from the TWT responding STA, then the STA may include any value in the Target Wake Time field.

**TG Editor: *Insert a new subclause as follows:***

**10.48.9 Multiple choice TWT parameters**

A STA that supports receiving more than one TWT element in a TWT Setup frame sets the Multiple Choice TWT Parameter Support field to 1 in the Extended Capabilities elements that it transmits.

A TWT requesting STA may send a TWT request that contains two TWT elements to a TWT responding STA if the most recently received Extended Capabilities element received from the responding STA has a Multiple Choice TWT Parameter Support field equal to 1. The TWT requesting STA shall either set the TWT Command fields of the two TWT elements to Suggest TWT or set the TWT Command fields of the two TWT elements to Demand TWT. For each TWT parameter of the proposed TWT agreeemnt, the STA may request either a single value or a range of values. To request a single value for a parameter, the STA sets the value of that parameter to be the same in each TWT element. To request a range of values for a parameter, the STA sets the parameter to one value in one of the TWT elements and to a different value in the other TWT element corresponding to the same TWT request. The numerically lower value for a parameter shall be included in the first element. The range indicated for a parameter is the range that starts with the lower value and includes all values up to the higher value.

The TWT responding STA shall set each TWT parameter of the TWT response to values selected from the range of values provided in the TWT request, if the TWT command of the TWT response is Accept TWT and the parameter included a range in the corresponding TWT request. The TWT responding STA shall set each TWT parameter of the TWT response to the single value provided in the TWT request, if the TWT command of the TWT response is Accept TWT and the parameter value is the same in each of the TWT elements in the corresponding TWT request.