IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution to CID 4003 | | | | |
| Date: 2020-07-29 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Guido R. Hiertz | Ericsson | Ericsson GmbH Ericsson Allee 1 52134 Herzogenrath Germany | +49-2407-575-5575 | hiertz@ieee.org |

Abstract

This document provides a resolution for CID 4003.

***Instruct the editor to modify IEEE P802.11-REVmd/D3.4 as follows:***

* General

The MAC architecture is shown in Figure 10-1 (Non-DMG non-CMMG non-S1G STA MAC architecture), Figure 10-2 (S1G STA MAC architecture), Figure 10-3 (DMG STA and CMMG STA MAC architecture).

[…]

In a DMG STA:

* The MAC provides services using the DMG channel access mechanisms.

In a CMMG STA:

* The MAC provides services using the CMMG channel access mechanisms.

In a either a DMG or a CMMG STA:

* Specific rules apply for access during scheduled periods, which include the association beamforming training (A-BFT) period, announcement transmission interval (ATI), contention based access period (CBAP), and service period (SP).
* The DCF is used during contention based access periods.
* Dynamic allocation (10.39.7 (Dynamic allocation of service period)) is built on service period and contention based access period.

The MAC maintains information in local variables called *MAC variables*. MAC variables that hold state information are also called *state variables*.

Ein Bild, das Screenshot enthält.

Automatisch generierte Beschreibung

Figure 10-3--DMG STA and CMMG STA architecture