IEEE P802.11  
Wireless LANs

|  |  |  |  |
| --- | --- | --- | --- |
| HE-STF Equation Correction for HE TB PPDU | | | |
| Date: 2020-07-22 | | | |
| Author(s): | | | |
| Name | Affiliation | Address | Email |
| Yan Zhang | NXP | 350 Holger way, San Jose, CA, 95134 | [yan.zhang\_5@nxp.com](mailto:yan.zhang_5@nxp.com) |

Abstract: This document contains proposed text changes to fix an error in HE-STF Equation for HE TB PPDU in D6.1.

Discussions:

In 27.3.11.9 HE-STF, HE-STF time domain representation signal for an HE TB PPDU transmitted by user *u* in the *r*-th RU as specified in Equation (27-39) should use *NSTS,r,u* instead of *NSTS,r,total* as the normalization factor since only  *NSTS,r,u* spatial streams are transmitted from this STA.

11ax editor: Please make the text changes as shown below.

* On P596L21 : Please change Equation (27-39) as shown below

(27-39)

* On P596L33 : Please add the following texts for clarification purpose.

is the HE-STF sequence for HE TB PPDU applied on subcarrier k. For an HE TB feedback NDP, replace with in Equation (27-39) .

is given in the Starting Spatial Stream subfield in the SS Allocation subfield of the Trigger frame User info field for the *u*-th user inthe *r*-th occupied RU in Figure 9-64e (SS Allocation subfield format).