IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| [The Comment regolution for CID 279] | | | | |
| Date: 2020-06-15 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Dongguk Lim | LG Electronics | 19, Yangjae-Daero 11 gil, Seoch-gu, Seoul, Korea |  | dongguk.lim@lge.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for CID 279

Revisions:

* Rev 0: Initial version of the document.

## CID 279

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 279 | 42.18 | 32.3.7.2.1 | fill TBD | as in comment | Revised  TGbd editor to make the changes shown in 11-20/xxxxr0 |

### Discusson: We have agreed that 11bd can use the 2 antennae and support the up to 2 spatial streams. So, for efficient transmission and for reduction of unintended beamforming, we should need to define the CSD values for pre-NGV modulated fields. And, by appling to the agreement described in 973r1, we can reuse the CSD values defined in 11ac for pre-NGV modulated fields.

**Propose:**

***TGbd editor: please change the TBD in 32.3.7.2.1 Cyclic shift for pre-NGV modulated fields to follows***

The cyclic shift value for the L-STF, L-LTF, L-SIG and RL-SIG, NGV-SIG and RNGV-SIG fields of the PPDU for transmit chain iTX out of a total of NTX are defined in Table 21-10 (Cyclic shift values for L-STF, L-LTF, L-SIG, and VHT-SIG-A fields of the PPDU). (#279)