IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed Draft Text for MLO Multi-Link Group Addressed Data Delivery |
| Date: 2020-09-05 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Kaiying Lu | MediaTek Inc. | 2840 Junction Ave, San Jose, CA 95134 |  | kaiying.lu@mediatek.com  |
| Yongho Seok | MediaTek Inc. | 2840 Junction Ave, San Jose, CA 95134 |  | yongho.seok@mediatek.com  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes draft text for the MLO Multi-Link Group Addressed Data Delivery based on the following portions of the SFD:

Revisions:

Rev 0: Initial version of the document.

1. 802.11be supports the following group addressed frames delivery mechanism in R1:
* An AP MLD should not cause a STA affiliated to a non-STR non-AP MLD to transmit an MPDU that overlaps with group addressed frames in a constrained link if another STA affiliated to the same non-STR non-AP MLD is expected to be receiving group addressed frames.

[Motion 122, #SP155, [10] and [171]]

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

***Insert new Clause 33 following Clause 32 as follows:***

33. Extremely High Throughput (EHT) MAC specification

33.x Multi-link operation

33.x.y1 Multi-link group addressed data transmission

An AP MLD should not transmit a frame that solicits an immediate response to a STA affiliated to a non-STR non-AP MLD, if the immediate response overlaps in time with group addressed MPDUs scheduled in a link of an NSTR link set of the non-STR non-AP MLD and another STA affiliated to the non-STR non-AP MLD is expected to be receiving those group addressed MPDUs. An AP MLD determines which STAs affiliated to a non-STR non-AP MLD are expected to be receiving group address MPDUs subject to the TBD rules.

(#Motion 122, SP155)

**Straw Poll: Do you support to incorporate the proposed draft text in this document 11-20/xxxxr0 to the TGbe Draft 0.1?**

**Result: Yes/No/Abstain**