IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed Spec Text for CR |
| Date: 2020-09-15 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. |  | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |
|  |  |  |  |  |

Abstract

This submission proposes spec text for CR for CID 57, 187, 268, 265, 262, 199, 198 and 197. The baseline for this comment resolution document is 802.11bc Draft 0.1.

***TGbc Editor: Please modify the paragraph starting at P37L25 as follows:***

1. The Title subfield indicates the title of the eBCS identified by the Content ID contained
2. in the Content ID subfield as a UTF-8 string. [#197, 198]

***TGbc Editor: Please modify the paragraph starting at P40L1 as follows:***

The Hostname subfield indicates the host name for negotiating the extension of the eBCS as a UTF-8 string. [#199]

***TGbc Editor: Please modify subclause 11.22.6.bc Termination Notice Procedure as follows starting at P48L28:***

1. After transmitting an eBCS Termination Notice frame, an eBCS STA shall transmit an eBCS Termination
2. Notice frame with an updated value in the Time To Termination subfield in an eBCS Termination Info
3. subfield if the eBCS identified by the Content ID in the Content ID subfield in the same eBCS Termination
4. Info subfield subfield has been negotiated to have a new Time To Termination value.
5. If the negotiated duration for the eBCS is longer than the maximum Time To Termination value, the
6. transmitting STA shall set the Time To Termination subfield to 65535. [#265]

# 34

1. An eBCS STA that receives an eBCS Termination Notice frame may negotiate for the extension of an
2. eBCS if the eBCS indicated in one of the eBCS Termination Info subfield terminates earlier than desired.
3. The eBCS STA may negotiate the extension of the eBCS using the request method as indicated in the
4. Request Method in the eBCS Termination Info subfield and follow the procedures defined in 11.22.6.bc
5. (eBCS Negotiation Procedure for Associated STAs) and 11.23.3.3 (ANQP Procedures).

# 40

1. An eBCS STA shall skip the transmission of any eBCS Request frame or a frame containing an Enhanced
2. Broadcast Request ANQP-element requesting for an eBCS if the STA receives an eBCS Termination
3. Notice frame with an acceptable Time To Termination value contained in the eBCS Termination Info
4. subfield containing the Content ID of the eBCS.

Note – Which values of a received Time to Termination subfield are considered acceptable is determined by the receiving STA and is beyond the scope of this standard. [#268]