IEEE P802.11
Wireless LANs

|  |
| --- |
| PDT for Motion 137, #SP266 (MLO Critical Updates Indication) |
| Date: 2020-11-10 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Abhishek Patil | Qualcomm |  |  | appatil@qti.qualcomm.com |
| George Cherian |  |  |  |
| Alfred Asterjadhi |  |  |  |
| Duncan Ho |  |  |  |
| Yanjun Sun |  |  |  |

Abstract

This document provides draft spec text for motion 137 SP#266 in TGbe draft D0.1.

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Limiting the scope of the document to Motion 137, #SP266

**Related Motion:**

In R1, an AP of an MLD shall provide early indication (in the Capability Information field) in Beacon frame(s) until (and including) the next DTIM Beacon frame when there is a change to the change sequence value for any other AP of that MLD reported in the RNR.

[Motion 137, #SP266, [3] and [223]]

**Proposed spec text:**

The baseline for this text is 802.11be D0.1

* BSS parameter critical update procedure

*TGbe editor: Please make changes to the following paragraph as shown below:*

[Motion 137, #SP266]

An AP within an AP MLD shall provide in the Capability Information field of the Beacon and Probe Response frames it transmits an indication (in the TBD subfield) of an update to the Change Sequence field value in the RNR for any AP in the same AP MLD. An AP of an MLD shall provide such indication in the Beacon frame(s) until (and including) the next DTIM Beacon frame.