IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| PDT-PHY-Spatial-Configuration-Table-Typo-Fixed | | | | |
| Date: 2020-10-10 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Ross Jian Yu | Huawei | Huawei Industrial Base, Shenzhen, Guangdong, China |  | ross.yujian@huawei.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This document contains proposed draft change to fix the typo proposed by Ron on spatial configuration table.

R0: initial version

**Instructions to the editor, please make the following changes on L29P204 of Draft P802.11be D0.1:**

**Table 34-27 - Spatial Configuration subfield encoding**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 101110-110000 | 2-4 | 2 | 2 | 2 | 2 | 2 | 2 |  | 14-16 |
| 110001 | 3 | 3 | 2 | 2 | 2 | 2 | 2 |  | 16 |