IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| [The Comment resolution for 32.3.8.2.1] | | | | |
| Date: 2020-01-xx | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Dongguk Lim | LG Electronics | 19, Yangjae-Daero 11 gil, Seoch-gu, Seoul, Korea |  | dongguk.lim@lge.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for CID1772

Revisions:

* Rev 0: Initial version of the document.

## CID 1772

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 1772 | 63.16 | 32.3.8.2.1 | 32.3.8.2.1 Cyclic shift for pre-NGV modulated fields shall not include RL-SIG in these paragraph | Remove RL-SIG from the first sentence. | Rejected.  We have determined that the value of cyclic shift for pre-NGV modulated field defined in Table 21-10 should be applied to RL-SIG, NGV-SIG, and RNGV-SIG. |

**References:**

**[1] 802.11bd D1.0**