IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| [The Comment resolution for 32.3.8.2.2] | | | | |
| Date: 2020-01-11 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Dongguk Lim | LG Electronics | 19, Yangjae-Daero 11 gil, Seoch-gu, Seoul, Korea |  | dongguk.lim@lge.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for following 10 CIDs: 1080, 1113, 1114, 1115, 1538, 1578, 1774, 1776, 1083, and 1817

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Resolution and document link updated

## CID 1080, 1113, 1114, 1115, 1538, 1578, 1774, 1776, 1083, and 1817

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 1080 | 63.35 | 32.3.8.2.2 | Eq 32-6 only covers 10MHz case. Need to cover 20Mhz too | as in comment | Revised.  The commenter is right. NGV supports both the 10MHz transmission and 20MHz transmission. And, the L-STF field of 10MHz transmission is duplicated per 10MHz in 20MHz transmission. So, Eq32-6 should be modified to cover the 20MHz transmission.  TGbd Editor: Incoroporate the changes in https://mentor.ieee.org/802.11/dcn/21/11-21-0022-01-00bd-the-comment-resolution-for-32-3-8-2-2.docx. |
| 1113 | 63.34 | 32.3.8.2.2 | in Eq 32.6, S\_k is not defined | correct equation | Revised.  The commenter is right.  The definition of S\_k is missing. The definitioan of S\_k should be added in 11bd spec  TGbd Editor: Incoroporate the changes in https://mentor.ieee.org/802.11/dcn/21/11-21-0022-01-00bd-the-comment-resolution-for-32-3-8-2-2.docx. |
| 1538 | 63.26 | 32.3.8.2.2 | change "The L-STF field for a 10 MHz or 20 MHz transmission is defined by Equation (19-8) and Equation (19-9) ..." to "The frequency domain sequence of L-STF field for 10 MHz and 20 MHz transmission are defined by Equation (19-8) and Equation (19-9) ..." | As in the comment. | Accepted.  TGbd Editor: Incoroporate the changes in https://mentor.ieee.org/802.11/dcn/21/11-21-0022-01-00bd-the-comment-resolution-for-32-3-8-2-2.docx. |
| 1578 | 63.34 | 32.3.8.2.2 | Eqs. (32-6) & (32-7) are applied to both 10 MHz and 20 MHz. Change the constant 26 to NR. | As in the comment. | Revised.  The commenter is right. NGV supports both the 10MHz transmission and 20MHz transmission. And, the L-STF field of 10MHz transmission is duplicated per 10MHz in 20MHz transmission. So, Eq32-6 should be modified to cover the 20MHz transmission.  Note to editor :Same resolution for CID 1080 |
| 1774 | 63.34 | 32.3.8.2.2 | In Equation (32-6), &#951;\_L-STF is included while it is not included in the general subfield equation (32-3). &#951;\_field should be included in equation (32-3) to be consistent | See comment | Revised.  The commenter is right.  The parameter of power boosting for L-STF and L-LTF should be included in equation 32-3.  TGbd Editor: Incoroporate the changes in https://mentor.ieee.org/802.11/dcn/21/11-21-0022-01-00bd-the-comment-resolution-for-32-3-8-2-2.docx. |
| 1776 | 63.34 | 32.3.8.2.2 | In Equation (32-6), k range from -26 to 26, which only covers 10MHz L-STF definition. | Please change k range to -NSR to NSR which includes both 10MHz and 20MHz NGV PPDU. | Revised  The commenter is right. NGV supports both the 10MHz transmission and 20MHz transmission. So, Eq32-6 should be modified to cover the 20MHz transmission.  Note to editor :Same resolution for CID 1080 |
| 1083 | 63.43 | 32.3.8.2.2 | Why applies 3dB power boosting to L-STF and L-LTF for MCS0? | as in comment | Reject.  For the improvement of decoding performance, we decided that 3dB power boosting is applied to L-STF and L-LTF when BPSK modulation is used. Please refer to the 11-19/1824r1. |
| 1817 | 63.44 | 32.3.8.2.2 | power boost for L-STF and L-LTF applied when BPSK, 10MHz and one spatial stream. | in addition to MCS0 or MCS10, other condition such as BW and Nss should be added | Revised.  The commenter is right.  Power boosting for L-STF and L-LTF is only applied to limited condition such as BPSK, NSS=1, 10MHz  TGbd Editor: Incoroporate the changes in https://mentor.ieee.org/802.11/dcn/21/11-21-0022-01-00bd-the-comment-resolution-for-32-3-8-2-2.docx. |
| 1114 | 63.34 | 32.3.8.2.3 | in Eq 32.6, \Delta\_f,NGV is not defined in the timely related parameters, but only \Delta\_f | correct equation | Revised  The commenter is right.  Change the Delta\_f,NGV to Delta\_f throughout in 11bd D1.0.  TGbd Editor: Incoroporate the changes in https://mentor.ieee.org/802.11/dcn/21/11-21-0022-01-00bd-the-comment-resolution-for-32-3-8-2-2.docx. |
| 1115 | 63.40 | 32.3.8.2.4 | the definition of \eta\_L-LTF is done per subcarrier but in the equation there is no dependency between the two | make the definition clear | Revised  The commenter is right.  Remove subcarrier index from in the 11bdD1.0 since it is a constant over 20MHz channel.  TGbd Editor: Incoroporate the changes in https://mentor.ieee.org/802.11/dcn/21/11-21-0022-01-00bd-the-comment-resolution-for-32-3-8-2-2.docx. |

**Propose :**

***TGbd editor: please modify the clause 32.3.8.2.2 L-STF definition as follows***

The frequency domain sequence of the L-STF field for a 10 MHz or 20 MHz transmission is defined by Equation (19-8) and Equation (19-9), respectively, in 19.3.9.3.3 (L-STF definition). (#1538)

The time domain representation of the signal on transmit chain shall be as specified in Equation (32-6).

(32-6) (#1080, #1578, #1776, and #1114)

where

is a modulation dependent power scaling factor for the L-STF field ~~on subcarrier index~~ with the following value (#1115)

(#1817)

represents the cyclic shift for transmit chain with a value given in Clause 32.3.8.2.1 (Cyclic shift for pre-NGV modulated fields)

is defined in Equation (32-4) and Equation (32-5)

has the value given in Table 33-x1 (Tone scaling factor and guard interval duration values for PHY fields)

is defined as in equations (19-8). (#1113)

***TGbd editor: please modify the equation 32-3 as follows***

(# 1774)

***TGbd editor: please add the following text to below P63 L30***

is the power scale factor of a given field within an OFDM symbol for NGV PPDU. For the L-STF and L-LTF field, is in the range of . The same value applies to the L-STF and L-LTF field. For other fields of NGV PPDU, . (# 1774)

**References:**

**[1] 802.11bd\_D1.0**