IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| [The Comment resolution for 32.3.8.3.5] | | | | |
| Date: 2020-01-11 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Dongguk Lim | LG Electronics | 19, Yangjae-Daero 11 gil, Seoch-gu, Seoul, Korea |  | dongguk.lim@lge.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for following 2 CIDs: 1084 and 1820

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Resolution and document link updated
* Rev 2: The resolution for CID 1084 (green part) is updated.

## CID 1084 and 1820

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 1084 | 68.62 | 32.3.8.3.5 | Don't understand the note. 10 MHz NGV-STF doesn't need per 10Mhz phase rotation. For 20MHz NGV-STF, if using the VHT 40MHz STF seqeunce, why is additional per 10MHz rotation needed | as in comment | Rejected.  The comment asks for a clarification for the note but does not provide a suggested change to the draft.  Discussion :  No additional phase rotation per 10MHz does not apply to the frequency sequence of 20MHz NGV-STF . And, other people can clearly understand that the phase rotation is applied on this frequency sequence for 20MHz transmission. |
| 1820 | 69.3 | 32.3.8.3.5 | Nsts is not defined with no STBC supported | Nsts should be replaced with Nss in Equatoin 32-16 | Accepted |

**Propose :**

***TGbd editor: please modify the equation (32-16) as follows***

(32-16) (#1820, #1114)

**References:**

**[1] 802.11bd D1.0**