IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution for CIDs related to Multi-Link element (CC 34) – Part 2 | | | | |
| Date: March 20, 2021 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Abhishek Patil | Qualcomm Inc. |  |  | appatil@qti.qualcomm.com |
| Gaurang Naik |  |  | gnaik@qti.qualcomm.com |
| George Cherian |  |  | gcherian@qti.qualcomm.com |
| Alfred Asterjadhi |  |  | aasterja@qti.qualcomm.com |
| Duncan Ho |  |  | dho@qti.qualcomm.com |
| Yanjun Sun |  |  | yanjuns@qti.qualcomm.com |

Abstract

This submission proposes resolutions for following 34 CIDs received for TGbe CC34:

2294, 1858, 1859, 1034, 2149, 1861, 2831, 1833, 1863, 1860, 2586, 2183, 1035, 2451, 1036, 1864, 1919, 3315, 1184, 1185, 2866, 3335, 2309, 2964, 2472, 2296, 2868, 2167, 3021, 3212, 3369, 3370, 1005, 1896

***TGbe editor: Please note Baselines are REVmd D5.0, 11ax D8.0, 11be D0.4.***

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

**PART A**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Pg/Ln** | **Section** | **Comment** | **Proposed Change** | **Resolution** |
| 2294 | Michael Montemurro | 126.01 | 35.3.2 | This title makes no sense. How is it a container? | Rename to "Requirements for multi-link operation" | **Revised**  Based on offline discussion with the commenter, the title of the subclause was changed to “Advertisement of multi-link information”.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2294 and revise the title in all references to the subclause throughout the draft.** |
| 1858 | Jarkko Kneckt | 126.37 | 35.3.2.1 | The lines 37 - 40 seem to discuss on the content of the per-STA profile. These details are not needed in general introduction clause. | Please move lines 37 - 40 to clause 35.3.2.2 | **Revised**  Agree with the comment. Moved the cited paragraphs to clause 35.3.2.2 at appropriate locations  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1858** |
| 1859 | Jarkko Kneckt | 126.37 | 35.3.2.1 | Per-STA profile does not have good introduction in the general paragraph. | Please add introduction for the Per-STA profile. | **Revised**  Agree with the comment. Moved the 1st paragraph of clause 35.3.2.2 to clause 35.3.2.1 as the last paragraph with the text updated to clarify that clause 35.3.2.2 provides details on advertisement of per-link information. The title of 35.3.2.2 is updated as “Advertisement of per-link information”  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1859 including updating the title of clause 35.3.2.2 throughout the draft.** |
| 1034 | Abhishek Patil | 126/47 | 35.3.2.2 | Remove the TBD. When the element is included in an ML Probe Response frame or (Re)Association Response frame, it carries complete profile. Complete profile includes all the capabilities and operational IEs with inheritance applied. For non-AP MLD, (Re)Association Request frame carries complete profile which includes the reported STA's capabilities. When the element is include in an ML Probe Response frame, it carries partial profile, the content depends on the content of soliciting ML Probe Request frame. For example, non-AP MLD can request specific element via the (Extended) Request element or non-AP MLD may request critical updates information. ML IE when included in the Beacon frame includes only MLD level information. | As in comment | **Revised**  The TBD was addressed.  The 3rd paragraph in clause 35.3.2.2 which was added by doc 11-21/242r4 (and incorporated in D04) covers when the profile carries complete information.  The subclause 35.3.2.2 was updated to clarify the case of partial information or the case when link information is not carried in the frame:  1. Basic variant ML IE when included in Authentication frame or Neighbor Report IE does not include Link Information field.  2. Beacon frame doesn’t carry complete profile (to prevent bloating). Beacon may carry partial profile in case of critical updates such as channel switch announcement or quiet element  3. Provided detailed conditions when probe response frame carries complete or partial profile. Duplicate text from clause 35.3.4.2 was deleted.  4. Approved text from 11-21/242r4 (incorporated in D0.4) already mentions that (Re)Association Request and Response frames carry complete profile in the per-sta profile.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1034.** |
| 2149 | Laurent Cariou | 0.00 | 35.3.2.2 | Fix: "exact set of elements/fields that constitute partial information is TBD", to refer to the Request element which specifies the requested partial information | as in comment | **Revised**  The TBD was addressed.  The 3rd paragraph in clause 35.3.2.2 which was added by doc 11-21/242r4 (and incorporated in D04) covers when the profile carries complete information.  The subclause 35.3.2.2 was updated to clarify the case of partial information or the case when link information is not carried in the frame:  1. Basic variant ML IE when included in Authentication frame or Neighbor Report IE does not include Link Information field.  2. Beacon frame doesn’t carry complete profile (to prevent bloating). Beacon may carry partial profile in case of critical updates such as channel switch announcement or quiet element  3. Provided detailed conditions when probe response frame carries complete or partial profile. Duplicate text from clause 35.3.4.2 was deleted.  4. Approved text from 11-21/242r4 (incorporated in D0.4) already mentions that (Re)Association Request and Response frames carry complete profile in the per-sta profile.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2149.** |
| 1861 | Jarkko Kneckt | 126/47 | 35.3.2.1 | Please list the elements that are mandatory to be present in a partial per-STA profile. | Please list the elements that are mandatory to include to the partial per-STA profile. | **Revised**  The TBD was addressed.  The 3rd paragraph in clause 35.3.2.2 which was added by doc 11-21/242r4 (and incorporated in D04) covers when the profile carries complete information.  The subclause 35.3.2.2 was updated to clarify the case of partial information or the case when link information is not carried in the frame:  1. Basic variant ML IE when included in Authentication frame or Neighbor Report IE does not include Link Information field.  2. Beacon frame doesn’t carry complete profile (to prevent bloating). Beacon may carry partial profile in case of critical updates such as channel switch announcement or quiet element  3. Provided detailed conditions when probe response frame carries complete or partial profile. Duplicate text from clause 35.3.4.2 was deleted.  4. Approved text from 11-21/242r4 (incorporated in D0.4) already mentions that (Re)Association Request and Response frames carry complete profile in the per-sta profile.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1861.** |
| 2831 | Srinivas Kandala |  | 0.00 | STA profile elements need to be expanded substantially | As in the Comment | **Revised**  The comment is not clear about the clause where the changes are expected. There are several contributions in the queue that are adding text to clause 9 to describe new sub-fields that are being added to the STA Control and STA Info fields. The contents of the STA Profile field depend based on whether the profile is complete or partial. Text in clause 35.3.2.2 was updated to provide rules for when the profile is complete or partial. The contents for complete profile are describe in the rest of this document as resolution to other comments.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2831.** |
| 1833 | Jarkko Kneckt | 75/35 | 9.4.2.295b.2 | The partial Per-STA Profile is not well defined. Does partial profile contain some mandatory fields that are always present in the non-copmplete profile? | Please clarify the fields that are always present and list the fields that may be optionally present in the non-complete profile. | **Revised**  Agree with the commenter. A paragraph was added to clause 35.3.2.1 to clarify that the Multi-Link Control field is always carried in the element and signals the presence of other fields in the Common Info field of the element. A paragraph was added to clause 35.3.2.2 to clarify that the Per-STA Control field is always present and signals the presence of other field in the Per-STA Profile subelement.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1833.** |
| 1863 | Jarkko Kneckt | 127.15 | 35.3.2.3 | The basic variant multi-link element may be added to the authenticate req/resp frames, but there is no description of the content of the multi-link element in this case. | Please clarify how basic variant of the multi-link element is used in the authentication req/resp frames. Alternatively, please create new ML element for authentication req/resp frames. | **Revised**  Agree with the commenter. Clause 35.3.2.2 was updated to clarify that per-STA profile is not carried in Basic variant ML IE that is included in an Authentication frame. Further, Table 9-40 was updated to indicate that Basic variant ML IE is present (not optionally present) in Authentication frame transmitted by a AP/STA affiliated with an MLD. This is consistent with the text in clause 35.3.5.4  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1863.** |

**35.3.2 Advertisement of multi-link information**[CID 2294]

**35.3.2.1 General**

***TGbe editor: Please move the following two paragraphs to clause 35.3.2.2 as shown below:***

[CID 1858]

[CID 1858]

***TGbe editor: Please add the following paragraph before the last paragraph in this subclause shown below:***

[CID 1833] A STA affiliated with an MLD shall provide an indication of the fields carried in the Common Info field of the Basic variant Multi-Link element via the subfields in the Multi-Link Control field.

***TGbe editor: Please make the following changes to the following paragraph which is moved from 35.3.2.2 as shown below:***

[CID 1859]include Link Info field in the Basic variant Multi-link element that it transmits to affiliated with as defined in 35.3.2.2[CID 1034, 2149, 1861, 1833, 2831]

**35.3.2.2 Advertisement of per-link information**[CID 1859]

***TGbe editor: Please move the 1st paragraph of this subclause to clause 35.3.2.1 as shown below:***

[CID 1034, 2149, 1861, 1833, 1859]

***TGbe editor: Please add the following two paragraphs after the paragraph starting “A reporting STA affiliated with an MLD shall set the Complete Profile subfield…” in this subclause as shown below:***

[CID 1833] The subfields of the Per-STA Control field in the Per-STA profile corresponding to a reported STA shall provide an indication of the presence of optional fields and elements carried in the STA Info field.

[CID 1858]

***TGbe editor: Please add the following paragraphs after the paragraph starting “The complete information of a reported STA …” as shown below:***

[CID 1034, 2149, 1861, 2831] An AP affiliated with an AP MLD shall not include complete profile of a reported AP affiliated with the same AP MLD in transmitted Beacon frame.

NOTE 1 – It is recommended that an AP affiliated with an AP MLD includes only the Common Info field in the Basic variant Multi-Link element that is carried in Beacon frames (see 35.3.4.4 (Multi-link element usage rules in the context of discovery)). An AP affiliated with an AP MLD includes in transmitted Beacons, the partial profile of a reported AP affiliated with its AP MLD when conditions defined in 35.3.9 (General procedures) are satisfied.

NOTE 2 – A Probe Request frame does not carry Basic variant Multi-Link element (see 35.3.4.4 (Multi-link element usage rules in the context of discovery)).

[CID 1863] An AP or a non-AP STA affiliated with an MLD shall not include Link Info field of the Basic variant Multi-Link element in the Authentication frame that it transmits.[CID 1858]

[CID 1034, 1833, 2149, 1861, 2831] An AP affiliated with an AP MLD may include either the complete profile or the partial profile of a reported AP affiliated with the same AP MLD in the transmitted Probe Response frames subject to the following rules:

* If the soliciting request is not an ML probe request, then the Probe Response frame should include only the Common Info field as defined in 35.3.4.4 (Multi-link element usage rules in the context of discovery), unless conditions defined in 35.3.9 (General procedures) are satisfied.
* If the soliciting request is an ML probe request that solicits the complete profile of an AP affiliated with the reporting AP’s AP MLD, then the ML probe response shall carry the complete profile of the requested AP.
* If the soliciting request is an ML probe request that solicits specific elements of an AP affiliated with the reporting AP’s AP MLD, then the partial profile of a requested AP sent by the reporting AP shall consists of one or more elements that are requested in the (Extended) Request element carried in the ML probe request as defined in 35.3.4.2 (Use of ML probe request and response).

**35.3.4.2 Use of ML probe request and response**

***TGbe: Please delete the following paragraph to clause 35.3.2.2***

[CID 1034, 2149, 1861, 2831]

**9.3.3.11 Authentication frame format**

***Insert a new row to*** [***Table 9-40 (Authentication frame body)***](#bookmark14)***:***.

**Table 9-40—Authentication frame body**[CID 1863]

|  |  |  |
| --- | --- | --- |
| **Order** | **Information** | **Notes** |
| <ANA> | Multi-Link | The Basic variant Multi-Link element is present if the STA is affiliated with an MLD and the frame exchange is with a peer STA that is affiliated with an MLD. Otherwise it is not present. |

**PART B**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Pg/Ln** | **Section** | **Comment** | **Proposed Change** | **Resolution** |
| 1860 | Jarkko Kneckt | 126/47 | 35.3.2.1 | The order of the information is not logical. The fields that are included in complete profile should be listed in clause that discusses on complete per-STA profile. | Please list the elements that are part of the complete per-STA profile in complete per-sta profile clause. | **Revised**  Agree with the commenter. The list of elements and fields that are part of the complete per-STA profile and Figure 35-1 are moved to 35.3.2.2.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1860.** |
| 2586 | Rojan Chitrakar | 127/25 | 35.3.2.3 | "...each Per-STA Profile subelement in a Basic variant Multi-Link element that is a complete profile shall contain a list of elements as follows:"  the bullets do not only talk about elements, it also talks about fields. | rephrase as:  "...each Per-STA Profile subelement in a Basic variant Multi-Link element that is a complete profile shall contain a list of fields and elements as follows:" | **Revised**  Agree with the comment. The cited sentence was updated to include fields.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2586.** |
| 2183 | Li-Hsiang Sun | 9.4.2.1 | 68.58 | DTIM count/period is currently in TIM or Multiple BSSID-index elements, but these elements (and their DTIM related fields) are unlikely to be included in the per-STA profile in some cases | define a new element for DTIM information of reported APs | **Revised**  Agree with the comment. DTIM Info field and Beacon Interval fields were added to per-STA profile with corresponding presence indicator bits in the control field.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2964.** |
| 1035 | Abhishek Patil | 127.29 | 35.3.2.3 | Fix the TBDs. One of the first field or element must be the Capabilities Information field for the reported STA. Also need to provide the BI, DTIM interval etc for each link. | As in comment | **Revised**  Agree with the comment.  The cited paragraph (now moved to clause 35.3.2.2) was updated to address the TBDs.  1. Each per-STA profile consists of a unknown set of fields whose presence is signaled via the subfields in the Control field and a variable number of fields and elements based on the frame that carries the ML IE and inheritance. The format of the Per-STA Profile sublement is updated to have 3 parts – STA Control, STA Info and STA Profile. This will make it easy to describe the contents of each portion of the subelement. Clause 9 was updated accordingly.  2. The text in the cited paragraph was extensively updated to provide details on the presence and order in which the elements and field appear when per-STA profile carries complete information.  3. Added a list of elements that are not carried in the per-STA profile  4. Included rules on inheritance.  Figure 35-1 was revised to demonstrate the contents of the Per-STA Profile subelement when the Basic variant Multi-Link element is carried by a STA affiliated with a non-AP MLD in an Association Request frame.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1035.** |
| 2451 | Patrice Nezou | 127/30 | 35.3.2.3 | The wording "fixing order" does not define any order. Please clarify. | Define an order to the list of element contained in a Basic variant Multi-Link element | **Revised**  Agree with the comment.  The cited paragraph (now moved to clause 35.3.2.2) was updated to address the TBDs.  1. Each per-STA profile consists of a unknown set of fields whose presence is signaled via the subfields in the Control field and a variable number of fields and elements based on the frame that carries the ML IE and inheritance. The format of the Per-STA Profile sublement is updated to have 3 parts – STA Control, STA Info and STA Profile. This will make it easy to describe the contents of each portion of the subelement. Clause 9 was updated accordingly.  2. The text in the cited paragraph was extensively updated to provide details on the presence and order in which the elements and field appear when per-STA profile carries complete information.  3. Added a list of elements that are not carried in the per-STA profile  4. Included rules on inheritance.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2451.** |
| 1036 | Abhishek Patil | 127/33 | 36.3.2.3 | The order and list of elements should depend on the type of frame carrying the element - e.g., if the element is carried in a Beacon frame, then follow 9-32, for ML Probe Response follow 9-32 and so on for (Re)assoc resp. Also update the text in figure 35-1 | As in comment | **Revised**  Agree with the comment. The text was updated to identify the Tables in clause 9.3.3 for the order in which the fields and element will be carried for each frame that carries the Basic variant ML IE.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1036.** |
| 1864 | Jarkko Kneckt | 128/06 | 35.3.2.3 | Per-STA profile is not optional in the association request/response frame. | Please change to optional/conditional subelements in figure 35-1. | **Revised**  Agree with the commenter. Text in clause 35.3.5.4 already specifies that (Re)Assoc Req/Resp frames carry complete profile. In addition, text in clause 35.3.2.2 was updated in doc 11-21/242r4 (and appears in D0.4) to suggest that these frames carry complete profile. The bulleted text was updated to indicate that order of the fields and elements in the per-STA profile is same as that for each of the frames. In addition, figure 35-1 was updated to show Association Request frame as an example carrying complete profile.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1864.** |
| 1919 | Jeongki Kim | 127/35 | 35.3.2.3 | Regarding the non-AP STA case, don't we need to consider the Probe Reqeust frame as well as Association Request frame? If yes, add the text related to Probe Request frame. | Add the text of Probe Request frame | **Rejected**  Probe Request frame doesn’t carry Basic variant ML IE as specified in clause 35.3.4.4 |
| 3315 | Yunbo Li | 127.40 | 35.3.2.3 | The descriptions of Non-Inheritance element are conflict. Non-Inheritance element is optioinal to included, but it is in the list of elements that shall be contained. | clarify that Non-Inheritance element shall be contained only when it is necessary. | **Rejected**  The cited bullet, text in 2nd paragraph of clause 35.3.2.3, and the text in figure 35-1 all indicate that the Non-Inheritance element is optionally carried as a subelement. |
| 1184 | Arik Klein | 128.07 | 35.3.2.3 | Figure 35-1 does not include "elements specific to the reported STA or with content that is not inherited from the reporting STA" that should precede the Last element (Non-Inheritance element) - not aligned with the requirements of the Basic variant Multi-Link element that is a complete profile as defined in P127L25 | Correct Figure 35 to align with the the requirements of the Basic variant Multi-Link element that is a complete profile as defined in P127L25 | **Revised**  Agree with the commenter. The bullets in preceding paragraph were updated to clarify that the fields and elements included in the STA profile are subject to inheritance as defined in clause 35.3.2.3. In addition the figure was updated to provide this clarification.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1184.** |
| 1185 | Arik Klein | 128.07 | 35.3.2.3 | Figure 35-1 includes several fields (designated as: Field1..Field K) following the Multi-link control field and followed by the Optional Subelements part. This is not aligned with the Basic Variant format, as described in section 9.4.295b where the Multi-link Control field is followed by Common Info field of the Basic variant Multi-Link element (see Figure 9-788eh) | Please correct the example in Figure 35-1 so it will be aligned with the Basic Variant format as described in section 9.4.295b | **Revised**  Agree with the commenter. The figure was simplified to provide a specific example – i.e., that of Association Request frame. In addition, a descriptive text was added after the figure for describing the contents of the element.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1185.** |
| 2866 | Stephen McCann | 128.20 | 35.3.2.3 | What do Element L and Element Y refer to within Figure 35-1 | Some text needs to be written to explain what these Elements are referring to. | **Revised**  Agree with the commenter. The figure was simplified to provide a specific example – i.e., that of Association Request frame. In addition, a descriptive text was added after the figure for describing the contents of the element.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2866.** |
| 3335 | Yusuke Tanaka | 128.26 | 35.3.2.3 | Please clarify what k, x, y, L and Y mean in figure 35-1. | As commented. | **Revised**  Agree with the commenter. The figure was simplified to provide a specific example – i.e., that of Association Request frame. In addition, a descriptive text was added after the figure for describing the contents of the element.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 3335.** |
| 2309 | Ming Gan | 128.06 | 35.3.2.3 | In Fig 35-1, some fields except for Per STA Control field in Per-STA Profile are missing | As in comment | **Revised**  Agree with the commenter. The figure was simplified to provide a specific example – i.e., that of Association Request frame. In addition, a descriptive text was added after the figure for describing the contents of the element.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2309.** |
| 2964 | Tomoko Adachi | 0.00 | 9.4.2.295b.2 | Information of additional requested links needs to be provided when used in (Re)Association Request frames. | As in comment. | **Revised**  Agree with the commenter. Approved text from 11-21/242r4 (incorporated in D0.4) already mentions that (Re)Association Request and Response frames carry complete profile in the per-sta profile. In addition, text in clause 35.3.2.2 and an example figure were added to clarify this aspect.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2964.** |

**35.3.2.2 Complete or partial per-STA profile**


***TGbe: Please delete the following NOTE after the paragraph starting “An AP affiliated with an AP MLD shall include, in (Re)Association Response frame” as shown below***

***TGbe: Please move the following paragraph and figure from clause 35.3.2.3 to this clause after the paragraph starting “An AP affiliated with an AP MLD shall include, in (Re)Association Response frame” and apply additional changes to the text and the figure as shown below:***

[CID 1860]When carried in a Management frame transmitted by an STA affiliated with an MLD, each Per-STA Profile subelement, that is a complete profile, shall comprise of the following:

* [CID 1035, 2451]the STA Control field,
* [CID 2451][CID 2451]
* [CID 1035, 2451]the STA Info field,
* [CID 2451]and the STA Profile field, with the following rules:
  + [CID 1036, 1864, 2451, 2964]If the reporting STA is an AP, the STA Profile field corresponding to the reported AP carries of [CID 2586]fields and elements [CID 1184](subject to inheritance rules defined in 35.3.2.3) in the order defined in Table 9-39, if the frame a Probe Response frame, that is an ML probe response or Table 9-35, if the frame is an Association Response frame or Table 9-37, if the frame is a Reassociation Response frame.
  + [CID 1036, 2451]If the reporting STA is a non-AP, the STA Profile field corresponding to the reported non-AP STA carries of [CID 2586]fields and elements [CID 1184](subject to inheritance rules defined in 35.3.2.3) in the order defined in Table 9-34 (Association Request frame body) if the frame is an Association Request frame or Table 9-36 if the frame is a Reassociation Request frame.
  + [CID 1035]The Timestamp field, AID field, Listen Interval field, Current AP Address field, and BSS Max Idle Period element are not included in the Per-STA Profile subelement.
  + When included, the Non-Inheritance element appears as the last element in the profile and carries a list of elements that are not inherited by the reported STA from the reporting STA (see 35.3.2.3).

[CID 1860, 1184, 1185, 2866, 3335, 2309, 2964]An example of a Basic variant Multi-Link element, carried in an Association Request frame, containing a complete per-STA profile is shown in Figure 35-1 (Example of Basic variant Multi-Link element in an Association Request Frame).



**Figure 35-1 – Example of Basic variant Multi-Link element in an Association Request frame**[CID 1860, 1035, 1864, 1184, 1185, 2866, 3335, 2309, 2964]

***TGbe editor: Please insert the paragraph below Figure 35-1 as shown below:***

[CID 1184, 1185, 2866, 3335, 2309, 2964]In Figure 35-1 (Example of Basic variant Multi-Link element in an Association Request Frame), a STA affiliated with a non-AP MLD, transmits an Association Request frame which includes Basic variant Multi-Link element that carries the complete profile of two other STAs affiliated with its non-AP MLD (STA x and STA y). The figure expands the Per-STA profile for one of the reported STA. The Type subfield of the Multi-Link Control field is set to 0 to indicate that the Multi-Link element is a Basic variant Multi-Link element. The Common Info field carries information that applies to the MLD level as described in 9.4.2.295b.2 (Basic variant Multi-Link element). In this example, only the MLD MAC Address field is shown. However, there can be other field present in the Common Info portion whose presence is signaled via the subfields in the Multi-Link Control field. Each Per-STA Profile subelement in the Link Info field carries the complete profile, with inheritance applied, of a reported STA affiliated with the non-AP MLD. Each Per-STA Profile subelement carries the STA Control field as the first field, followed by the STA Info field and the STA Profile field. In this example, only the STA MAC Address field is shown. However, there can be other field present in the STA Info portion whose presence is signaled via the subfields in the STA Control field. The STA Profile field carries variable number of fields and elements in the order defined in Table 9-34 with inheritance applied (see 35.3.2.3).

**9.4.2.295b.2 Basic variant Multi-Link element**[CID 1035, 2183, 2451]

***TGbe editor: Please update the text after Table 9-322an as follows:***

Each Per-STA Profile subelement starts with STA Control field followed by the STA Info field and the STA Profile field as defined in 35.3.2 (Container for multi-link information).

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | Subelement ID | | | Length | STA Control | STA Info | STA Profile |
| Octet: |  | 1 |  | 1 | TBD | variable | variable |

**Figure 9-788xx—Per-STA Profile subelement format**

The format of the STA Control field is defined in [Figure 9-788ej (STA Control field format)](#bookmark46).

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | B0 |  | B3 | B4 | B5 | B6 | B7 TBD |
|  | Link ID | | Complete Profile | Beacon Interval Present / MAC Address Present | DTIM Info Present | Reserved |
| Bits: |  | 4 |  | 1 | 1 | 1 | TBD |

### Figure 9-788ej—STA Control field format

***TGbe editor: Please add the following paragraphs after the paragraph starting: “The Complete Profile subfield is…” as follows:***

When the Basic variant Multi-Link element is transmitted by an STA affiliated with a non-AP MLD, bit B5 of STA Control field represents the MAC Address Present subfield.

When the Basic variant Multi-Link element is transmitted by an AP affiliated with an AP MLD, bit B5 of STA Control field represents the Beacon Interval Present subfield.

The MAC Address Present subfield indicates the presence of the STA MAC Address subfield in the STA Info field. The MAC Address Present subfield is set to 1 if the STA MAC Address subfield is present in the STA Info field; otherwise set to 0.

The Beacon Interval Present subfield indicates the presence of the Beacon Interval subfield in the STA Info field. The Beacon Interval Present subfield is set to 1 if the Beacon Interval subfield is present in the STA Info field; otherwise set to 0.

The DTIM Info Present subfield indicates the presence of the DTIM Info subfield in the STA Info field. The DTIM Info Present subfield is set to 1 if the DTIM Info subfield is present in the STA Info field; otherwise set to 0. A non-AP STA sets the DTIM Info Present subfield to 0 in transmitted Basic variant Multi-Link element.

***TGbe editor: Please delete “Other subfields are TBD.” and add the following paragraphs as shown below:***

The STA MAC Address subfield carries the MAC address of the STA affiliated with the non-AP MLD that can operate on the link identified by the Link ID subfield.

When the Basic variant Multi-Link element is transmitted by a STA affiliated with a non-AP MLD:

The Beacon Interval subfield is optionally present and is defined in 9.4.1.3 (Beacon Interval field).

The DTIM Info subfield is optionally present and has the format as defined in Figure 9-788xx.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | DTIM Period | | | DTIM Count |
| Octet: |  | 1 |  | 1 |

**Figure 9-788xx—DTIM Info subfield format**

The DTIM Period field and the DTIM Count field are defined in 9.4.2.5 (TIM element).

The contents of the STA Profile field when a STA affiliated with an MLD transmits the Basic variant Multi-Link element are defined in clause 35.3.2.2

**9.4.2.295b.3 Probe Request variant Multi-Link element**[CID 1035, 2451, 2183]

***TGbe editor: Please update the add the following paragraph in this subclause as shown below:***

The Per-STA Profile Subelements field contains zero or more Per-STA Profile subelements as defined in 9.4.2.295b.2 (Basic variant Multi-Link element). Each Per-STA Profile subelement starts with a STA Control field as defined in 9.4.2.295b.2 (Basic variant Multi-Link element). Bits B5 and B6 of the STA Control field of the Probe Request variant Multi-Link element are reserved and set to 0.

**35.3.2.3 Inheritance in a per-STA profile**[CID 1860]

***TGbe editor: Please move the following text and Figure 35-1 to clause 35.3.2.2 as shown below***

**PART C**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Pg/Ln** | **Section** | **Comment** | **Proposed Change** | **Resolution** |
| 2472 | Payam Torab Jahromi | 127/08 | 35.3.2.3 | STAs of an MLD may not have similar capabilities, so suggest to change the justification for inheritance. Inheritance is a tool that opportunistically reduces the frame size. Also "would inherit" -> inherits. | Change the first paragraph to "It is possible for STAs of an MLD to have similar capabilities and operational parameters on different links. As a result some elements carried in the per-STA profile for a reported STA can be identical to same elements for the reporting STA. To reduce the frame size, when a per-STA profile carries complete information for a reported STA, it inherits the elements from the reporting STA." | **Revised**  **TGbe editor, please apply the change as suggested by the comment while adding a comma “,” after the “As a result” in the second sentence. NOTE, this change is not shown in document 11-21/0254r0.** |
| 2296 | Michael Montemurro | 127/10 | 35.3.2.3 | This information is neither useful or relevant to any requirements in the specification. | At cited location, delete "In order to reduce frame bloating," | **Revised**  Agree with the commenter. The cited part of the sentence was removed as a resolution to CID 2472.  **TGbe editor, no changes are needed to address this comment.** |
| 2868 | Stephen McCann | 127/12 | 35.3.2.3 | The term "complete information" needs to be defined in this clause, or a forward reference needs to be added. | Move the paragraph at P130L13, to the cited clause. | **Revised**  The description of complete information was added to clause 35.3.2.2 by 11-21/242r4 (and appears in D0.4). Please see D0.4 pg 191 ln 38  **TGbe editor: no further action is required as a resolution to this CID.** |
| 2167 | Laurent Cariou | 0.00 | 35.3.2.3 | Clarify that the inheritence only applies when the complete information is provided | as in comment | **Revised**  Agree with the commenter. A note was added to clarify.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 2167.** |
| 3021 | Xiaofei Wang | 127/19 | 35.5.2.3 | It is unclear to which frame "the frame" refers. Please rewrite and clarify | as in comment | **Revised**  The statement was clarified to state that the frame refers to the one that is carrying the Basic variant Multi-Link element.  A figure was added to clause 35.3.2.3 along with description to explain inheritance when the profile carries complete information.  A figure was also added to clause 35.3.17 along with description to explain inheritance in a multiple BSSID scenario.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 3021.** |
| 3212 | Young Hoon Kwon | 127.18 | 35.3.2.3 | In case the reported STA is affiliated with the same MLD as an MLD that an AP of a nontransmitted BSSID is affiliated with, it is not clear if the reporting STA implies the AP of the nontransmitted BSSID or the reporting STA implies another AP corresponding to the transmitted BSSID. Further clarification is needed. | As shown in the comment. | **Revised**  Agree with the comment. For the scenario described in the comment, the reporting STA is the AP corresponding to the transmitting BSSID. In addition, an example figure and description text was added to clause 35.3.17 to explain the inheritance in a multiple BSSID set.  **TGbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 3212.** |
| 3369 | Zhiqiang Han | 127.17 | 35.3.2.3 | No any condition is specified in the Table 9-32,please clarify it | Please clarify it. | **Revised**  The identified statement was clarified to state that the condition for the existence of a certain element in a Management frame is given by the table corresponding to that frame in Clause 9.3.3.  **Tgbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 3369.** |
| 3370 | Zhiqiang Han | 127.19 | 35.3.2.3 | which condition? where is the corresponding condition? | Please clarify it. | **Revised**  The identified statement was clarified to state that the condition for the existence of a certain element in a Management frame is given by the table corresponding to that frame in Clause 9.3.3.  **Tgbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 3370.** |

**35.3.2.3 Inheritance in a per-STA profile**

***TGbe editor: Please add NOTE after the first paragraph as shown below:***

[CID 2167]NOTE – The inheritance mechanism described in this subclause is not applicable when the Per-STA Profile subelement of the Basic variant Multi-Link element carriers the partial information of the reported STA.

***TGbe editor: Please split the second paragraph as shown along with additional changes shown below:***

[CID 3021, 3212, 3369, 3370]A STA that transmits a Management frame carrying the Basic variant Multi-link element shall include an element that is specific to the reported STA in the complete profile of the reported STA carried in the Basic variant Multi-Link element. An element is specific to a reported STA if any one of the following conditions is satisfied:


* its value is different from the element, if advertised by the reporting STA that has the same Element ID and Extended Element ID (if present)
* the reported STA satisfies the condition for that element to be included in the frame that carries the Basic variant Multi-Link element while the reporting STA does not satisfy the corresponding condition.

NOTE – The conditions to include an element in a particular Management frame are as specified in clause 9.3.3 (for example, Table 9-35 specifies the conditions for an element to be included in an Association Response frame).

When an element that is carried in a Management frame transmitted by the reporting STA is not present in a complete profile of a reported STA, then the element is considered to be part of the reported STA’s profile and the value to use is the same as that of the corresponding element carried in the reporting STA’s frame unless the complete profile carries the Non-Inheritance element (see 9.4.2.240 (Non-Inheritance element)) and the element is listed in the Non-Inheritance element.

***TGbe editor: Please add the following description text and figure before the last paragraph as shown below:***

[CID 3021, 3212]Figure 35-xx (Example of inheritance in a complete per-STA profile) illustrates inheritance when a per-STA profile carries complete information. The example shows a Management frame transmitted by a reporting STA that is affiliated with an MLD. The Management frame carries several elements with their corresponding element IDs shown in parenthesis. The frame also carries Basic variant Multi-Link element which is carrying a complete profile for a reported STA x. The per-STA profile for STA x includes elements with ID B and D since the elements have value different from the corresponding elements carried in the frame. The profile also includes element with ID Y which is specific to STA x. In addition, elements with ID C and ID F are inherited and are not carried in the profile for STA x. The values for these two elements are the same as that carried in the frame. Furthermore, elements with ID A and ID E are not applicable to STA x as their corresponding (Extended) Element IDs are listed in the Non-Inheritance element.




**Figure 35-xx: Example of inheritance in a complete per-STA profile**[CID 3021]

**35.3.17 Multi-BSSID**[CID 3021, 3212]

***TGbe editor: Please add the following description text and figure at the end of this subclause as shown below:***

Figure 35-yy (Example of inheritance in a complete per-STA profile for a Multiple BSSID scenario) illustrates inheritance when a per-STA profile carries complete information in a Basic variant Multi-Link element that is contained in a Nontransmitted BSSID Profile of a Multiple BSSID element. The example shows a Management frame transmitted by a transmitted BSSID. The Management frame carries several elements with their corresponding element IDs shown in parenthesis. The frame also carries Multiple BSSID element which includes profile for nontransmitted BSSID N. The Nontransmitted BSSID Profile contains Basic variant Multi-Link element carrying complete profile for AP x. The BSSID N is inheriting elements with ID B, C and E. It does not inherit element with ID A and is listed in the Non-Inheritance element. Since the value of element F for BSSID N is not the same as that advertised by the transmitted BSSID, the element is carried in the profile for BSSID N. An element with ID Y is specific to the BSSID N and is included in its profile. AP x inherits elements with ID D and F directly from the BSSID N and element with ID C indirectly from the transmitted BSSID (via the BSSID N’s inheritance). AP x does not inherit element A (same as nontransmitted BSSID). The elements with ID B and Y are specific to AP x and appear in its profile. Furthermore, AP x does not inherit element E from the transmitted BSSID and is listed in the Non-Inheritance element present in its profile.



**Figure 35-yy: Example of inheritance in a complete per-STA profile for a Multiple BSSID scenario**

**PART D**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Pg/Ln** | **Section** | **Comment** | **Proposed Change** | **Resolution** |
| 1005 | Abhishek Patil | 57.50 | 9.3.3.2 | Fix the TBD - the Basic variant of ML IE is optionally present in the beacon (for example when the AP support SAE authentication) | As in comment | **Revised**  During discovery, an AP affiliated with an AP MLD needs to identify that it supports multi-link operation and that it is affiliated with an AP MLD. Therefore, the AP’s Beacon frame or a Probe Response frame (that is not a ML probe response) needs to carry Basic variant Multi-Link element carrying the MAC Address of the AP MLD. At the same time, such frames should not be bloated and must limit the amount of information they carry. Therefore, these frames must only carry the Common Info field unless certain conditions, that require the per-STA profile to be present are satisfied.  Resolves two TBDs  **Tgbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1005.** |
| 1896 | Jeongki Kim | 57.52 | 9.3.3.2 | The Basic variant Multi-Link element will be present in the Beacon frame if the AP is affiliated with an AP MLD. So remve the TBD in the related text. If there is the case that does not include ML element, change TBD to optionally. | Either Remove the TBD or change TBD to optionally | **Revised**  During discovery, an AP affiliated with an AP MLD needs to identify that it supports multi-link operation and that it is affiliated with an AP MLD. Therefore, the AP’s Beacon frame or a Probe Response frame (that is not a ML probe response) needs to carry Basic variant Multi-Link element carrying the MAC Address of the AP MLD. At the same time, such frames should not be bloated and must limit the amount of information they carry. Therefore, these frames must only carry the Common Info field unless certain conditions, that require the per-STA profile to be present are satisfied.  Resolves two TBDs  **Tgbe editor please implement changes as shown in doc 11-21/0254r0 tagged as 1896.** |

***TGbe editor: Please update the add the following Tables as shown below:***

**Table 9-32—Beacon frame body**[CID 1005, 1896]

|  |  |  |
| --- | --- | --- |
| **Order** | **Information** | **Notes** |
| <ANA> | Multi-Link | The Basic variant Multi-Link element is present if the AP is affiliated with an AP MLD. Otherwise it is not present. |

**Table 9-39—Probe Response frame body**[CID 1005, 1896]

|  |  |  |
| --- | --- | --- |
| **Order** | **Information** | **Notes** |
| <ANA> | Multi-Link | The Basic variant Multi-Link element is present if the AP is affiliated with an AP MLD. Otherwise it is not present. |

**35.3.4.4 Multi-link element usage rules in the context of discovery**[CID 1005, 1896]

***TGbe editor: Please update the following paragraph in this subclause as shown below:***

An AP affiliated with an AP MLD shall include, in a Beacon frame or a Probe Response frame, which is not an ML probe response, only the Common Info field of the Basic variant Multi-Link element as defined in 9.4.2.295b (Multi-Link element) unless conditions in 35.3.9 are satisfied.

An AP affiliated with an AP MLD shall include the MLD MAC address of that AP MLD in the Beacon and Probe Response frames it transmits in the Common Info field of the Basic variant Multi-Link element.