IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution for TBD in OFDM modulation | | | | |
| Date: 2021-04-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Rui Cao | NXP | 350 Holger Way, San Jose, CA 95134 |  | rui.cao\_2@nxp.com |
|  |  |  |  |  |

Abstract

This submission proposed for one TBD in the OFDM modulation (36.3.13.12) in TGbe D0.4.

Revisions:

* Rev 0: Initial version of the document.

**Discussions**: The draft text for Segment deparser is updated in 802.11-21/0543r1. Since STBC is not defined for 11be, need to update the notation of the signal in the OFDM modulation equation using the one from Segment deparser.

*TGbe Editor: Please make the following change in P413L31 in subclause 36.3.13.12 of D0.4.*

**34.3.13.12 OFDM modulation**

The time domain waveform of the Data field of an EHT PPDU that is not an EHT TB PPDU for transmit chain , , shall be as defined in Equation (36-83).

(36-83)

*TGbe Editor: Please make the following change in P413L63 in subclause 36.3.13.12 of D0.4.*

is the transmitted constellation for user in the -th RU/MRU at subcarrier k, spatial stream m, and Data field OFDM symbol and is defined by Equation (36-84).

(36-84)

*TGbe Editor: Please make the following change in P414L31 in subclause 36.3.13.12 of D0.4.*

The time domain waveform of the Data field of an EHT TB PPDU for user in the -th RU/MRU from transmit chain , , shall be as defined in Equation (36-86).

(36-86)