IEEE P802.11
Wireless LANs

|  |
| --- |
| CR for CID 2162 and 2163 |
| Date: 2021-04-22 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Ming Gan | HuaweiHuawei |  |  | ming.gan@huawei.com |
| Jason Yuchen Guo |  |  |  |
| Yunbo Li | Huawei |  |  |  |
| Guogang Huang | Huawei |  |  |  |
| Yiqing Li | Huawei |  |  |  |
| Mengyao Ma | Huawei |  |  |  |
| Hongjia Su | Huawei |  |  |  |

Abstract

This submission proposes resolutions of comments received from TGbe comment collection (TGbe Draft 0.4).

* 2162, 2163

Revisions:

* Rev 0: Initial version of the document.
* Rev 2: Add the condition of MLD ID presence based on Laurent’s suggestion
1. **Introduction**

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. The introduction and the explanation of the proposed changes are not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11be editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause**  | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
| 2162 | Laurent Cariou | 9.4.2.295b.3 |   |   | "The subfields of the Multi-Link Control field of the Probe Request variant Multi-Link element except the Type subfield are TBD." All these subfields should be set to 0 as no other information is needed in MLD probe request | as in comment | **Revised.**Propose to add MLD ID into the Probe Request variant Multi-Link element to simplify the parsing at the AP MLD side, please refer to the discussion part in this document for the detailTGbe editor to make the changes shown in 21/0741r3 under all headings that include CID 2162. |
| 2163 | Laurent Cariou | 9.4.2.295b.3 |   |   | "The presence and format of the Common Info field in the Probe Request variant Multi-Link element are TBD." It is much simpler if the format is identical as the basic type, and to set all control bits that indicate presence of fields to 0, so that there are no fields present | as in comment | **Revised.**Propose to add MLD ID into the Probe Request variant Multi-Link element to simplify the parsing at the AP MLD side, please refer to the discussion part in this document for the detail TGbe editor to make the changes shown in 21/0741r3 under all headings that include CID 2163. |

**Discussion:** None.

The non-AP MLD could use the following setting for the ML Probe Request frame

1. The A1 and A3 address fields are set to the MAC address of the recipient AP which parses this ML Probe Request frame (from which the RNR element is received)
2. The MLD ID subfield in the common part of Probe Request variant ML element is set to MLD ID of the targeted AP MLD

Note -this basic info of the AP MLD, such as MLD ID, could be easily obtained by RNR element. And ML Probe Rquest is only used outside the context of active scanning

The benefit with MLD ID is clear (it can not be obtained by other methods)

* **ML Probe Request frame can be used to solicit the info of any single AP MLD as shown in the following figure (assume AP\_1x is the recipient AP)**
	+ An AP MLD which includes the recipient AP, such as MLD 1
	+ An AP MLD which contains the non-transmitted BSSID that in the same multiple BSSID set as the recipient AP, such as MLD 3
	+ An AP MLD for which there is no affiliated AP working on the same link as the recipient AP and there is at least one AP of the AP MLD is in the same multiple BSSID set as an AP affiliated with the AP MLD of the recipient AP, such as MLD 2
* **The RA of ML Probe Request frame can always be set to the MAC address of the recipient AP that corresponds to the transmitted BSSID , such that to simplify the parsing at the AP MLD side**



***TGbe editor: Please modify the subclause 9.4.2.247b.3Probe Request variant Multi-Link element as follows***

**9.4.2.247b.3 Probe Request variant Multi-Link element**

The Probe Request variant Multi-Link element is used to request an AP to provide information of other APs affiliated with the same AP MLD as the AP. The inclusion of a Probe Request variant Multi-Link element in a Probe Request frame identifies it as an MLD probe request.

The format of the Presence Bitmap subfield of the Probe Request variant Multi-Link element is defined in Figure 9-788xx (Presence Bitmap subfield of the Probe Request variant Multi-Link element format).

|  |  |  |
| --- | --- | --- |
|  | B0  | B1 B11 |
|  | MLD ID Present | Reserved |
| Bits: | 1 | 11 |
| Figure 9-788xx—Presence Bitmap subfield of the Probe Request variant Multi-Link element format |

The MLD ID Present subfield is set to 1 if the MLD ID field is present in the Common Info field. Otherwise the MLD ID Present subfield is set to 0.

The format of the Common Info field of the Probe Request variant Multi-Link element is defined in Figure 9-788yy (Common Info field of the Probe Request variant Multi-Link element).

|  |  |
| --- | --- |
|  | MLD ID |
| Octets: | 0 or 1 |
| Figure 9-788yy—Common Info field of the Probe Request variant Multi-Link element |

The MLD ID subfield indicates the identifier of the AP MLD to which the ML Probe Request frame that carries the Probe Request variant Multi-Link element is targeted. (#CID2162, 2163)

The format of the Link Info field of the Probe Request variant Multi-Link element is defined in Figure 9-788ek (Link Info field of the Probe Request variant Multi-Link element format).

|  |  |
| --- | --- |
|  | Per-STA Profile Subelements |
| Octets: | Variable |
| Figure 9-788ek—Link Info field of the Probe Request variant Multi-Link element |

The Per-STA Profile Subelements field contains zero or more Per-STA Profile subelements as defined in 9.4.2.295b.2 (Basic variant Multi-Link element). Each Per-STA Profile subelement starts with a Per-STA Control field as defined in 9.4.2.295b.2 (Basic variant Multi-Link element).

A Per-STA Profile subelement includes only a (Extended) Request element if a non-AP STA requests partial information from the AP corresponding to the per-STA profile, and does not include any elements if the non-AP STA requests complete information from the AP. If the (Extended) Request element is present in the Per-STA Profile subelement, the Complete Profile subfield of the Per-STA Control field shall be set to 0.

***TGbe editor: Please modify the subclause 35.3.4.2 Use of ML probe request and response as follows***

**35.3.4.2 Use of ML probe request and response**

An ML probe request is a Probe Request frame that is sent outside the context of active scanning that is used to discover an AP:

—with the Address 1 field set to the broadcast address and the Address 3 field set to the BSSID of an AP, or with the Address 1 field set to the BSSID of an AP’s BSS.

—with the MLD ID subfield (if present) set to the MLD ID which identifies the targeted AP MLD (#CID2162, 2163)

—and that includes a Probe Request variant Multi-Link element defined in 9.4.2.295b.3 (Probe Request variant Multi-Link element).

If either the Address 1 field or the Address 3 field of the ML Probe Request frame is set to MAC address of the AP affiliated with an AP MLD that corresponds to the nontransmitted BSSID, then MLD ID Present subfield in the Probe Request variant Multi-Link element of the ML Probe Request frame is set to 0. Otherwise, MLD ID Present subfield in the Probe Request variant Multi-Link element of the ML Probe Request frame is set to 1. (#CID2162, 2163)

…

An ML probe response is a Probe Response frame:

—that is transmitted in response to receiving an ML probe request

—and that includes Basic variant Multi-Link element which can carry complete or partial per-STA profile(s), based on the soliciting request, for each of the requested AP(s) of the AP MLD.