IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolution for CIDs related to ML probe response |
| Date: 2021-12-01 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Jiin Kim | LG Electronics | 19, Yangjae-daero 11gil, Seocho-gu, Seoul 137-130, Korea |  | jiin.kim@lge.com |
| Insun Jang | LG Electronics |  | insun.jang@lge.com |
| Sunhee Baek | LG Electronics |  | sunhee.baek@lge.com |
| Jinsoo Choi | LG Electronics |  | js.choi@lge.com |

Abstract

This document proposes resoulution for CIDs 6449, 5252 related ML probe response.

Revisions:

* Rev 0: initial version of the document
* Rev 1: Revised resolutions

***TGbe editor: Please note that baseline is 11be D1.5.***

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Pg/Ln** | **Section** | **Comment** | **Proposed Change** | **Resolution** |
| 6449 | 251/55 | 35.3.4.2 | We need to consider the nontransmitted BSSID set case for partial info request. Please define a signaling for partial information request for nontransmitted BSSID set. | Please see the comment. | **Revised**Currently, the issue to include ML IE for the nontrasnmitted BSSID case is related to ML fragmentation being discussed. For that, both of proposals (from doc. 1508 and doc. 1869) have had the same direcition of including ML IE in ML Probe Response (frame) body with different details. Therefore, D1.5 already covers the case without separate descriptions for the nontrasnmitted BSSID case.**Note to the Editor:**No further changes are required for the resolution of this CID in this document |
| 5252 | 251/55 | 35.3.4.2 | In current draft, there is no case of partial info request for nontransmitted BSSID. Please add the case | As in the comment, we need to consider partial information request for the case of nontransmitted BSSID | **Revised**Currently, the issue to include ML IE for the nontrasnmitted BSSID case is related to ML fragmentation being discussed. For that, both of proposals (from doc. 1508 and doc. 1869) have had the same direcition of including ML IE in ML Probe Response (frame) body with different details. Therefore, D1.5 already covers the case without separate descriptions for the nontrasnmitted BSSID case.**Note to the Editor:**No further changes are required for the resolution of this CID in this document. |

1. **Proposed spec text**

No further changes are required