IEEE P802.11 Wireless LANs

|  |
| --- |
| Channel numbering for LC HT and LC VHT PHY modes |
| Date: 2021-09-03 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Chong Han  | pureLiFi |  |  | chong.han@purelifi.com  |
| Nikola Serafimovski  |  |  | nikola.serafimovski@purelifi.com |
| Stephan Berner |  |  | stephan.berner@purelifi.com |
| Mostafa Afgani |  |  | Mostafa.afgani@purelifi.com |
| Tamas Weszely |  |  | Tamas.weszely@purelifi.com |

Abstract

This document provides text to be incorporated in the TGbb draft for the channel numbering for LC HT and LC VHT PHY modes.

## 32.3.2.1.2 Channelization for the other LC PHY modes

Channel center frequencies are defined at every integer multiple of 5 MHz above the channel starting frequency. The relationship between center frequency and channel number is given in Equation (1)

Channel center frequency = Channel starting frequency + 5 x nch (MHz) (1)

where nch = 1,..., 61 and Channel starting frequency = 21 MHz.

The channel bandwidths supported by each LC PHY mode is available in 32.3.2 (LC PHY modes). The set of valid operating channel numbers is defined in Table E-4 in E.1. (Country information and operating classes).

###