IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolutions to 32.3.9.9 Midambles | | | | |
| Date: 2021-09-13 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Yujin Noh | Senscomm |  |  | yujin.noh at senscomm.com |
|  |  |  |  |  |

Abstract

This submission shows


* Comments from TGbd draft 2.0.
* Resolutions applied to TGbd draft 2.0.
* 1 CIDs: 2108

Revisions:


* Rev 0: Initial version of the document.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 2108 | 100.63 | N\_MA is a derived number instead of a set number. | Revise to "when N\_MA is greater than zero in accordance with eq. (32-36)." | Revised  Agreed in principle. The text is improved based on the proposed change.  TGbd Editor: Incorporate the changes in 11-21-1466-00-00bd- Resolutions to 32.3.9.9 Midambles |

***Discussion***



However, it is calculated based as below.

******

***To TGbd Editor:*** ***P100L63*** *update the description as below.*

***------------- Begin Text Changes ---------------***

An NGV STA shall include midambles in an NGV PPDU transmission when *NMA* is ~~set to a nonzero value~~ greaterthan zero in accordance with Equation (32-36).

***------------- End Text Changes ------------------***