IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CC36 comment resolution: Multi-Link Fragmentation | | | | |
| Date: 2020-08-20 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Liwen Chu | NXP |  |  | Liwen.chu@nxp.com |

Abstract

This submission proposes resolutions for multiple comments related to TGbe D1.0 with the following CIDs:

5063, 4015

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **PP** | **LL** | **Comment** | **Proposed Change** | Resolution |
| 5063 | 133 | 32 | When a Per-STA Profile subelement of the Basic variant Multi-Link element carries the complete profile of a reported STA of an MLD, even with inheritance, there may be scenarios where the size of the subelement exceeds 255 octets. It is not clear how the spec addressed this scenario. | As in comment. The commenter will provide a contribution to address this issue. | **Revised**  Agree with the commenter. A procedure to fragment the Per-STA Profile subelement when the size of the subelement content exceeds 255 octets is defined. MLProbe Request/Response Action frames are defined to avoid the fragmentation of ML element and Per-STA Profile as subelement in Multiple BSSID element. This can avoid the implementation complexity.  **TGbe editor, please incorporate changes as shown in 11-21/1508r0 tagged 5063** |
| 4015 | 133 | 27 | Table 9-92 indicates if an element is fragmentable or not. Clause 10.28.11 defines the procedure if the Information field of a fragmentable element is more than 255 octets. However, there is no procedure defined for the case where the Data field of a subelement (within an element) is more than 255 octets. It is possible that the Per-STA Profile subelement of the Basic variant Multi-Link element is greater than 255 octets. | Define a procedure to handle the case where the Per-STA Profile subelement carries in the Link Info field of Multi-Link element is greater than 255 octets. | **Revised**  Agree with the commenter. A procedure to fragment the Per-STA Profile subelement when the size of the subelement content exceeds 255 octets is defined. MLProbe Request/Response Action frames are defined to avoid the fragmentation of ML element and Per-STA Profile as subelement in Multiple BSSID element. This can avoid the implementation complexity.  **TGbe editor, please incorporate changes as shown in 11-21/1508r0 tagged 5063** |

Discussion:

Each Per-STA Profile carries information specific to a STA affiliated with an MLD. For example, during MLO discovery and ML (re)setup, the Per-STA Profile subelement for each reported STA carries complete profile. When the profile carries complete information, the inheritance mechanism would help keep the profile size small. However, in scenarios where the reported STA has many fields/elements that are different from the reporting STA or specific to the reported STA, it is possible that the subelement size exceeds 255 octets. The Multi-Link element is fragmentable and the procedures described in clause 10.28.11 and 10.28.12 would apply. However, there is no procedure defined for handling the case where a subelement size exceeds 255 octets. For example, the length field in the subelement can only signal up to 255 octets. The MLO framework needs to define a procedure for fragmenting a subelement when the content of the subelement exceed 255 octets. This issue is not seen in case of Nontransmitted BSSID Profile subelement carried in a Multiple BSSID element because the baseline standard requires carrying multiple Multiple BSSID elements with the nontransmitted BSSID profile fragmented across multiple Nontransmitted BSSID Profile subelements that are carried across different Multiple BSSID element. Also note, Multiple BSSID element is a legacy element and can’t be fragmented – i.e., Fragment element (defined by 11ai) does not apply to Multiple BSSID element.

This contribution defines a subelement fragmentation procedure for Per-STA Profile subelement of Multi-Link element that is similar to the element fragmentation procedure described in 10.28.11.

The fragmentation of Multi-Link element dsisussed above can be used when an AP affiliated with an AP MLD that doesn’t support Mutiple BSSID or an AP affiliated with an AP MLD that has transmitted BSSID transmit basic variant Multi-Link element.

When an AP with transmitted BSSID transmits basic variant Multi-Link element for a AP MLD that has affiliated AP with nontransmitted BSSID in reporting link, the Multi-Link element is carried in Multiple BSSID element as shown below.

Multiple BSSID element

Nontransmitted BSSID profile subelement

Multi-link element

Per STA profile subelement

Specific element

Accordingly, the following fragmentation may be needed when Multi-Link element is carried in Multiple BSSID lement. This is complecated for the implementation.

Multiple BSSID element > 255

=> multiple Multiple BSSID elements

Nontransmitted BSSID profile subelement > 255

* Spread out into two subelement in different multiple BSSIDelement

Multi-link element >255

* 11ai frag/defrag without respecting element boundary in sublement

With length indication tweak

Per STA profile subelement > 255

* 11ai like subelement frag/defrag without length indication tweak

Specific element

One solution could be to define the Action frames for ML probe request and ML probe response frame where an AP with nontransmitted BSSID that is affiliated with AP MLD can transmit ML probe response frame. With this update, the only new fragment requirement is the fragmentation of Multi-Link element when it is not carried in subelement.

End of the discussion

**9.4.2.295b.2 Basic variant Multi-Link element**

***TGbe editor: Please update Table 9-322ap as shown below:***

The Subelement ID field values for the defined subelements are shown in [Table 9-322ap (Optional subelement IDs for Basic variant Multi-Link element)](#bookmark105).

**Table 9-322ap—Optional subelement IDs for Basic variant Multi-Link element**[5063]


|  |  |  |
| --- | --- | --- |
| **Subelement ID** | **Name** | **Extensible** |
| 0 | Per-STA Profile | Yes |
| 1–220 | Reserved |  |
| 221 | Vendor Specific | Vendor defined |
| 222 – 253 | Reserved |  |
| 254 | Fragment | No |
| 255 | Reserved |  |

***TGbe editor: Please add the following as a new subclause after subclause 35.3.2.3:***

**35.3.2.4 Per-STA Profile Subelement Fragmentation**[5063]

If the length of a Per-STA Profile subelement for a reported STA exceeds 255 octets, the transmitting STA shall fragment the contents across a series of subelements consisting of the Per-STA Profile subelement (Subelement ID set to 0), immediately followed by one or more Fragment subelements (Subelement ID set to 254) as illustrated in Figure 35.xx (Per-STA Profile subelement fragmentation). All the information for a fragmented subelement shall be carried across the same Basic variant Multi-Link element and its Fragment element(s). A Per-STA profile subelement shall not be fragmented if the length of the Data field of the subelement is less than 255 octets. A Fragment subelement shall not be the first subelement or the only subelement within a Link Info field of the Basic variant Multi-Link element.

NOTE – When the Per-STA Profile subelement length is greater than 255 octets, the length of Basic variant Multi-Link element that carries the subelement would exceed 255 octets. As a result, the element will be fragmented by following the procedure defined in 10.28.11 (Element fragmentation).



**Figure 35-xx: Per-STA Profile subelement fragmentation**

The information to be fragmented is divided into *P* + *Q* portions, where the following define each variable:

* *L* is the size of the information in octets.
* *P* is .
* *Q* is equal to 1 if *L* mod 255 > 0 and equal to 0 otherwise.

The Per-STA Profile subelement into which the information does not fit is filled with the first segment of information. This subelement is immediately followed by *P* – 1 Fragment subelements, each containing the subsequent segments of 255 octets of information. If *Q = 1*, these subelements are immediately followed by another Fragment subelement containing the remaining segment of information. The length of this last Fragment subelement shall be (L mod 255).

NOTE—A Fragment subelement never follows a subelement with fewer than 255 octets of information.

A Per-STA Profile subelement that has its information fragmented shall be followed by one or more Fragment subelements. To reconstruct the original information, the portion of information from the Per-STA Profile subelement shall be concatenated, in order, with the portions of information from the series of Fragment subelements that follow it. The defragmentation procedure shall complete when any subelement other than a Fragment subelement is encountered or the end of the last Fragment element of the Basic variant Multi-Link element is reached.

NOTE – The receiving STA follows the procedure defined in 10.28.12 (Element defragmentation) to defragment the Basic variant Multi-Link element.

* + - 1. **Probe Request frame format**

***TGbe editor: change 9.3.3.5 as follows(#5063)***

**Table 9-38—Probe Request frame body(#1004)(#2246)(#3357)**

|  |  |  |
| --- | --- | --- |
| **Order** | **Information** | **Notes** |
|  |  |  |
| <Last assigned + 1> | EHT Capabilities | The EHT Capabilities element is present if dot11EHTOptionIm- plemented is true; otherwise it is not present. |

**9.4.2.295b.3 Probe Request variant Multi-Link element**

***TGbe editor: change the first paragraph in 9.4.2.295b.3 as follows: (#5063)***

The Probe Request variant Multi-Link element is used to request an AP to provide information of other APs affiliated with the same AP MLD as the AP.(#2583)(#3360).

**9.6.7 Public Action details**

**9.6.7.1 Public Action frames**

***TGbe editor: add the following two rows in Table 9-408 (Public Action field values) of 9.6.7.1: (#5063)***

|  |  |
| --- | --- |
| <ANA> | MLProbe Request |
| <ANA> | MLProbe Response |

***TGbe editor: add the following subclauses in 9.6.7 as follows: (#5063)***

**9.6.7.x1 MLProbe Request frame format**

A STA affiliated to an non-AP MLD uses the MLProbe Request frame to solicit MLProbe Response from an AP affiliated with an AP MLD. The Action field of the MLProbe Request frame contains the information shown in Table 9-xxx1 (MLProbe Request frame Action field format).

**Table 9-xxx1 MLProbe Request frame Action field values**

|  |  |
| --- | --- |
| **Value** | **Meaning** |
| 1 | Category |
| 2 | Public Action |
| 3 | Request |
| 4 | Extended Request |
| 5 | Multi-Link |
| 6 | Vendor Specific |

**9.6.7.x2 MLProbe Response frame format**

An AP affiliated with an AP MLD responds with the MLProbe Response after receiving a MLProbe Request. The Action field of the MLProbe Response frame contains the Category, Public Action, the IEs of the reporting link requested in soliciting MLProbe Request (if any), and basic variant Multi-Link element.

**9.6.10 Protected Dual of Public Action frames**

***TGbe editor: add the following two rows in Table 9-448 (Public Action field values defined for Protected Dualof Public Action frames) of 9.6.10: (#5063)***

|  |  |  |
| --- | --- | --- |
| <ANA> | Protected MLProbe Request | 9.6.7.x1 (MLProbe Request frame format) |
| <ANA> | Protected MLProbe Response | 9.6.7.x2 (MLProbe Response frame format) |

**35.3.2 Advertisement of multi-link information in Multi-Link element(#2294)**

**35.3.2.1 General**

***TGbe editor: change the 1st, 2nd paragraphes in 35.3.2.1 as follows: (#5063)***

(#2241)(#1154)(#2850)(#2450)(#3366)(#3152)(#1716)(#2898)(#1155)(#1414)(#2581)(#3367)(#3359)(#2859)(#2295)An AP affiliated with an AP MLD shall follow the rules defined in 35.3.4.4 (Multi-Link element usage rules in the context of discovery) for including a Basic variant Multi-Link element in a Beacon frame that it transmits or in a Probe Response frame that it transmits.

(#1155)(#1414)(#2581)(#3367)(#3359)(#2859)(#2295)An AP affiliated with an AP MLD shall follow the rules in 35.3.4.2 (Use of MLProbe Request and Response (#2583)(#3360)) for including a Basic variant Multi-Link element in a MLProbe Response frame that it transmits.

***TGbe editor: change the 4th paragraph in 35.3.2.1 as follows: (#5063)***

(#1183)(#1777)(#1918)(#2414)(#2582)(#3211)(#3249)(#3368)(#2182)(#2295)A STA affiliated with a non-AP MLD shall follow the rules in 35.3.4.2 (Use of MLProbe Request and Response (#2583)(#3360)) for including a Probe Request variant Multi-Link element in a MLProbe Request frame that it transmits.

**35.3.2.2 Advertisement of complete or partial per-link information(#1859)**

***TGbe editor: change 35.3.2.2 as follows (the paragraphes not shown are not changed): (#4018)***

……

(#1034)(#2149)(#1861)(#2831)An AP affiliated with an AP MLD shall not include a complete profile of a reported AP affiliated with the same AP MLD in the transmitted Beacon frame or a Probe Response frame as defined in 35.3.4.4 (Multi-Link element usage rules in the context of discovery) and 35.3.10 (Multi-link general procedures(#2324)(#2600)).

(#1858)(#1010)(#1128)The Basic variant Multi-Link element when carried in the Neighbor Report element shall not include a Link Info field.

(#1034)(#1833)(#2149)(#1861)(#2831)An AP affiliated with an AP MLD may include either the complete profile or the partial profile of a reported AP affiliated with the same AP MLD in a transmitted MLProbe Response frame, as defined in [35.3.4.2 (Use of MLProbe Request and Response (#2583)(#3360))](#bookmark13).

……

(#1860)When carried in a Management frame transmitted by an STA affiliated with an MLD(#2295), each Per-STA Profile subelement, that is a complete profile, shall comprise of the followings:

* (#1035)(#2451)The STA Control field (see Figure 9-788eo (STA Control field format(#1906)(#1907)(#1078)(#1475)(#2981))),
* the STA Info field (presence of subfields within the field are signaled in the STA Control field), and
* the STA Profile field with the following rules:
  + (#1036)(#1864)(#2451)(#2964)(#2586)(#1184)If the reporting STA is an AP, the STA Profile field corresponding to the reported AP carries fields and elements (subject to inheritance rules defined in [35.3.2.3 (Inheritance in a per-STA profile)](#bookmark8)) in the order defined in Table 9-39 (Probe Response frame body(#1004)(#2246)(#3359)), if the frame is a MLProbe Response, Table 9-35 (Association Response frame body(#1004)(#2246)(#3354)), if the frame is an Association Response frame, or Table 9-37 (Reassociation Response frame body(#1004)(#2246)(#3356)), if the frame is a Reassociation Response frame.
  + (#1036)(#2451)(#2586)(#1184)If the reporting STA is a non-AP STA, the STA Profile field cor- responding to the reported non-AP STA carries fields and elements (subject to inheritance rules defined in [35.3.2.3 (Inheritance in a per-STA profile)](#bookmark8)) in the order defined in Table 9-34 (Associ- ation Request frame body(#1004)(#2246)(#3353)) if the frame is an Assocation Request frame, or Table 9-36 (Reassociation Request frame body(#1004)(#2246)(#3355)) if the frame is a Reas- sociation Request frame.
  + (#1035)If the reporting STA is an AP, the Timestamp field, Beacon Interval field, AID field, SSID element, TIM element, and BSS Max Idle Period element are not included in the STA Pro- file field.
  + (#1035)If the reporting STA is a non-AP STA, the Listen Interval field and Current AP Address field are not included in the STA Profile field.
  + (#3315)Optionally, a Non-Inheritance element appears as the last element in the profile and car- ries a list of elements that are not inherited by the reported STA from the reporting STA (see
    - 1. [(Inheritance in a per-STA profile)](#bookmark8)).

……

**35.3.2.2.2 Inheritance in the per-STA profile of Probe Request variant Multi-Link ele- ment(#2416)**

***TGbe editor: change 35.3.2.2.2 as follows(the paragraphes not shown are not changed): (#5063)***

If a non-AP STA affiliated with a non-AP MLD requests the same partial information for an AP to which it sends an MLProbe Request and for another AP affiliated with the same AP MLD as the AP and that is requested in the MLProbe Request (see [35.3.4.2 (Use of MLProbe Request and Response(#2583)(#3360))](#bookmark13)), the non-AP STA may include the (Extended) Request element only in the Probe Request frame body, and this element will be inherited for the other requested AP even if it is not carried in the Per-STA Profile subelement corresponding to the other requested AP, following the rules defined in [35.3.4.2 (Use of MLProbe Request and Response(#2583)(#3360))](#bookmark13).

[Figure 35-5 (Example of inheritance in a Request element for MLProbe Request (#2416))](#bookmark11) illustrates a MLProbe Request transmitted by a non-AP STA that is affiliated with a non-AP MLD. The non-AP STA requests partial information for three APs and complete information for one AP, where all APs are affiliated with the same AP MLD. The non-AP STA includes a Request element in the Probe Request frame body requesting the element with element ID “a” for the AP to which the Probe Request frame is sent. The frame carries a Probe Request variant Multi-Link element that includes three Per-STA Profile subelements requesting information for AP x, AP y, AP z.

……

## Figure 35-5—Example of inheritance in a Request element for MLProbe Request (#2416)

***TGbe editor: change 35.3.4.2 as follows:(#5063)***

35.3.4.2 Use of MLProbe Request and Response(#2583)(#3360)

(#2583)(#3360)(#1187)An MLProbe Request is used to discover an AP:

* + - * + (#1045)(#1187)(#1673)(#2150)with the Address 1 field set to the broadcast address and the Address 3 field set to the BSSID of an AP, or with the Address 1 field set to the BSSID of an AP’s BSS.
        + (#1808)(#2124)(#3217)and that includes a Probe Request variant Multi-Link element defined in 9.4.2.295b.3 (Probe Request variant Multi-Link element).

(#1046)(#2151)(#2583)(#3360)(#1675)An MLProbe Request allows a non-AP STA to request an AP to include the complete or partial set of capabilities, parameters and operation elements of other APs affiliated to the same AP MLD as the AP. An AP affiliated to the same AP MLD as the AP identified in the Address 1 or Address 3 field of the Probe Request frame is a requested AP if one of the following conditions is met:

* + - * + the Multi-Link element in the Probe Request frame does not include any per-STA profile.
        + (#1420)the link ID of the AP is equal to the value in the Link ID field in a Per-STA Profile subelement in the Multi-Link element in the Probe Request frame.

(#1744)(#1047)The complete information of a requested AP is defined in [35.3.2.2 (Advertisement of](#bookmark6) [complete or partial per-link information(#1859))](#bookmark6).

(#2416)The partial information of a requested AP sent by a reporting AP consists of one or more elements that are requested in the (Extended) Request element carried in the MLProbe Request.

(#2416)If a STA affiliated with a non-AP MLD sends an MLProbe Request to an AP to retrieve partial information for AP(s) affiliated with the same AP MLD as the AP, the STA shall include the (Extended) Request element in the Probe Request frame body and/or a Per-STA Profile subelement in a Probe Request variant Multi-Link element carried in the Probe Request frame. In this case, the Complete Profile subfield of the STA Control field in the Per-STA Profile subelement shall be set to 0. The (Extended) Request element carried in the per-STA profile corresponding to the requested AP that requests the same partial information as the AP can be inherited from the (Extended) Request element in the frame body, subject to the rules defined in [35.3.2.3.2 (Inheritance in the per-STA profile of Probe Request variant Multi-Link](#bookmark10) [element(#2416))](#bookmark10).

(#2416)An MLProbe Request allows a non-AP STA to request an AP to include the complete information of all APs affiliated with the same AP MLD as the AP if the Probe Request frame does not include the (Extended) Request element in the frame body and the Probe Request variant Multi-Link element in the Probe Request frame does not include any per-STA profile.

(#2416)An MLProbe Request allows a non-AP STA to request an AP to include the same requested partial information for all APs affiliated with the same AP MLD as the AP if the Probe Request frame includes the (Extended) Request element in frame body and the Probe Request variant Multi-Link element in the Probe Request frame does not include any per-STA profile.

(#1155)(#1414)(#2581)(#3367)(#3359)(#2859)An MLProbe Response is an Action frame:

* + - * + that is transmitted in response to receiving an MLProbe Request
        + and that is transmitted by an AP affiliated with the AP MLD identified by the soliciting MLProbe Request frame
        + and that includes Basic variant Multi-Link element which can carry complete or partial per-STA profile(s), based on the soliciting request, for each of the requested AP(s) of the AP MLD.

NOTE: the solicited MLProbe Response doesn’t include the Multiple BSSID element if the AP in the reporting link affiliated with the polled MLD doesn’t have transmitted BSSID

(#2416)(#2583)(#3360)(#1422)If an AP that is affiliated with an AP MLD receives an MLProbe Request from a non-AP STA requesting complete information, it shall respond with an MLProbe Response, which is a Probe Response frame that includes a Basic variant Multi-Link element with (#2419)a per-STA profile with complete information for each of the APs that are affiliated to the same AP MLD as the AP and that are requested by the MLProbe Request, subject to the rules defined in 11.1.4.3.4 (Criteria for sending a response)(#1048). If it receives an MLProbe Request from a non-AP STA requesting partial information, it shall respond with an ML probe response that includes a Basic variant Multi-Link element with (#2419)a per-STA profile with at least the elements requested from the (Extended) Request element for each of the APs that are affiliated to the same AP MLD as the AP and that are requested by the MLProbe Request, unless the elements requested are not part of the complete information for each of the APs and subject to the rules defined in 11.1.4.3.4 (Criteria for sending a response)(#1048).

(#2583)(#3360)(#1423)If an AP that is part of an AP MLD receives an MLProbe Request requesting complete information and responds with an MLProbe Response , the Address 1 field of the Probe Response frame may be set to the broadcast address unless the AP is not including its actual SSID in the SSID element of its Beacon frames.

35.3.4.3 Non-AP behavior(#1010)(#1020)

***TGbe editor: change 35.3.4.3 as follows(the paragraphes not shown are not changed): (#5063)***

A non-AP MLD shall be able to discover an AP MLD when it receives a Basic variant Multi-Link element carried in a Beacon frame or Probe Response frame, transmitted by an AP affiliated with the AP MLD or by the AP corresponding to the transmitted BSSID in the same multiple BSSID set as at least one of the APs affiliated with the AP MLD.

A non-AP MLD shall be able to discover an AP MLD and the capabilities and operational parameters of one or more APs affiliated with an AP MLD when it receives a Basic variant Multi-Link element that carries a complete profile of the reported AP carried in the MLProbe Response frame transmitted by an AP affiliated with the AP MLD.

……

(#1676)(#1042)(#1044)None of the non-AP STAs of a non-AP MLD shall send an MLProbe Request to an AP of the AP MLD in the corresponding link if any non-AP STA of the same non-AP MLD has already received a ML\_Probe Response including complete information from any of the AP of the AP MLD in any link, since the MLME-SCAN.request primitive with ScanType parameter indicating an active scan was issued.

35.3.4.3 Non-AP behavior(#1010)(#1020)

***TGbe editor: change the first three paragraphes in 35.3.4.3 as follows: (#5063)***

A non-AP MLD shall be able to discover an AP MLD when it receives a Basic variant Multi-Link element carried in a Beacon frame or Probe Response frame, transmitted by an AP affiliated with the AP MLDor by the AP corresponding to the transmitted BSSID in the same multiple BSSID set as at least one of the APs affiliated with the AP MLD.

A non-AP MLD shall be able to discover an AP MLD and the capabilities and operational parameters of one or more APs affiliated with an AP MLD when it receives a Basic variant Multi-Link element that carries a complete profile of the reported AP carried in the ML\_Probe Response frame transmitted by an AP affiliated with the AP MLD.

35.3.4.4 **Multi-Link element usage rules in the context of discovery**

***TGbe editor: change the first paragraph in 35.3.4.4 as follows: (#5063)***

(#3016)(#1005)(#1896)(#1155)(#1414)(#2581)(#3367)(#3359)(#2859)(#2241)(#2295)An AP affiliated

with an AP MLD shall include, in a Beacon frame or a Probe Response frame only the Common Info field of the Basic variant Multi-Link element as defined in 9.4.2.295b (Multi-Link element) unless conditions in [35.3.10 (Multi-link general procedures(#2324)(#2600))](#bookmark28) are satisfied.

***TGbe editor: change the 3rd, 4th paragraphes in 35.3.4.4 as follows: (#5063)***

(#2583)(#3360)A Probe Request frame shall not include a Multi-Link element of any type.

(#1192)(#2581)(#3367)A MLProbe Request shall include a Probe Request variant Multi-Link element and shall not include other variant Multi-Link element.