IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D2.0 Comment Resolution for Section 32.3.7 (Mathematical description of signals) | | | | |
| Date: 2021-09-15 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Rui Cao | NXP | 350 Holger Way, San Jose,CA |  | [rui.cao\_2@nxp.com](mailto:rui.cao_2@nxp.com) |

Abstract

This submission proposes resolutions for comments received on Section 32.3.7 (Mathematical description of signals) in TGbd D2.0. The following is the list of 3 CIDs:

* 2183, 2006, 2184

Revisons:

* r0: initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 2183 | 32.3.7.3 | 84.09 | The definition of Qk for NGV modulated fields is incomplete, as no values for the matrix are specified here. Hence, add the following subclause to the sentence "NSS columns as further described in 32.3.9.8.1 (Transmission in NGV format)." | as in comment | Accepted |
| 2006 | 32.3.7.3 | 84.36 | "N\_STS,total = 1" should be changed to "N\_STS,total=2" | As in the comment. | Accepted. |
| 2184 | 32.3.7.3 | 84.35 | "the row for NSTS,total = 1 corresponds to NSS = 1 and the row for NSTS,total = 1 corresponds to NSS = 2". Please replace in the second occurrence of "NSTS,total = 1" by "NSTS,total = 2". | as in comment | Accepted  11bd Editor: This is the same comment as CID 2006. The resolution to CID 2006 applies here. No further changes are needed. |