**IEEE P802.11**

**Wireless LANs**

|  |  |
| --- | --- |
| Project | IEEE P802.11 Working Group for Wireless LANs |
| Title | **IEEE 802.11TGbb Coexistence Assessment Document** |
| Date Submitted | [15/11/2021] |
| Source | [Tuncer Baykas] [Hyperion Technologies][Istanbul, Turkey][Volker Jungnickel][Fraunhofer HHI][Berlin, Germany][Nikola Serafimovski][Purelifi][United Kingdom] | Email: [tbaykas@ieee.org]E-mail:[volker.jungnickel@hhi.fraunhofer.de]E-mail:[ <nikola.serafimovski@purelifi.com>] |
| Re: | [IEEE 802.11 TGbb Coexistence Assurance Document]] |
| Abstract | [IEEE 802.11 TGbb Coexistence Assurance Document] |
| Purpose | [Fulfillment of Commitment to the TGbb CSD] |
| Notice | This document has been prepared to assist the IEEE P802.11. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.11. |

# Introduction

This document is supplemental to IEEE Std 802.11bb and describes the coexistence properties of IEEE Std. 802.11bb, a standard operating in the optical spectrum. While the standard describes the MAC and PHY layers, the focus of this document is on coexistence.

# Background

**Excerpts from 802.11bb PAR**

**Title:** Standard for Information Technology--Telecommunications and Information Exchange Between Systems Local and Metropolitan Area Networks--Specific Requirements - Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications Amendment: Light Communications

**5.2 Scope:** : This amendment specifies a new PHY layer and modifications to the IEEE 802.11 MAC that enable operation of wireless light communications (LC). This amendment specifies a PHY that provides:

1. Uplink and downlink operations in 800 nm to 1,000 nm band,
2. All modes of operation achieve minimum single-link throughput of 10 Mb/s as measured at the MAC data service access point (SAP),
3. Interoperability among solid state light sources with different modulation bandwidths.

This amendment specifies changes to the IEEE 802.11 MAC that are limited to the following:

1. Hybrid coordination function (HCF) channel access,
2. Overlapping basic service set (OBSS) detection and coexistence,
3. Existing power management modes of operation (excluding new modes), and modifications to other clauses necessary to support these changes.

**5.4 Purpose:** The purpose of this standard is to provide wireless connectivity for fixed, portable, and moving stations within a local area. This standard also offers regulatory bodies a means of standardizing access to one or more frequency bands for the purpose of local area communication.

# Coexistence of 802.11bb with other standards.

Light does not interfere with other parts of the electromagnetic spectrum and communication below 3 THz but operates in an orthogonal part of the electromagnetic spectrum.

The propagation of light is confined within the illuminated area, typically spanning a few meters diameter of illuminated area. In addition, the directivity of light helps minimizing interference with neighboring networks.

Prior to starting a new network, coordinators are mandated to ensure that there are no overlapping LC networks in operation.

The currents standards in the light spectrum are

* Remote controls
	+ Remote controls are narrowband and their modulation spectrum is not relevant for 802.11bb which operates at higher modulation frequencies on all its PHYs.
* IrDA in various variants up to GigaIR
	+ IrDA has found mass market adoption in 1990s was IrDA, operating in the infrared. Modern devices replaced IrDA by Bluetooth and 802.11. Given the rapid replacement of mobile devices in the market, it can be concluded that IrDA is no longer relevant in the market, i.e. there is no need to consider coexistence by 802.11bb.
* IEEE 802.15.7-2018
	+ 802.15.7-2018 defined wireless communication in the optical spectrum. It can be operated in PHY I-PHY III with photodiode receivers and in PHY IV, V and VI using optical cameras. PHY I and PHY IV-VI operate at lower modulation frequencies, which are not relevant for 802.11bb. PHY II and PHY III were never adopted by the market. Hence, there is no need to consider coexistence by 802.11bb.
* ITU-T G.9991
	+ Coexistence between the two systems can be ensured by spatial separation or by using different optical wavelengths. Implementers are encouraged the avoid direct overlap of 802.11bb and ITU-T G.9991 systems to avoid interference.
* IEEE P802.15.13
	+ Coexistence between the two systems can be ensured by spatial separation or by using different optical wavelengths. Implementers are encouraged the avoid direct overlap of 802.11bb and 802.13.15 systems to avoid interference.
* IEEE 802.15.7a
	+ Coexistence between the two systems can be ensured by spatial separation or by using different optical wavelengths.

# Conclusion

The 802.11 TG bb believes that the standard will be able to coexist with all standards in the field of optical wireless communications available in the market. Appropriate means to coexist are to use dedicated wavelength and spatial separation by implementers.