IEEE P802.11
Wireless LANs

|  |
| --- |
| CIDs Assigned to Xiaofei Part 1 |
| Date: 2022-01-17 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 111 West 33rd StreetNew York, NY 10120USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |
| Carol Ansley | Cox Communications |  |  | carol@ansley.com |

Abstract

This submission proposes the spec text for resolutions for the CID 2184. The baseline for this comment resolution document is 802.11bc Draft 2.1.

* Rev 0: first draft

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 2184 | 43.38 | 38 | 9.4.5.32 | "A broadcast service is being transmitted" makes no sense. A service is a service, not something that can be transmitted | Change to "An EBCS traffic stream is being transmitted" | Revised. Agree with the comment. Proposed changes as well as related changes have been incorporated as shown in 11-21/1937r0.Notes to 11bc editor: please incorporate changes in 11-21/1937r0 under tag #2184. |

***TGbc Editor: Please modify the text of 9.4.5.32 as follows (802.11bc D2.1).***

The Info ID and Length fields are defined in 9.4.5.1 (General). The Enhanced Broadcast Services Response

Tuples field, if present, contains one or more Enhanced Broadcast Services Response Tuple fields. The

30

Enhanced Broadcast Services Response Tuple field is defined in [Figure 9-839ac (Enhanced Broadcast](#bookmark132)

[Services Response Tuple format](#bookmark132)).

Content ID

Transmission Status

 Octets: 1 1

#####  Figure 9-839ac—Enhanced Broadcast Services Response Tuple format

 The Transmission Status field indicates whether the EBCS traffic stream referenced by the

43

Content ID field is being transmitted. A value of 1 indicates that the traffic stream is being transmitted and a

value of 0 indicates that the traffic stream is not being transmitted. All other values are reserved.

The Transmission Status field values are defined in [Table 9-340k (](#bookmark133)

[Transmission Status field values).](#bookmark133)

49

#####  Table 9-340k—Transmission Status field values

|  |  |
| --- | --- |
| **Value** | **Description** |
| 0 | The EBCS traffic stream identified by the Content ID field is not being transmitted |
| 1 |  The EBCS traffic stream identified by the Content ID field is being transmitted |
| 2-255 | Reserved |