IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolution for CIDs related to Multiple BSSID set |
| Date: January 17, 2021 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Abhishek Patil | Qualcomm Inc |  |  | appatil@qti.qualcomm.com |

 Abstract

This submission proposes resolutions for comments received in LB258 (REVme D1.0) for multiple BSSID set feature.

***TGm editor: The baseline for this document is REVme D1.0.***

**Revisions:**

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGm Draft. This introduction is not part of the adopted material.

Part 1:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
| 1004 | Abhishek Patil | 9.4.2.45 | 1356 | 36 | "Any element specific to the BSS or with content that is different from the transmitted BSSID." is a broad statement and doesn't capture the details of the inheritance mechanism. Add reference to 11.1.3.8.4 (Inheritance of element values) which provides the details of the inheritance mechanism. | Update the bullet as: "Any element specific to the BSS or with content that is different from the transmitted BSSID (see 11.1.3.8.4 (Inheritance of element values) for details on the inheritance operation)" | **Revised**Agree with the comment. The proposed text was added as stated by the comment. In addition, a statement in clause 11.1.3.8.1 was updated to clarify the intention and the abbreviations for EMA was added to clause 3.4**TGm editor, please implement changes as shown in doc 11-22/0116r0 tagged as 1004** |

* Multiple BSSID element

***TGm editor: Please update the 4th bullet in the following paragraph this subclause as shown below:***

A nontransmitted BSSID profile carried in one or more Nontransmitted BSSID Profile subelements across one or more multiple BSSID elements in the same frame contains a list of elements for the AP or the DMG STA that has a nontransmitted BSSID and is defined as follows:

* Any element specific to the BSS or with content that is different from the transmitted BSSID (see 11.1.3.8.4 (Inheritance of element values) for details on the inheritance operation)[1004].

**11.1.3.8.1 General**

***TGm editor: Please update the following paragraph this subclause as shown below:***

[1004]A nontransmitted BSSID is discoverable if the AP corresponding to the transmitted BSSID includes information of that BSSID in its Beacon and Probe Response frames (though not necessarily in every frame).

**3.4 Acronyms and abbreviations**

***TGm editor: Please add the following entry in alphabetical order to this subclause as shown below:***

[1004]EMA enhanced multiple BSSID advertisement

Part 2

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |