IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed Comment Resolution for CID 2305 (REVme D1.0) |
| Date: 2022-02-07 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Stephen McCann | Huawei Technologies Co., Ltd | Southampton, UK |  | stephen.mccann@ieee.org  |

Abstract

This document proposes a comment resolutions for CID 2305 (REVme D1.0).

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

| **comments** |
| --- |
| **CID** | **Page** | **Clause** | **Resn Status** | **Comment** | **Proposed Change** | **Resolution** | **Owning Ad-hoc** |
| 2305 | 211.37 | 3.2 |  | The listed format of the "2.16 GHz mask physical layer" is not the same as that of the "160 MHz mask physical layer" (P211L1) | Change the format of the "2.16 GHz mask physical layer" to match that of the others. Commentor will create a submission to suggest some changes. |  | ED1 |

  |

**Discussion**

Ensure that the clause 3.2 definitions use consistent language, where there are optional PHY elements in a list.

**Proposed Comment Resolution**

Revised: Make the following editorial changes within clause 3.2

**2.16 GHz mask physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is transmitted using the transmit spectral mask defined in Clause 20 (Directional multi-gigabit (DMG) PHY specification) and is one of the following:

a) A directional multi-gigabit (DMG) PPDU.

b) A 2.16 GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

c) A 2.16 GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**2.16 GHz physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is one of the following:

a) A Clause 20 (Directional multi-gigabit (DMG) PHY specification) directional multi-gigabit (DMG) PPDU. b) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 2.16-GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

c) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 2.16-GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**2.16+2.16 GHz mask physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is

transmitted using the 2.16+2.16 GHz transmit spectral mask defined in Clause 28 (Enhanced directional

multi-gigabit (EDMG) PHY specification) and that is one of the following:

a) A 2.16+2.16 GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A 2.16+2.16 GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**2.16+2.16 GHz physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is one of the following:

a) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 2.16+2.16 GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 2.16+2.16 GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**4.32 GHz mask physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is transmitted using the 4.32 GHz transmit spectral mask defined in Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) and that is one of the following:

a) A 4.32 GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A 4.32 GHz non- enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

c) A 2.16 GHz EDMG PPDU (TXVECTOR parameter FORMAT equal to EDMG).

d) A 2.16 GHz non-EDMG PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**4.32 GHz physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is one of the following:

a) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 4.32-GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 4.32-GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**4.32+4.32 GHz mask physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is transmitted using the 4.32+4.32 GHz transmit spectral mask defined in Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) and that is one of the following:

a) A 4.32+4.32 GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A 4.32+4.32 GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**4.32+4.32 GHz physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is one of the following:

a) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 4.32+4.32 GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 4.32+4.32 GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**6.48 GHz mask physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is transmitted using the 6.48 GHz transmit spectral mask defined in Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) and that is one of the following:

a) A 6.48 GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A 6.48 GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

c) A 4.32 GHz EDMG PPDU (TXVECTOR parameter FORMAT equal to EDMG).

d) A 4.32 GHz non-EDMG PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

e) A 2.16 GHz EDMG PPDU (TXVECTOR parameter FORMAT equal to EDMG).

f) A 2.16 GHz non-EDMG PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**6.48 GHz physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is one of the following:

a) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 6.48-GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 6.48-GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**8.64 GHz mask physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is transmitted using the 8.64 GHz transmit spectral mask defined in Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) and that is one of the following:

a) An 8.64 GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) An 8.64 GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

c) A 6.48 GHz EDMG PPDU (TXVECTOR parameter FORMAT equal to EDMG).

d) A 6.48 GHz non-EDMG PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

e) A 4.32 GHz EDMG PPDU (TXVECTOR parameter FORMAT equal to EDMG).

f) A 4.32 GHz non-EDMG PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

g) A 2.16 GHz EDMG PPDU (TXVECTOR parameter FORMAT equal to EDMG).

h) A 2.16 GHz non-EDMG PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).

**8.64 GHz physical layer (PHY) protocol data unit (PPDU)**: A PPDU that is one of the following:

a) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 8.64-GHz enhanced directional multi-gigabit (EDMG) PPDU (TXVECTOR parameter FORMAT equal to EDMG).

b) A Clause 28 (Enhanced directional multi-gigabit (EDMG) PHY specification) 8.64-GHz non-enhanced directional multi-gigabit (non-EDMG) PPDU (TXVECTOR parameter FORMAT equal to NON\_EDMG).