IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D1.0 CRs on 36.3.13.13 DCM | | | | |
| Date: 2022-02-06 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Bo Gong | Huawei |  |  | [gongbo8@huawei.com](mailto:gongbo8@huawei.com) |
| Jian Yu | Huawei |  |  | ross.yujian@huawei.com |

This submission shows

* Resolution for 2 comments received from TGbe comment collection (based on TGbe Draft D1.0)
* The proposed changes are based on 11be D1.4.

The submission provides resolutions to the following CIDs

5431, 7013

# Revision Notes

|  |  |
| --- | --- |
| R0 | Initial revision |
|  |  |
|  |  |
|  |  |

## CID 5431

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page. Line | Clause Number | Comment | Proposed Change | Resolution |
| 502.30 | 36.3.13.13 | May not need to create and mention the term "EHT-SIG MCS 3" (when the EHT-SIG MCS field is set to 3, which is essentially EHT-MCS 15). It is just like we don't call 20 MHz bandwidth as BW 0 (when the BW field is set to 0). | Remove "and EHT-SIG MCS 3". | Accepted |

## CID 7013

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page. Line | Clause Number | Comment | Proposed Change | Resolution |
| 502.29 | 36.3.13.13 | There is a contradiction between 'DCM is a modulation scheme..applied for ...EHT-SIG MCS 3' and 'DCM is applicable only to BPSK...'. Also in 36.3.13.7 it is stated that DCM is applicable to MCS 14 an 15 (no mention of MCS 3). | If DCM is applicable to MCS 3 as well (for EHT-SIG), add text clarifying that DCM is applicable in EHT-SIG also for 16QAM on top of BPSK+DCM. | Revised  The expression ‘and EHT-SIG MCS 3’ should be removed since EHT-SIG MCS 3 is essentially EHT-MCS 15.  **Note to the TGbe Editor that the resolutions for CIDs 5431, and 7013 are the same.** |