IEEE P802.11  
Wireless LANs

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | CC36 CR on CID 6118 And 6915 | | | | | | Date: 2022-03-03 | | | | | | Author(s): | | | | | | Name | Affiliation | Address | Phone | email | | Alice Chen | Qualcomm |  |  | alicel@qti.qualcomm.com | | Sameer Vermani | Qualcomm |  |  | svverman@qti.qualcomm.com | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |

Abstract

This submission proposes resolutions for the following comments from the CC36 on P802.11be D1.0: CID 6118 and 6915 regarding definition of the MIB variable dot11EHTBaseLineFeaturesImplementedOnly.

NOTE – Set the Track Changes Viewing Option in the MS Word to “All Markup” to clearly see the proposed text edits.

**Revision History:**

R0: Initial version. Resolve CIDs 6118, 6915.

# CID 6188, 6915

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 6915 | C.3 | 592.33 | In the description of dot11EHTBaseLineFeaturesImplementedOnly, it seems indicate, when false, that the features that have not been implemented are all optional. It is not a good idea to indicate features that have not been implemented are optional or not. Annex B (PICS) should do the job. | Remove "optional". (2 places) | Accepted.  Note to editor: This is in P740L42 in 802.11be spec draft D1.4. |
| 6188 | C.3 | 592.41 | What optional EHT features cannot be indicated in the EHT Capabilities element? Why not? | Clarify. | Revised.  Currently all R1 featuers could be indicated in the EHT capabilities element. We used the proposed change to CID 6915 (deleting “optional”) for clarity.  Note to editor: This CID has the same resolution to CID 6915. No additional change is needed. |