**IEEE P802.11  
Wireless LANs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB266 CR for 35.3.16.5.1 (PPDU end time alignment) Part 1 | | | | |
| Date: 2022-07-10 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Yongho Seok | Mediatek |  |  | yongho.seok@mediatek.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for multiple comments related to TGbe D2.0 with the following CIDs (7 CIDs):

* 11136, 11444, 11446, 12660, 12661, 13807, 13808

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the subsequent TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| --- | --- | --- | --- | --- | --- |
| 11136 | 35.3.16.5.1 | 455.38 | "any of PPDUs containing a Trigger frame" reads oddly | Try "any of the PPDUs containing a Trigger frame" | Accepted |
| 11444 | 35.3.16.5.1 | 455.16 | Replace 'STAs of a non-AP MLD' with 'STAs affiliated with a non-AP MLD'. Same comment for L19. | As in comment | Accepted |
| 11446 | 35.3.16.5.1 | 456.10 | Replace 'AP in the AP MLD' with 'AP affiliated with the AP MLD'. Also revise 'STA in the non-AP MLD' to 'STA affiliated with the non-AP MLD'.Same comment for L14. | As in comment | Accepted |
| 12660 | 35.3.16.5.1 | 455.19 | The AP MLD does not transmit any frame, but only one of its affiliated APs. Please revise the following sentence, as proposed: "When an AP MLD simultaneously transmits to the STAs ..." | Please revise the sentence as follows: "When more than one AP affiliated with an AP MLD simultaneously transmit to the STAs ..." | Accepted |
| 12661 | 35.3.16.5.1 | 455.19 | Need to use a unified terminology along the TGbe spec, and replace "of" with "affiliated with" in the following sentence: "When an AP MLD simultaneously transmits to the STAs of a non-AP MLD operating on a pair of ..." | Please revise the sentence as follows: "When an AP MLD simultaneously transmits to the STAs affiliated with a non-AP MLD operating on a pair of..." | Revised-  Agree in principle.  TGbe change to:  "When more than one AP affiliated with an AP MLD simultaneously transmit to the STAs ..." |
| 13807 | 35.3.16.5.1 | 455.29 | The conditions below are only need for the PPDUs that solicit immediate response | please add "soliciting immediate response" after "PPDUs" | Accepted |
| 13808 | 35.3.16.5.1 | 455.37 | carries should be carry | Change "carries" to "carry". | Accepted |