IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB266 CR for 35.13 Intra PPDU Power Save | | | | |
| Date: July 11, 2022 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Jason Yuchen Guo | Huawei |  |  | guoyuchen@huawei.com |
| Ming Gan | Huawei |  |  |  |
| Yunbo Li | Huawei |  |  |  |
| Guogang Huang | Huawei |  |  |  |
| Mengyao Ma | Huawei |  |  |  |
| Hongjia Su | Huawei |  |  |  |
| Yousi Lin | Huawei |  |  |  |

Abstract

This submission proposes resolutions for following 1 CID received for TGbe LB266:

13042

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 13042 | Chunyu Hu | 520.36 | 35.13 | Since EHT MU PPDU covers both SU and MU PPDU in EHT, should the conditions that apply to an HE MU PPDU be extended to cover HE SU PPDU as well? | Insert "HE SU PPDU" before "HE MU PPDU" in the first bullet. | Revised-  Agree in principle with the comment. Although in 26.14.1 (Intra-PPDU power save for non-AP HE STAs), the conditions applied to HE SU PPDU and HE ER SU PPDU also apply to the HE MU PPDU, it is better to call out the HE SU PPDU and the HE ER SU PPDU explicitly to cover the SU PPDU case.  TGbe editor:  Please implement changes as shown in this document tagged as 13042. |

***TGbe editor: Please note baselines are Draft P802.11be\_D2.0 and REVme D1.0***

**35.13 Intra-PPDU power save for non-AP EHT STAs**

A non-AP EHT STA that operates in intra-PPDU power save mode shall follow the rules defined in 26.14.1 (Intra-PPDU power save for non-AP HE STAs) and with the following additions:

— The conditions that apply to an HE MU PPDU, HE SU PPDU, or HE ER SU PPDU (#13042) shall also apply to an EHT MU PPDU, and

— The conditions that apply to an HE TB PPDU shall also apply to an EHT TB PPDU.

**Straw Poll: Do you support to incorporate the proposed draft text in this document 11-22/1073r0 to the next revision of TGbe Draft?**

**Result: Yes/No/Abstain**