IEEE P802.11
Wireless LANs

|  |
| --- |
| CC40 CR for CIDs 7, 470, and 509 |
| Date: 2022.07.26 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Rui Du | Huawei Technologies | H3, Huawei Base, Shenzhen, Guangdong, China, 518129 |  | Ray.du@huawei.com |
| Narengerile |  |  |  |
| Mengshi Hu |  |  |  |

Abstract

This submission contains the proposed comment resolutions for the CIDs 7, 470, and 509.

R0: initial document

## CID 7, 470, 509.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Page.Line | Clause Number | Comment | Proposed Change | Resolution |
| 7 | 33.45 | 9.4.2.317 | Measurement report type, field needs to define the sensing measurment report types that need to be used in 11bf. | Measurement report type' needs to include different CSI reports that are agreed upon to be indicated as the measurement report type. | REVISED. The group agreed that CSI is the only measurement report type in 11bf.Table 9-401s has been referenced as the definition of Measurement Report Type subfield. TGbf Editor make changes specified in 22/1206r0. |
| 470 | 33.23 | 9.4.2.317 | CSI Feedback Support is missing | Create 1 bit CSI Feedback Support parameter subfield in Figure 9-1002av | REJECTED.Sensing Measurement Report field can indicate it.  |
| 509 | 33.29 | 9.4.2.317 | In Figure 9-1002av, the size of Measurement Report Type is TBD. Define the report type and the size of this field. | as in comment | REVISED.The size and definition of Measurement Report Type subfields have been added in Draft 0.2.TGbf Editor make changes specified in 22/1206r0. |

**Discussion 1**

Athough CSI is the only sensing measurement report type for sub-7 GHz WLAN sensing, it is good to keep the Sensing Measurement Report Type subfield for future use.

***Instructions to the editor: please make the following changes to P44L37 and P44L54 in the subclause 9.4.2.317 Sensing Measurement Parameters element in D0.2 as shown below:***



Figure 9-1002au – Sensing Measurement Parameters element format



Figure 9-1002av – Sensing Measurement Parameters field format

***Instructions to the editor: please make the following changes to P45L13 in the subclause 9.4.2.317 Sensing Measurement Parameters element in D0.1 as shown below:***

The Sensing Measurement Report Type subfield is set to a number that identifies the type of sensing measurement report being requested. The types of sensing measurement report that have been allocated are defined in Table 9-401s (Sensing Measurement Report Type field definition)(#217, #255, #587, #837, #902,

#488, #509). If the sensing initiator is a sensing receiver, the Sensing Measurement Report Type subfield is reserved(#667).

Table 9-401s - Sensing Measurement Report Type subfield definition

|  |  |
| --- | --- |
| Name  | Sensing Measurement Type |
| 0 | CSI |
| 1-255 | Reserved  |

**Reference: TGbf Draft 0.2.**