IEEE P802.11
Wireless LANs

|  |
| --- |
| LB266 CR on EHT Operation element |
| Date: 2022.07.29 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Guogang Huang | Huawei Technologies | F3-6-A124, Huawei Base, Bantian, Longgang, Shenzhen, Guangdong, China, 518129 |  | huangguogang1@huawei.com |
| Yuchen Guo |  |  |  |
| Yunbo Li |  |  |  |
| Yousi Lin |  |  |  |
| Ming Gan |  |  |  |

Abstract

This submission contains proposed comment resolutions to comments on P802.11be D2.0. The following 29 CIDs are resolved:

10807 10808 10990 10991 11026 11037 11043 11044 11045 11046 11512 11513 11514 11857 11858 11859 11860 11861 11862 12056 12131 12824 12969 12970 13363 13364 13382 13467 13468

Revisions:

- Rev 0: Initial version of the document.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page.****Line** | **Comment** | **Proposed Change** | **Resolution** |
| 10807 | Dong Guk Lim | 9.4.2.311 | 209.38 | To clarify it, change the reference. | Change "Figure 9-1002a (EHT Operation element for mat)" with " Figure 9-1002ai and Figure 9-1002aj" | RevisedAgree in principle. The correct reference is provided.TGbe editor to make the changes with the CID tag (#10807) in 11/22-1267r0 |
| 10990 | Yanjun Sun | 9.4.2.311 | 209.38 | The reference (to Figure 9-1002a) is incorrect and please update it to the correct one. | As in comment | RevisedAgree in principle. The correct reference is provided.TGbe editor to make the changes with the CID tag (#10807) in 11/22-1267r0 |
| 11512 | Xiaofei Wang | 9.4.2.311 | 209.38 | The basic EHT-MCS and NSS set field is not defined in figure 9-1002a. Please provide a correct reference. | as in comment | RevisedAgree in principle. The correct reference is provided.TGbe editor to make the changes with the CID tag (#10807) in 11/22-1267r0 |
| 11857 | Alfred Asterjadhi | 9.4.2.311 | 209.36 | Wrong reference. Replace with the correct subclause for where basic EHT MCS and NSS Set are defined. | As in comment. | RevisedAgree in principle. The correct reference is provided.TGbe editor to make the changes with the CID tag (#10807) in 11/22-1267r0 |
| 12824 | Laurent Cariou | 9.4.2.311 | 209.38 | The Basic EHT-MCS And NSS Set field is defined in Figure 9-1002a (EHT Operation element format). The reference is not correct: should be 9-1002ai. | as in comment | RevisedAgree in principle. The correct reference is provided.TGbe editor to make the changes with the CID tag (#10807) in 11/22-1267r0 |
| 10808 | Dong Guk Lim | 9.4.2.311 | 209.43 | EHT Operation Information Present field is used to indicate whether the EHT Operation Information exists or not in the EHT Operation element. and, to confirm the difference in channel bandwidth information as described in text from L43 to L46, there needs to include an EHT Operation Information. it means that the EHT Operation Information is included in the EHT Operation element and the EHT Operation Information Present field is set to 1. so, it is a little strange that EHT Operation Information Present field should be set to 1 after checking of difference of CH BW. To clarify it, delete this text or modify it. | As in the comment. | RevisedAgree in principle. This paragraph is revised.TGbe editor to make the changes with the CID tag (#10808) in 11/22-1267r0 |
| 10991 | Yanjun Sun | 9.4.2.311 | 209.50 | "HT Operation Information Present" needs to be changed to "EHT Operation Information Present " | As in comment | RevisedTGbe editor to make the changes with the CID tag (#10991) in 11/22-1267r0 |
| 11043 | Po-Kai Huang | 9.4.2.311 | 209.50 | For the sentence, "The Disabled Subchannel Bitmap Present subfield is valid only when the HT Operation Information Present subfield is set to 1.", it shuold be "EHT Operation Information Present subfield is set to 1". I consider that this is an obvious typo. | change "The Disabled Subchannel Bitmap Present subfield is valid only when the HTOperation Information Present subfield is set to 1." to "The Disabled Subchannel Bitmap Present subfield is valid only when the EHTOperation Information Present subfield is set to 1." | RevisedTGbe editor to make the changes with the CID tag (#10991) in 11/22-1267r0 |
| 11514 | Xiaofei Wang | 9.4.2.311 | 209.50 | where is "HT Operation Information present subfield" defined and included? | as in comment | RevisedTGbe editor to make the changes with the CID tag (#10991) in 11/22-1267r0 |
| 13363 | Liwen Chu | 9.4.2.311 | 209.49 | change "only when the HT Operation Information Present subfield is set to 1" to "only when the EHT Operation Information Present subfield is set to 1" | As in comment | RevisedTGbe editor to make the changes with the CID tag (#10991) in 11/22-1267r0 |
| 11026 | Hanqing Lou | 9.4.2.311 | 209.43 | "The EHT Operation Information Present subfield is set to 1 if the channel width indicated in an HT Operation, VHT Operation, or HE Operation element that is present in the same Management frame is different from the Channel Width field indicated in the EHT Operation Information field". The Disabled Subchannel Bitmap subfield is in the EHT Operation Information field. If the channel width is the same as VHT Operation Element, but Disabled subchannel Bitmap is updated, will the EHT Operation Information Present subfield be set to 1? | When Disabled Subchannel Bitmap Present subfield is 1, the EHT Operation Information Present subfield shall be 1. | RejectedSince P802.11ac doesn’t support static channel puncturing, the mentioned case will not happened, i.e. the channel width is the same as the VHT Operation Element, but the Disabled subchannel Bitmap is updated. In addition, the following text has been added to clarify the relationship between the EHT Operation Information Present subfield and the Disabled Subchannel Bitmap Present subfield. TGbe editor: No changes are needed. |
| 11037 | Po-Kai Huang | 9.4.2.311 | 212.04 | Table 9-401b is not needed. EHT BSS channel width is determined solely by the indication in the Channel Width field and CCFS0 and CCFS1 setting is also based on the Channel Width subfield. The Table creates confusion because it may suggest EHT BSS channel width depends jointly by Channel Width subfield, CCFS0 subfield and CCFS1 subfield. Suggest to delete Table 9-401b because Table 9-401a is enough. | Delete Table 9-401b. | AcceptTGbe editor to make the changes with the CID tag (#11037) in 11/22-1267r0 |
| 11044 | Po-Kai Huang | 9.4.2.311 | 209.43 | For the sentence, "The EHT Operation Information Present subfield is set to 1 if the channel width indicated in an HT Operation, VHT Operation, or HE Operation element that is present in the same Management frame is different from the Channel Width field indicated in the EHT Operation Information field." It is probably better to clarify that the channel width indication is indicated jointly by HT Operation, VHT Operation, or HE Operation if they are present. Hence, the sentence is not interpreted literally by just looking one of the indication. | Change the sentence to "The EHT Operation Information Present subfield is set to 1 if the channel width indicated jointly by an HT Operation element (if present), VHT Operation element (if present), or HE Operation element (if indicaiton for channel width present) in the same Management frame is different from the Channel Width field indicated in the EHT Operation Information field." | RevisedAgree in principle. This sentence is revised.TGbe editor to make the changes with the CID tag (#11044) in 11/22-1267r0 |
| 12969 | Chunyu Hu | 9.4.2.311 | 209.43 | Improve readability: "set to 1 if the channel width indicated in ..." and also fixed the inconsistency in "channel width" and "Channel Width" ==> "set to 1 if the channel Width indicated in the EHT Operation Information field is different from that indicated in an HT Operation, VHT Operation ..." | As in comment | RevisedAgree in principle. This sentence is revised.TGbe editor to make the changes with the CID tag (#12969) in 11/22-1267r0 |
| 13468 | Liwen Chu | 9.4.2.311 | 209.43 | Change the text to "The EHT Operation Information Present subfield is set to 1 if the allowed maximal channel width of VHT/HE PPDU indicated in VHT Operation, or HE Operation element is different from the allowed maximal channel width of EHT PPDU in the BSS." | As in comment | RevisedAgree in principle. This sentence is revised.TGbe editor to make the changes with the CID tag (#13468) in 11/22-1267r0 |
| 11045 | Po-Kai Huang | 9.4.2.311 | 209.43 | For the sentence, "The EHT Operation Information Present subfield is set to 1 if the channel width indicated in an HT Operation, VHT Operation, or HE Operation element that is present in the same Management frame is different from the Channel Width field indicated in the EHT Operation Information field." Add "Otherwise, the EHT Operation Information Present subfield is set to 0." after the sentence, so the spec is clear on the intention. | Add "Otherwise, the EHT Operation Information Present subfield is set to 0." after "The EHT Operation Information Present subfield is set to 1 if the channel width indicated in an HT Operation, VHT Operation, or HE Operation element that is present in the same Management frame is different from the Channel Width field indicated in the EHT Operation Information field." | RevisedAgree in principle. Add “otherwise, it is set to 0”TGbe editor to make the changes with the CID tag (#11045) in 11/22-1267r0 |
| 11046 | Po-Kai Huang | 9.4.2.311 | 210.14 | The following sentence is not entirely accurate "The EHT STA obtains the channel configuration information from the EHTOperation Information field, if present, in the EHT Operation element. " Specifically, the primary channel needs to be obtained from HT operation element or 6 GHz Operation Information field in HE Operation element since EHT Operation Information field does not include primary channel indication. | Revise "The EHT STA obtains the channel configuration information from the EHTOperation Information field, if present, in the EHT Operation element. " as "The EHT STA obtains the channel width information and channel center frequency information of EHT BSS bandwidth from the EHTOperation Information field, if present, in the EHT Operation element." | RevisedAgree in principle. This sentence is revised.TGbe editor to make the changes with the CID tag (#11046) in 11/22-1267r0 |
| 11513 | Xiaofei Wang | 9.4.2.311 | 209.36 | the definition for Basic EHT-MCS and Nss set field should be moved to after EHT operation parameters field. | as in comment | RejectedThis format style aligns with the HE Operation element, i.e. the optional fields are arranged after the mandatory fields.TGbe editor: No changes are needed |
| 11858 | Alfred Asterjadhi | 9.4.2.311 | 209.44 | Add a reference as to where the rules for the BW differences between amendments are specified. | As in comment. | RejectedThere is no exact reference. The corresponding rules are descripted in many subclauses.TGbe editor: No changes are needed |
| 11859 | Alfred Asterjadhi | 9.4.2.311 | 209.50 | I think the rule here needs to refer to the dependency of setting this bit to one when the EHT Op Info present is one, rather than validity of the field. So I suggest to simply say this bit is set to 1 only if Eht Op Info Present is 1 or smth like that. | As in comment. | RevisedAgree in principle. The sentence is revisedTGbe editor to make the changes with the CID tag (#11859) in 11/22-1267r0 |
| 11860 | Alfred Asterjadhi | 9.4.2.311 | 210.03 | The wording on this condition is confusing. Please rephrase to make it clearer. | As in comment. | RevisedThe second bullet is revised.TGbe editor to make the changes with the CID tag (#11860) in 11/22-1267r0 |
| 11861 | Alfred Asterjadhi | 9.4.2.311 | 210.09 | Is there a dependence on the value of this field and the previously defined one? Please clarify. | As in comment. | RejectedThere is no dependency between the setting of the Group Addressed BU Indication Limit and the Group Addressed BU Indication Exponent subfields.TGbe editor: no changes are needed. |
| 11862 | Alfred Asterjadhi | 9.4.2.311 | 212.27 | What is the setting of the bits of the Disabled Subchannel Bitmap that fall outside of the BSS bandwidth? Please clarify | As in comment. | RevisedAgree in principle. The paragraph is revised.TGbe editor to make the changes with the CID tag (#11862) in 11/22-1267r0 |
| 13364 | Liwen Chu | 9.4.2.311 | 212.25 | the bits of Disabled Subchannel Bitmap that are not covered by BSS BW are undefined. | Clarify that those bits are reserved. | RevisedAgree in principle. The paragraph is revised.TGbe editor to make the changes with the CID tag (#11862) in 11/22-1267r0 |
| 12056 | Massinissa Lalam | 9.4.2.311 | 210.20 | I don't see the need to have "CCFS1" subfield. EHT is not supporting non-contiguous operation (like 80+80, or a new 160+160) for a single BSS. For such deployment, MLO should be preferred. As such CCFS1 subfield and any reference to it should be deleted and CCSF0 description in Table 9-401a should be updated to:"For 20, 40, 80, 160 or 320 MHz BSS bandwidth, indicates the channel center frequency index for the 20, 40, 80, 160 or 320 MHz channel on which the EHT BSS operates.".There is zero reason why we should add an extra octet carrying useless information. | As in comment | RejectedThe group discussed this part and could not reach a consensus that would resolve the comment. In addition, the format style aligns with VHT/HE Operation elements.TGbe editor: no changes are needed. |
| 12131 | Lei Huang | 9.4.2.311 | 210.22 | When BW = 80 MHz or 160 MHz, 8-bit Disabled Subchannel Bitmap field is enough. | change size of the Disabled Subchannel Bitmap field to 0, 1 or 2 octets. | RevisedAgree in principle. The corresponding text is revised. TGbe editor to make the changes with the CID tag (#12131) in 11/22-1267r0 |
| 12970 | Chunyu Hu | 9.4.2.311 | 209.59 | Improve wording: "to indicate" ==> "that indicates" | As in comment | AcceptedTGbe editor to make the changes with the CID tag (#12790) in 11/22-1267r0 |
| 13382 | Liwen Chu | 9.4.2.311 | 209.43 | Per the text, the EHT Operation Information Present will be set to 1 in 5GHz band when the BSS operating channel is more than 40 MHz. This should not be what people want. | update the text to fix the issue. | RejectedPer the cited sentence, when the channel width is different from the one indicated in HE/VHT/HE Operation elements, then the EHT Operation Information Present subfield will be set to 1.TGbe editor: no changes are needed. |
| 13467 | Liwen Chu | 9.4.2.311 | 209.44 | the inclusion of HT Operation in the sentence means that once the BSS operating channel is >=80MHz, the EHT Operation Information Present will be 1. | update the text to fix the issue. | RejectedPer the cited sentence, when the channel width is different from the one indicated in HE/VHT/HE Operation elements, then the EHT Operation Information Present subfield will be set to 1.TGbe editor: no changes are needed. |

***TGbe editor: Change the following subclause as follows:***

**9.4.2.311 EHT Operation element**

The operation of EHT STAs in an EHT BSS is controlled by the following:

* The HT Operation element, HE Operation element, and EHT Operation element if operating in the 2.4 GHz band
* The HT Operation element, VHT Operation element (if present), HE Operation element, and EHT Operation element if operating in the 5 GHz band
* The HE Operation element and EHT Operation element if operating in the 6 GHz band

The format of the EHT Operation element is shown in Figure 9-1002a (EHT Operation element format).

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | Element ID | Length | Element ID Extension | EHT Operation Parameters  | Basic EHT-MCS And Nss Set | EHT Operation Information |
| Octets: | 1 | 1 | 1 | 1 | 4 | 0, 3, 4 or 5[#12131] |

**Figure 9-1002a – EHT Operation element** **format**

The Element ID, Length, and Element ID Extension fields are defined in 9.4.2.1 (General).

The EHT Operation Parameters field is defined in Figure 9-1002b (EHT Operation Parameters field format).

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | B0 | B1 | B2 | B3 | B4 B5 | B6 B7 |
|  | EHT Operation Information Present | Disabled Subchannel Bitmap Present | EHTDefault PE Duration | Group Addressed BU Indication Limit | Group Addressed BU Indication Exponent | Reserved |
| Bits: | 1 | 1 | 1 | 1 | 2 | 2 |

**Figure 9-1002b – EHT Operation Parameters field format**

[#12970]The Basic EHT-MCS And NSS Set field indicates the EHT-MCSs for each number of spatial streams in EHT PPDUs that are supported by all EHT STAs in the BSS (including IBSS and MBSS) for transmission and reception. [#10990]The Basic EHT-MCS And NSS Set field is defined in Figure 9-1002ai (EHT-MCS Map (20 MHz-Only Non-AP STA) subfield and Basic EHT-MCS and NSS Set field format) and Figure 9-1002aj (EHT-MCS Map (BW≤80MHz, Except 20MHz-Only Non-AP STA), EHT-MCS Map (BW=160MHz), and EHT-MCS Map (BW=320MHz) subfield format).

[#10808][#11044, #12969, #13468]The EHT Operation Information Present subfield is set to 1, if the channel width indicated in the EHT Operation Information field is different from the one indicated jointly in an HT Operation element (if present), VHT Operation element (if present), or HE Operation element (if a 6 GHz Operation Information field is present) in the same Management frame; otherwise, it is set to 0.[#11045]

The Disabled Subchannel Bitmap Present subfield is set to 1 if the Disabled Subchannel Bitmap field is present and set to 0 otherwise. [#11859]The Disabled Subchannel Bitmap Present subfield is reserved if the [#10991]EHT Operation Information Present subfield is equal to 0.

The EHT Default PE Duration subfield is set to 1 to indicate that the PE field duration for an EHT TB PPDU solicited by a TRS Control subfield is 20 μs and set to 0 to indicate that the PE field duration is the same as that indicated in the HE Operation Parameters field in the HE Operation element.

The Group Addressed BU Indication Limit subfield indicates whether there is a limit on the number of bits [#12970]that indicates the presence of buffered group addressed frames of all other APs affiliated with the same AP MLDs as all nontransmitted BSSIDs in a multiple BSSID set in the TIM element or not.

The Group Addressed BU Indication Limit subfield is set to 0 if one of the conditions is met:

* The AP is not in multiple BSSID set.
* The AP is in a multiple BSSID set and the total number of bits that is needed to indicate the presence of buffered group addressed frames of all other APs affiliated with the same AP MLDs as all nontransmitted BSSIDs in the TIM element is not greater than 48 bits.[#11860]

Otherwise, the Group Addressed BU Indication Limit subfield is set to 1.

The Group Addressed BU Indication Exponent subfield is set to the exponent from which *N* is calculated as defined in 35.3.15.1 (Group addressed frame delivery).

The EHT Operation Information field is present if the EHT Operation Information Present subfield is equal to 1; otherwise it is not present. [#11046]The EHT STA obtains the channel width information and the channel center frequency information of the EHT BSS bandwidth from the EHT Operation Information field, if present, in the EHT Operation element. The subfields of EHT Operation Information field are defined Figure 9-1002c (EHT Operation Information field format).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Control | CCFS0 | CCFS1 | Disabled Subchannel Bitmap |
| Octets: | 1 | 1 | 1 | 0, 1 or 2[#12131] |

**Figure 9-1002c – EHT Operation Information field format**

The Control subfield is defined in Figure 9-1002d (Control subfield format),

|  |  |  |
| --- | --- | --- |
|  | B0 B2 | B3 B7 |
|  | Channel Width | Reserved |
| Bits: | 3 | 5 |

**Figure 9-1002d – Control subfield format**

[#12970]The Channel Width, CCFS0 and CCFS1 subfields are defined in Table 9-401a (Channel width, CCFS0, and CCFS1 subfields).

**Table 9-401a—Channel width, CCFS0, and CCFS1 subfields**

|  |  |  |
| --- | --- | --- |
| **Subfield** | **Definition** | **Encoding** |
| Channel Width | This subfield defines the EHT BSS bandwidth. | Set to 0 for 20 MHz EHT BSS bandwidth. Set to 1 for 40 MHz EHT BSS bandwidth.Set to 2 for 80 MHz EHT BSS bandwidth.Set to 3 for 160 MHz EHT BSS bandwidth.Set to 4 for 320 MHz EHT BSS bandwidth.Values in the ranges 5 to 7 are reserved. |
| CCFS0 | This subfield defines a channel center frequency for a 20, 40, 80, 160, or 320 MHz EHT BBS. | For 20, 40 or 80 MHz BSS band width, indicates the channel center frequency index for the 20, 40 or 80 MHz channel on which the EHT BSS operates.For 160 MHz BSS bandwidth, indicates the channel center frequency index of the primary 80 MHz channel.For 320 MHz BSS bandwidth, indicates the channel center frequency index of the primary 160 MHz channel. |
| CCFS1 | This subfield defines a channel center frequency for a 160 or 320 MHz EHT BBS. | For a 20, 40 or 80 MHz BSS bandwidth, this subfield is set to 0.For a 160 MHz BSS bandwidth, indicates the channel center frequency index of the 160 MHz channel on which the EHT BSS operates.For a 320 MHz BSS bandwidth, indicates the channel center frequency index of the 320 MHz channel on which the EHT BSS operates.[#11037] |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

[#11037]

The Disabled Subchannel Bitmap subfield is present if the Disabled Subchannel Bitmap Present subfield is equal to 1 and provides a list of subchannels that are punctured within the BSS bandwidth; otherwise it is not present.

The Disabled Subchannel Bitmap subfield is [#12131]an 8-bit or 16-bit bitmap where the lowest numbered bit corresponds to the 20 MHz subchannel that lies within the BSS bandwidth and that has the lowest frequency of the set of all 20 MHz subchannels within the BSS bandwidth. Each successive bit in the bitmap corresponds to the next higher frequency 20 MHz subchannel. [#11862]A bit in the bitmap and that lies within the BSS bandwidth is set to 1 to indicate that the corresponding 20 MHz subchannel is punctured and is set to 0 to indicate that the corresponding 20 MHz subchannel is not punctured. [#11862]A bit in the bitmap that falls outside of the BSS bandwidth is reserved. [#12131]The Disabled Subchannel Bitmap subfield is a 16-bit bitmap if the channel width indicated in the Channel Width subfield is equal to 320 MHz; otherwise, it is an 8-bit bitmap.