IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for CC40 11bf D0.1 Sensing Measurement Report | | | | |
| Date: 2022-09-13 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Rojan Chitrakar | Panasonic |  |  | Rojan.chitrakar@sg.panasonic.com |
| Rajat Pushkarna |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions of comments received from TGbf comment collection 40 (TGbf Draft 0.1).

* CIDs: 294, 65, 119 (3 CIDs)

Revisions:

* Rev 0: Initial version of the document.

1. **Introduction**

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbf Draft. The introduction and the explanation of the proposed changes are not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbf Draft (i.e., they are instructions to the 802.11bf editor on how to merge the text with the baseline documents).***

***TGbf Editor: Editing instructions preceded by “TGbf Editor” are instructions to the TGbf editor to modify existing material in the TGbf draft. As a result of adopting the changes, the TGbf editor will execute the instructions rather than copy them to the TGbf Draft.***

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| CID | Commenter | Clause | Page | Line | Comment | Proposed Change | Resolution |
| 294 | Rojan Chitrakar | 9.4.2.318 | 34 | 01 | Since elements can only carry up to 255 octets, using elements to carry sensing measurement reports will limit the report size to 255 or less. It would be better to use fields instead as is done in HT/VHT/HT/EHT for the beamforming feedback. | Use field(s) to carry to carry the sensing measurement reports instead of element. | **Revised.**  Agree with the comment that it is better to use fields to carry the Sensing Measurement Report. This was discussed in 22/1248r1 and 11bf group agreed to use field(s) to carry the sensing measurement reports instead of element. The related spec text is provided in this CR document.  TGbf editor to make the changes shown in IEEE 11-22-1579r0 under all headings that include CID 294. |
| 65 | Alecsander Eitan | 9.4.2.318 | 34 | 15 | The length of field "Sensing Measurement Report Type" shall be 1 octet | Length shall be 1 octet based on Table 9-401s | **Revised.**  The length of the field is implicitly equal to 3 bits as per Table 9-401s in D0.3. During related discussion in 22/1458, the group indicated preference to keep the Type field out of the Control field.  TGbf editor to make the changes shown in IEEE 11-22-1579r0 under all headings that include CID 65. |
| 119 | Sigurd Schelstraete | 9.4.2.318 | 34 | 15 | Why is the length of the "Sensing Measurement Report Type" subfield TBD? Table 9-491s appears to show 256 possible values (1 byte). | See comment | **Revised.**  The length of the field is implicitly equal to 3 bits as per Table 9-401s in D0.3. During related discussion in 22/1458, the group indicated preference to keep the Type field out of the Control field. The resolution is the same as that for CID 65 in IEEE 11-22-1579r0.  TGbf editor to make the changes shown in IEEE 11-22-1579r0 under all headings that include CID 65. |

Baseline is TGbfD0.3

Reference for CIDs 65, 119:

Table

Description automatically generated

SP: Do you agree to incorporate the changes provided in IEEE 11-22-1579r0 for CIDs 294, 65, 119 to the next revision of 802.11bf draft?

**Discussion:** Please refer to 22/1248r1 for discussion related to this topic. The following SP was run on the 11bf call on August 23, 2022 and was unanimously supported:

***Straw Poll 1:*** *Do you agree to replace the Sensing Measurement Report element with a field?*

***Note:*** *The content of the field is based on the content of the Sensing Measurement Report element. Formatting details are TBD.*

An Example (Simplified frame format): A 40416 octets long Sensing Measurement Report is split into 4 segments and carried in four Sensing Measurement Report frames.

Assumption: the recipient STA supports maximum MPDU size of 11454 octets.



* Elements
* General

***TGbf editor: Delete Sensing Measurement Report element from Table 9-128 (Element IDs):***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| * Element IDs | | | | |
| Element | Element ID | Element ID Extension | Extensible | Fragmentable |
| Sensing Measurement Parameters (see 9.4.2.317 (Sensing Measurement Parameters element)) | 255 | <ANA> | Yes | TBD |
|  |  |  |  |  |
| … |  |  |  |  |

***TGbf editor: Delete 9.4.2.318 (Sensing Measurement Report element) and move its content to 9.6.7.51.2 (Sensing Measurement Report):***

**(CIDs 294)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  | | | | | | |

|  |  |
| --- | --- |
|  | |
|  |  |
|  |  |
|  |  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |
|  |  |  |
|  |  |
|  |  |  |
|  |  |
|  |  |  |
|  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |

**9.6 Action frame format details** **(CIDs 294)**

**9.6.7.1 Public Action frames**

**9.6.7.51 Sensing Measurement Report frame format**

***TGbf editor: Modify the subclause as follows (Track Change ON):***

**9.6.7.51.1 General**

The Sensing Measurement Report frame is an Action or an Action No Ack of category Public transmitted to provide WLAN sensing measurements. The format of the Sensing Measurement Report frame Action field is defined in Figure 9-1139d (Sensing Measurement Report frame Action field format).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Category | Public Action | Dialog Token | Sensing Measurement Report Container(s) |
| Octets: | 1 | 1 | 1 | variable |
| * **Sensing Measurement Report frame Action field format** | | | | |

The Category field is defined in 9.4.1.11 (Action field).

The Public Action field is defined in 9.6.7.1 (Public Action frames).

The Dialog Token field is defined in 9.4.1.12 (Dialog Token field). It is set to a nonzero value chosen by the STA sending the sensing measurement request to identify the request/report transaction.

The Sensing Measurement Report Container is described in 9.6.7.51.2 (Sensing Measurement Report Container).

**9.6.7.51.2 Sensing Measurement Report Container (CIDs 294, 65)**

**9.6.7.51.2.1 General**

Container Container xxxxContainer field Container



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Length | Sensing Measurement Report Type | Sensing Measurement Report Control | Sensing Measurement Report |
| Bits: | 16 | 3 (#65) | 37 | variable |
| **Figure 9-xxxx - Sensing Measurement Report Container format** | | | | |

The Length field indicates the number of octets in the Sensing Measurement Report Container field, including the two octets for the Length subfield.

|  |  |
| --- | --- |
|  | |
|  |  |
|  |  |
| 7 |  |

9.6.7.51.2.3 (Sensing Measurement Report Control field if the Sensing Measurement Report Type field is 0)9.6.7.51.2.4 (Sensing Measurement Report field if the Sensing Measurement Report Type field is 0)9.6.7.51.2.2 (CSI encoding and decoding for Sensing Measurement Report field)

**9.6.7.51.2.2**

**9.6.7.51.2.2a**

9.6.7.51.2.2b9.6.7.51.2.2c

**9.6.7.51.2.2b**

**9.6.7.51.2.2c**

**9.6.7.51.2.3**

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
| Measurement Instance ID | 8 | Indicates the sensing measurement instance corresponding to the Sensing Measurement Report | Set to the measurement instance ID corresponding to the Sensing Measurement Report |
| Remaining Report segments | 4 | Indicates the number of remaining segments for the associated Sensing Measurement Report | Set to 0 for the last segment of a segmented report or the only  segment of an unsegmented report.  Set to a value between 1 and 15 for a segment that is not the last  segment of a segmented report. |
| First Report Segment | 1 | Indicates whether this is the first segment | Set to 1 for the first segment of a segmented report or the only  segment of an unsegmented report.  Set to 0 if not the first segment. |
| Reserved | 8 |  | Reserved |

**9.6.7.51.2.4**

The size of the Sensing Measurement Report field depends on the values in the Sensing Measurement Report Control field. The Sensing Measurement Report field contains a Sensing Measurement Report information or successive portions thereof in the case of segmented sensing measurement report (see 11.21.18.6.X (Rules for generating segmented sensing measurement report)).

information

information

information

information

**information**

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |
|  |  |  |
|  |  |
|  |  |  |
|  |  |
|  |  |  |
|  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |

***TGbf editor: Insert the following subclause at the end of 11.21.18.6 (TB sensing measurement instance):***

**11.21.18.6.X Rules for generating segmented sensing measurement report (CIDs 294)**

If the inclusion of a Sensing Measurement Report information would result in a Sensing Measurement Report frame or a Protected Sensing Measurement Report frame that exceeds the maximum MPDU size supported by the recipient (see Table 9-34 (Maximum data unit sizes (in octets) and durations (in microseconds)), then the Sensing Measurement Report information shall be split into up to sixteen report segments. Each report segment shall be included in a separate Sensing Measurement Report frame or Protected Sensing Measurement Report frame and shall contain successive portions of the Sensing Measurement Report information. Each report segment shall be of equal length except the first report segment and the last report segment that may be smaller. Each Sensing Measurement Report frame or Protected Sensing Measurement Report frame that includes a report segment that is not the last report segment shall have a length equal to the maximum MPDU size supported by the recipient. Each report segment is identified by the value of the Remaining Report Segments subfield and the First Report Segment subfield in the Sensing Measurement Report Control field as defined in 9.6.7.51.2.3 (Sensing Measurement Report Control field if the Sensing Measurement Report Type field is 0). The other nonreserved subfields of the Sensing Measurement Report Control field and the Sensing Measurement Report Type subfield shall be the same for all report segments. All report segments shall be sent in a single A-MPDU contained in a PPDU and shall be included in the A-MPDU in the descending order of the values of the Remaining Report Segments subfield.