IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Revisions to RSN Extension Element | | | | |
| Date: 2022-09-13 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Kurt Lumbatis | CommScope |  |  | Kurt.Lumbatis@commscope.com |
|  |  |  |  |  |

Abstract

This document seeks to make changes to 8.4.2.241 Table 9-363

Revisions:

• Rev 0 – Initial version of the document

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbh D0.2 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbh D0.2 Draft. (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbh Editor: Editing instructions preceded by “TGbh Editor” are instructions to the TGbh editor to modify existing material in the TGbh draft. As a result of adopting the changes, the TGbh editor will execute the instructions rather than copy them to the TGbh Draft.***

# Proposed text (Proposed text modifications are based on Draft 11bh 0.2)

TGbh editor: Make the following changes in Table 9-363 per the following:

|  |  |  |
| --- | --- | --- |
| **Bit** | **Information** | **Notes** |
| <ANA> | Device ID Active | The STA sets the Device ID Active field to 1 to indicate Device ID is active. Otherwise, the STA sets the Device ID Active field to 0. |

**References:**