IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution of CID1 in LB267 against D3.0 | | | | |
| Date: 2022-09-14 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Volker Jungnickel | Fraunhofer HHI |  |  | [volker.jungnickel@hhi.fraunhofer.de](mailto:volker.jungnickel@hhi.fraunhofer.de) |
| Nikola Serafimovski | pureLiFi Ltd. |  |  | [nikola.serafimovski@purelifi.com](mailto:nikola.serafimovski@purelifi.com) |
|  |  |  |  |  |

Abstract

This contribution proposes revised working text and a graph for CID 1 in the LB 267 against D3.0.

Rev.0: initial text for discussion

C:\Volker\Projekte\MAI laufend\OWC Standard\03 802.11bb\Drafts\D4.0\Fig.32-5_CCA_example_D40.emf

The LC AP receives PPDU1 from non-AP LC STA 1 and repeats the signal to non-AP LC STAs in its coverage area. The non-AP LC STA 2 then detects a channel busy condition on receiving the repeated signal. After retransmitting PPDU1, the LC AP sends PPDU2 to non-AP LC STA 1 in response to PPDU1. Non-AP LC STA 2 sends PPDU3 to the LC AP after it detects an idle channel condition. The LC AP repeats the signal and, as a result, non-AP LC STA1 finds the channel busy.