IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment Resolution for Clause 11.20.6.5 | | | | |
| Date: 2002-09-30 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Osama Aboul-Magd | Huawei Technologies | 303 Terry Fox Drive  Ottawa, ONT, K2K 3J2 | 613-287-1405 | Osama.aboulmagd@huawei.com |
|  |  |  |  |  |

Abstract

This document includes proposed resolutions for CIDs 10589, 10845, 10846, and 14117

R0: Initial draft

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 10589 | 11.20.6.5.2 | 329.63 | Need rules for 160 MHz transmission in a 320 MHz direct link | As in comment | Revised  Agree with the commenter. Rules for 160 MHz transmission in a 320 MHz direct link seem to be missing.  TGbe Editor: Please make changes under CID 10589 in <this document> |
| 10845 | 11.20.6.5.1 | 329.25 | There is no 80MHz, 160MHz, or 80+80MHz in HT. Should be HE. | As in comment | Revised  Agree with the commenter.  TGbe Editor: Please make changes under CID 10845 in <this document> |
| 10846 | 11.20.6.5.1 | 329.43 | HE is missing? Modify VHT STAs to VHT and HE STAs. | As in comment | Rejected  The list was copied from the baseline and the second bullet was added to reflect EHT information. |
| 14117 | 11.20.6.5.1 | 329.39 | VHT Operation Information in Table 9-313 may need to be updated because it is referenced by Wide Bandwidth Channel Switch element | As in comment | Rejected  The comment is not clear and is not specific. The commenter suggest Table 9-313 MAY need to be updated but doesn’t mention how the update should be done or where. |

**CID 10589**

Discussion:

The commenter is referring to the text:

“A TDLS peer STA shall not transmit a 40 MHz PPDU that does not use the primary 40 MHz channel of its 80 MHz, 160 MHz, or 80+80 MHz, or 320 MHz direct link. A TDLS peer STA shall not transmit an 80 MHz PPDU that does not use the primary 80 MHz channel of its 160 MHz or 80+80 MHz, or 320 MHz direct link.”

Agree with the commenter. Rules for 160 MHz transmission in a 320 MHz direct link seem to be missing.

***TGbe Editor: Please make the changes below:***

A TDLS peer STA shall not transmit a 40 MHz PPDU that does not use the primary 40 MHz channel of its 80 MHz, 160 MHz, or 80+80 MHz, or 320 MHz direct link. A TDLS peer STA shall not transmit an 80 MHz PPDU that does not use the primary 80 MHz channel of its 160 MHz or 80+80 MHz, or 320 MHz direct link. A TDLS peer STA shall not transmit a 160 MHz PPDU that does not use the primary 160 MHz of its 320 MHz direct link.

**CID 10845**

Agree with the commenter.

TGbe Editor: Please make changes shown below

A wideband TDLS off-channel TDLS direct link is a 40 MHz, 80 MHz, 160 MHz, or 320 MHz off-channel TDLS direct link for EHT STAs, a 40 MHz, 80 MHz, 160 MHz, or 80+80 MHz off-channel TDLS direct link for VHT and HE STAs or a 2 MHz, 4 MHz, 8 MHz, or 16 MHz off-channel TDLS direct link for S1G STAs.

**References:**