IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11be D2.0 CR for Miscellaneous CIDs IV | | | | |
| Date: 2022-12-19 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Po-Kai Huang | Intel |  |  |  |

Abstract

This submission proposes resolutions for the following CIDs:

10487

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Revised resolution based on the discussion during teleconference.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe D2.0 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe D2.0 Draft. (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 10487 | Eldad Perahia | 35.3.6.2.2 | 426.04 | "An AP MLD may remove one or more of its affiliated APs." In order for 802.11be to support Enterprise use cases, for better management capability, it is required to have a method to temporarily prohibit frame exchanges on links. | as in comment | Revised –  11be has incorporated mechanism for AP MLD to have mandatory TID-to-link mapping in 35.3.7.1.7 (Advertised TID-to-link mapping in Beacon and Probe Response frames) and 35.3.7.3.2 (Affiliated AP link disablement).  *When an AP MLD advertises that a link is disabled for all associated non-AP MLDs, after the time indicated by the Mapping Switch Time field is reached:*  …….  *an EHT (#12242)non-AP STA affiliated with a non-AP MLD that is associated with the AP MLD shall not use the link to transmit individually addressed frames to the AP affiliated with the AP MLD that is operating on a link that is disabled.*  TGbe editor makes changes based on 11-22-1023r5 CID 14054. No further change is required for the current draft. |

**Discussion: None**