IEEE P802.11
Wireless LANs

|  |
| --- |
| LB272 Resolutions for MS Termination MLME |
| Date: May 15, 2023 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Pei Zhou | OPPO |  |  | zhoupei1@oppo.com |
|  |  |  |  |
|  |  |  |  |

Abstract

This submission proposes resolutions to the following LB272 CIDs.

* 1210, 1415, 1416, 1417, 1418, 1419, 1879.

The text used as references are 802.11bf D1.0 and 11-23/0625r1.

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Revised according to Claudio’s offline suggestions.

**Comments:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 1879 | Yonggang Fang | 6.3.136.8.2 | 35.01 | The MeasurementSetupID should not be present if the Termination All TB Measurement Setups parameter or the Termination All non-TB Measurement Setups parameter is set to 1. | Suggest to change "The MeasurementSetupID is present if the Termination All TB Measurement Setups parameter or the Termination All non-TB Measurement Setups parameter is set to 1. " | **Revised.**The mentioned text was already removed according to 11-23-0625-01-00bf-pdt-on-new-clause-6. There is no need to make any change. |
| 1416 | John Coffey | 6.3.136.6.2 | 32.62 | "This parameter is reserved if the Termination All TB Measurement Setups parameter or the Termination All non-TB Measurement Setups parameter is set to 1." What does "reserved" mean here? For example, what is the transmitter supposed to do? | Change "reserved" to "reserved (set to 0 on transmit and ignored on receive)". | **Revised.**The mentioned text was removed according to 11-23-0625-01-00bf-pdt-on-new-clause-6. There is no need to make any change. |
| 1415 | John Coffey | 6.3.136.7.2 | 33.45 | "This parameter is reserved if the Termination All TB Measurement Setups parameter or the Termination All non-TB Measurement Setups parameter is set to 1." What does "reserved" mean here? For example, what is the transmitter supposed to do? | Change "reserved" to "reserved (set to 0 on transmit and ignored on receive)". | **Revised.**The mentioned text was already removed according to 11-23-0625-01-00bf-pdt-on-new-clause-6. There is no need to make any change. |
| 1417 | John Coffey | 6.3.136.6.2 | 34.14 | "This parameter is reserved if the Termination All TB Measurement Setups parameter or the Termination All non-TB Measurement Setups parameter is set to 1." What does "reserved" mean here? For example, what is the transmitter supposed to do? | Change "reserved" to "reserved (set to 0 on transmit and ignored on receive)". | **Revised.**The mentioned text was already removed according to 11-23-0625-01-00bf-pdt-on-new-clause-6. There is no need to make any change. |
| 1418 | John Coffey | 6.3.136.8.2 | 35.05 | "This parameter is reserved if the Termination All TB Measurement Setups parameter or the Termination All non-TB Measurement Setups parameter is set to 1." What does "reserved" mean here? For example, what is the transmitter supposed to do? | Change "reserved" to "reserved (set to 0 on transmit and ignored on receive)". | **Revised.**The mentioned text was already removed according to 11-23-0625-01-00bf-pdt-on-new-clause-6. There is no need to make any change. |
| 1419 | John Coffey | 6.3.136.8.2 | 35.27 | "This parameter is reserved if the Termination All TB Measurement Setups parameter or the Termination All non-TB Measurement Setups parameter is set to 1." What does "reserved" mean here? For example, what is the transmitter supposed to do? | Change "reserved" to "reserved (set to 0 on transmit and ignored on receive)". | **Revised.**The mentioned text was already removed according to 11-23-0625-01-00bf-pdt-on-new-clause-6. There is no need to make any change. |
| 1210 | Solomon Trainin | 6.3.136.8.1 | 34.40 | "... or that the sensing measurement setup(s) are terminated implicitly as the result of the measurement setup expiry timer expired." This timer is an entity used in defining normative behavior. I suggest giving the timer a name so that references to the timer are consistent throughout the spec text. Suggest to name the timer MeasurementSetupExpiry timer. | Change the name as in the comment in all appearances in the draft text. | **Revised.**The mentioned text was already removed according to 11-23-0625-01-00bf-pdt-on-new-clause-6. There is no need to adopt the proposed change in clause 6.3.However, it is needed to change “measurement setup expiry timer” in all appearances in the draft text to “MeasurementSetupExpiry timer”.TGbf Editor make changes as in doc.: 11-23/0529r1. |

***TGbf Editor:*** *Please change the draft text so that references to the “measurement setup expiry timer” are consistent throughout the spec text.*

**SP: Move to approve resolutions to CIDs 1210, 1415, 1416, 1417, 1418, 1419, 1879,**

**as specified in doc.: 11-23/0529r1 and incorporate the text changes into the latest TGbf draft.**