IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB271 CR for 36.2.6 Support for non-HT, HT, VHT, and HE formats | | | | |
| Date: 2023.04.18 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Bo Gong | Huawei Technologies | H3, Huawei Base, Bantian, Longgang, Shenzhen, Guangdong, China, 518129 |  | gongbo8@huawei.com |
| Jian Yu |  | ross.yujian@huawei.com |

Abstract

This submission contains proposed comment resolutions to comments on P802.11be D3.0.

The changes are based on P802.11be D3.0.

This submission provides a resolution to the following CIDs:

* 15023, 15072, 17182, 17183


Revisions:

* Rev 0: Initial version of the document.

## CID 15023

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page.  Line | Clause Number | Comment | Proposed Change | Resolution |
| 687.19 | 36.2.6.1 | "20"MHz is missing in the figure. (in clause 19 and 21 boxes) | add "20"MHz channel width | Revised.  **Instructions to the editor:**  Please add “20” between “on” and “MHz” in the boxes of clause 19 and 21 in Figure 36-1 in Line 19, Page 687 in TGbe Draft D3.0. |

Discussions:



## CID 15072

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page.  Line | Clause Number | Comment | Proposed Change | Resolution |
| 691.10 | 36.2.6.4 | Text missing on "without the PHYCONFIG\_VECTOR DISABLED\_SUBCHANNEL\_BITMAP" | without the PHYCONFIG\_VECTOR parameter DISABLED\_SUBCHANNEL\_BITMAP | Revised.  Agreed in principle. Reflect the detailed explanation.  **Instructions to the editor:**  **Please make the changes as shown in 11/23-0686r0 under CID 17182.**  Note that the resolutions for CID 15072 and CID 17182 are the same. |

## CID 17182

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page.  Line | Clause Number | Comment | Proposed Change | Resolution |
| 691.08 | 36.2.6.4 | First bullet doesn't read right: except that without (...) | Change first bullet to "the PHYCONFIG\_VECTOR DISABLED\_SUBCHANNEL\_BITMAP is ignored" | Revised.  Agreed in principle. Reflect the detailed explanation.  **Instructions to the editor:**  **Please make the changes as shown in 11/23-0686r0 under CID 17182.**  Note that the resolutions for CID 15072 and CID 17182 are the same. |

**Instructions to the Editor:**

Please make the following changes in Line 10, Page 691in TGbe Draft D3.0:

On receipt of a PHY-CONFIG.request(PHYCONFIG\_VECTOR) primitive, the EHT PHY behaves, for the  
purposes of VHT PPDU transmission and reception, as if it were a Clause 21 (Very High Throughput (VHT)  
PHY specification) PHY that received the PHY-CONFIG.request(PHYCONFIG\_VECTOR) primitive  
except that:  
— the PHYCONFIG\_VECTOR parameter DISABLED\_SUBCHANNEL\_BITMAP is ignored  
— the CHANNEL\_WIDTH parameter, if it is equal to 320 MHz, is replaced by 160 MHz  
— the CENTER\_FREQUENCY\_SEGMENT\_0 parameter, if the CHANNEL\_WIDTH parameter is  
equal to 320MHz, is replaced by the center of the primary 160 MHz channel.

## CID 17183

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page.  Line | Clause Number | Comment | Proposed Change | Resolution |
| 691.43 | 36.2.6.4 | First bullet doesn't read right: except that without (...) | Change first bullet to "the PHYCONFIG\_VECTOR DISABLED\_SUBCHANNEL\_BITMAP is ignored" | Revised.  Agreed in principle. Reflect the detailed explanation.  **Instructions to the editor:**  **Please make the changes as shown in 11/23-0686r0 under CID 17183.** |

**Instructions to the Editor:**

Please make the following changes in Line 45, Page 691in TGbe Draft D3.0:

On receipt of a PHY-CONFIG.request(PHYCONFIG\_VECTOR) primitive, the EHT PHY behaves, for the  
purposes of HE PPDU transmission and reception, as if it were a Clause 27 (High Efficiency (HE) PHY  
specification) PHY that received the PHY-CONFIG.request(PHYCONFIG\_VECTOR) primitive except  
that:  
— the PHYCONFIG\_VECTOR parameter DISABLED\_SUBCHANNEL\_BITMAP is ignored  
— the CHANNEL\_WIDTH parameter, if it is equal to 320 MHz, is replaced by 160 MHz  
— the CENTER\_FREQUENCY\_SEGMENT\_0 parameter, if the CHANNEL\_WIDTH parameter is  
equal to 320 MHz, is replaced by the center of the primary 160 MHz channel.