**IEEE P802.11  
Wireless LANs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB266 CR for 35.3.16.5 (PPDU end time alignment) | | | | |
| Date: 2023-06-18 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Yongho Seok | Mediatek |  |  | yongho.seok@mediatek.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for multiple comments related to TGbe D3.0 with the following CIDs ( 2 CIDs):

* 16882

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the subsequent TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| --- | --- | --- | --- | --- | --- |
| 16882 | 35.3.16.5.1 | 555.59 | "the timing margin is set to half of SIFS" -- but SIFS is 10 us in the 2G4 band | Change to "the timing margin is set to half of (non-2.4 GHz) SIFS" | Revised-  Agree in principle.  TGbe editor: In the NOTE2 of 35.3.16.5.1 (General), replace  “SIFS” with  “aSIFSTime + aSignalExtension” |
| 15828 | 35.3.16.5.1 | 555.35 | "When more than one AP affiliated with AP MLD simultaneously transmits to the non-AP STAs..." is grammatically inconsistent | Replace with "When more than one Aps affiliated with an AP MLD simultaneously transmit to the non-AP STAs..." | Revised-  TGbe editor: Replace "When more than one AP affiliated with AP MLD simultaneously transmits to the non-AP STAs..." with "When more than one AP affiliated with an AP MLD simultaneously transmit to the non-AP STAs..." |