### **IEEE P802.11 Wireless LANs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Miscellaneous Comment Resolutions | | | | |
| Date: 2023-05-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Brian Hart | Cisco Systems |  |  | brianh@cisco.com |
|  |  |  |  |  |
|  |  |  |  |  |

**Abstract**

CIDs 4013, 4023, 4014

**Revisions:**

* Rev 0: Initial version of the document.

***TGme editor: Please note Baseline is 11me D3.0. Edits are expressed via Word track changes:***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 4013 | Table 9-34expresses units in the title of the table, which is non-traditional (i.e., easy to miss) and not as precise as could be | 621 | 9.2.4.8.1 | 1 | Dete "(octets)" and "in microseconds" from table header, and instead add these as labels to each row (i.e. all rows are octets except the last which is microseconds) | Accepted |

*For context:*

**Table 9-34—Maximum data unit sizes and durations**

|  |  |  |
| --- | --- | --- |
|  | Non-HT non-VHT non-HE(11ax) non-S1G non-DMG PPDU and non-HT duplicate PPDU | … |
| … | … | … |
| PSDU size (octets) | xx | … |
| PPDU duration (microseconds) | xx | … |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 4023 | 12.2.10 lays out the opportunities and requirements for non-AP STAs seeking privacy (i.e., with dot11MACPrivacyActivated equal to true) including some minimal behaviors to assure expected/usual ESS behavior. In reality, these minimal behaviors apply equally to non-AP STAs not seeking privacy. This second class of STAs will naturally tend to follow the same minimal behaviors yet this is not required since the associated language is omitted via the current narrow text: "MAC privacy enhancements are enabled on a non-AP STA when dot11MACPrivacyActivated is set to true ... The STA ...". The current language on minimal behaviors should be generalized to include clients not seeking privacy. | 2790 | 12.2.10 | 58 | Change "The" to "A" at P2790L58. Change "The" to "A" at P2790L60.5. | Revised. Changes substantially in line with the comment are made in 23/0831r<motionedRev> |

***TGme editor, make the following changes under CID 4023***

12.2.10 Requirements for support of MAC privacy enhancements

MAC privacy enhancements are enabled on a non-AP STA when dot11MACPrivacyActivated is set to true.

…

A non-AP STA connecting to an infrastructure BSS shall retain a single MAC address for the duration of its connection across an ESS. A PMKSA created as part of an RSNA will contain the MAC address used to create the PMKSA. A non-AP STA that supports PMKSA caching shall, if necessary, change its MAC address back to that value when attempting a subsequent association to the ESS using PMKSA caching.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 4014 | The definition of the VHT Maximum MPDU Length field has been used and abused, and is not actually the max MPDU length for HE compressed feedback. HE has a workaround in 26.7.1, but it is weak since it leaves the text here as an invalid and misleading definition. | 1223 | 9.4.2.156.2 | 10 | Change to "Indicates the maximum MPDU length that the STA is capable of receiving (see 10.11 (A-MSDU operation)) \*, excluding an HE compressed beamforming/CQI Report frame (see 26.7.1 (General))\* Note that this change also addresses the Maximum MPDU Length field defined in Figure 9-901, since that is defined by xref back to this table. | Revised. Changes substantially in line with the comment are made in 23/0831r<motionedRev> |

***Discussion***

This comment resolution blew up to address all sounding feedback, and associated terms. We make changes in three Parts (each with its own change-text)

***Part A: get the terms correct:***

We have five somewhat related, defined terms:

|  |
| --- |
| * In 9.4.1.47 VHT Compressed Beamforming Report field:   **VHT Compressed Beamforming Report information** (Table 9-103)   * In 9.4.1.60 CMMG Compressed Beamforming Report field   **CMMG Compressed Beamforming Report** field   * In 9.4.1.63 HE Compressed Beamforming Report field   **HE Compressed Beamforming Report information** (Table 9-121)   * In 10.35.5.2 Rules for VHT sounding protocol sequences:   **VHT compressed beamforming feedback** comprises the VHT Compressed Beamforming Report information (see Table 9-103 (VHT Compressed Beamforming Report information)) and the MU Exclusive Beamforming Report information (see Table 9-106 (MU Exclusive Beamforming Report information)). Subclause 9.6.22.2 (VHT Compressed Beamforming frame format) specifies how VHT compressed beamforming feedback is converted into a VHT Compressed Beamforming frame, and it also specifies the rules for the presence or absence of the two fields listed here.   * In 26.7.1 General:   The HE beamformee returns an estimate of the channel state in an **HE compressed beamforming/CQI report** carried in one or more HE Compressed Beamforming/CQI frames. There are three types of HE compressed beamforming/CQI report:   * SU feedback: The HE compressed beamforming/CQI report consists of an HE Compressed Beamforming Report field. * MU feedback: The HE compressed beamforming/CQI report consists of an HE Compressed Beamforming Report field and HE MU Exclusive Beamforming Report field. * CQI feedback: The HE compressed beamforming/CQI report consists of an HE CQI Report field. |

Editorial comment CID317 changed “VHT/CMMG Compressed Beamforming report" to “VHT/CMMG Compressed Beamforming report information" but, since this relates to segments, this should be changed to “VHT/CMMG compressed beamforming feedback” instead. In general, we find that undefined terms (using similar words) are used and should be replaced by defined terms:

***TGme editor: change the following under CID 4014:***

***P661L12:***

The Feedback Segment Retransmission Bitmap field indicates the requested feedback segments of VHT compressed beamforming feedback

***P671L27:***

The Feedback Segment Retransmission Bitmap subfield indicates the requested feedback segments of an HE compressed beamforming/CQI report.

***P820L1***

The CMMG Compressed Beamforming Report field has the structure defined in Table 9-116 (CMMG Compressed Beamforming Report field), where Na is the number of angles used for the CMMG compressed beamforming feedback matrix.

Table 9-116—CMMG Compressed Beamforming Report field

***P820L37:***

Ns is the number of subcarriers for which the CMMG compressed beamforming feedback matrix is sent back to the CMMG beamformer. Ns is a function of the Channel Width and Grouping subfields in the CMMG MIMO Control field. Table 9-117 (Subcarrier indices for which a compressed beamforming feedback matrix is sent back) lists Ns, the exact subcarrier indices and their order for which the CMMG compressed beamforming feedback matrix is sent back. No padding is present between angles in the CMMG Compressed Beamforming Report field, even if they correspond to different subcarriers. If the length of the CMMG Compressed Beamforming Report field is not an integral multiple of 8 bits, up to 7 0s are appended to the end of the field to make its size an integral multiple of 8 bits.

***P823L39/50:***

Table 9-119—Subfield values of the CMMG Operating Mode field

|  |  |
| --- | --- |
| Subfield | Description |
| RX NSS | If the RX NSS Type subfield is 0, indicates the maximum number of spatial streams that the STA can receive. If the RX NSS Type subfield is 1, indicates the maximum number of spatial streams that the STA can receive as a beamformee in an SU PPDU using a beamforming steering matrix derived from a CMMG Compressed Beamforming Report field(#317) with the Feedback Type subfield indicating SU in the corresponding CMMG Compressed Beamforming frame sent by the STA. Set to 0 for NSS = 1 Set to 1 for NSS = 2 … Set to 3 for NSS = 4 |
| RX NSS Type | Set to 0 to indicate that the RX NSS subfield carries the maximum number of spatial streams that the STA can receive. Set to 1 to indicate that the RX NSS subfield carries the maximum number of spatial streams that the STA can receive in an SU PPDU using a beamforming steering matrix derived from a CMMG Compressed Beamforming Report field(#317) with the Feedback Type subfield indicating SU in the corresponding CMMG Compressed Beamforming frame sent by the STA. NOTE—An AP always sets this field to 0. |

***P834L51:***

the Average SNR of Space-Time Stream i field of the HE Compressed Beamforming Report information

***P2044L4:***

NOTE 2—The feedback segments of VHT compressed beamforming feedback(#317) are not MSDU/MMPDU fragments.***P3667L3:***

The Feedback Segment Retransmission Bitmap field indicates the feedback segments to be polled in VHT compressed beamforming feedback (#317)

***P3895L47***

The HE compressed beamforming/CQI report is carried in a single HE Compressed Beamforming/CQI frame if the resulting frame is less than or equal to 11 454 octets in length (see 26.7.3 (Rules for HE sounding protocol sequences)). Otherwise, the HE compressed beamforming/CQI report is segmented, and each segment is carried in an HE Compressed Beamforming/CQI frame.

***P3904L1:***

An HE beamformee that transmits HE compressed beamforming/CQI report shall include neither the HE Compressed Beamforming Report information nor the HE MU Exclusive Beamforming Report information if the transmission duration of the PPDU carrying the HE Compressed Beamforming Report information and any HE MU Exclusive Beamforming Report information would exceed the maximum PPDU duration.

***Part B: clarify that segments are part of an MMPDU.***

***(TGme editor: change-text from Part A has been Word-change-accepted in the following for clarity, but these kind of changes are not intended to change or override whatever Word-changes are agreed in Part A)***

***P2043L52:***

10.35.5.3 Rules for fragmented feedback in VHT sounding protocol sequences

If VHT compressed beamforming feedback would result in a VHT Compressed Beamforming frame that exceeds the VHT beamformer’s maximum MPDU length capability, the VHT compressed beamforming feedback shall be split into up to 8 feedback segments, with each feedback segment sent in a different VHT Compressed Beamforming frame and containing successive portions of the VHT compressed beamforming feedback consisting of the VHT Compressed Beamforming Report information followed by any MU Exclusive Beamforming Report information. Each of the feedback segments except the last shall be transmitted in a frame that contains the maximum number of octets allowed by the VHT beamformer’s maximum MPDU length capability. The last feedback segment may be transmitted in a smaller frame. Each feedback segment is identified by the value of the Remaining Feedback Segments subfield and the First Feedback Segment subfield in the VHT MIMO Control field as defined in 9.4.1.46 (VHT MIMO Control field); the other nonreserved subfields of the VHT MIMO Control field shall be the same for all feedback segments. All feedback segments shall be sent in a single A-MPDU and shall be included in the A-MPDU in the descending order of the Remaining Feedback Segments subfield values.

NOTE 2—The feedback segment of VHT compressed beamforming feedback(#317) are not MSDU/MMPDU fragments, rather each feedback segment, together with the other fields in the Frame Body field of the VHT Compressed Beamforming frame (see Figure 9-120 (Management frame format) and 9.6.22.2 (VHT Compressed Beamforming frame format)), constitute a single unfragmented MMPDU.

26.7.1 General

An HE beamformer shall support a maximum MPDU length for a frame containing the HE compressed beamforming/CQI report, that is the minimum of 11 454 octets and the maximum length of the frame containing the HE compressed beamforming/CQI report that the HE beamformer intends to solicit from its HE beamformees.

26.7.4 Rules for generating segmented feedback

If the HE compressed beamforming/CQI report solicited by the HE beamformer would result in an HE Compressed Beamforming/CQI frame that exceeds 11 454 octets in length, then the HE compressed beamforming/CQI report shall be split into up to 8 feedback segments. Each feedback segment shall be included in a separate HE Compressed Beamforming/CQI frame and shall contain successive segments of the HE compressed beamforming/CQI report. Each feedback segment shall be of equal length, except the last feedback segment that may be smaller. Each HE Compressed Beamforming/CQI frame that includes a feedback segment that is not the last feedback segment shall have a length of 11 454 octets. Each feedback segment is identified by the value of the Remaining Feedback Segments subfield and the First Feedback Segment subfield in the HE MIMO Control field as defined in 9.4.1.62 (HE MIMO Control field(11ax)); the other nonreserved subfields of the HE MIMO Control field shall be the same for all feedback segments. All feedback segments shall be sent in a single A-MPDU contained in a PPDU and shall be included in the A-MPDU in the descending order of the Remaining Feedback Segments subfield values.

***TGbe editor: immediately following this para, insert the following NOTE and renumber all notes in this section accordingly***

NOTE 0—A feedback segment of the HE compressed beamforming/CQI report together with the other fields in the Frame Body field of the HE Compressed Beamforming/CQI frame (see Figure 9-120 (Management frame format) and Table 9-618(HE Compressed Beamforming/CQI frame Action field format), constitute a single unfragmented MMPDU.

***Part C: update Table 9-34 (Maximum data unit sizes (in octets) and durations (in microseconds) and clarify role of Maximum MPDU Length in VHT Capabilities element***

|  |
| --- |
| ***Part C discussion***  Reviewing all the sounding feedback   * 10.33, 10.35: HT sounding feedback (CSI/compressed/non-compressed) feedback can reach:   + PPDU     - Implicit sounding: “The procedures for HT transmit beamforming with implicit feedback use only HT and non-HT PPDU”     - Explicit sounding: “The procedures in this subclause apply only to HT and non-HT PPDUs”   + MMPDU     - CSI/uncompressed: Category + HT Action + MIMO Control + CSI = 1 + 1 + 6 + 4\*1 + ceil(114\*(3+2\*4\*4\*8)/8) = 3703 octets.     - Compressed: Category + HT Action + MIMO Control + Compressed = 24 + 4 + 1 + 1 + 6 + 4\*1 + ceil(114\*(12\*(4+6)/2)/8) = 895 octets (a non-factor)     - But, from Table 9-34, Non-HT and HT MMPDUs are limited to 2304 octets, so need to clarify that there is an exception for HT CSI/uncompressed feedback.   + MPDU:     - MAC header + ?HT Control + Category + HT Action + MIMO Control + CSI + FCS = 24 + 4 + 1 + 1 + 6 + 4\*1 + ceil(114\*(3+2\*4\*4\*8)/8) + 4 = 3735 octets.     - Table 9-34, Note 5 says “No direct constraint on the maximum MPDU size; indirectly constrained by the maximum A-MSDU size” but HT sounding feedback is not contained in an A-MSDU. Need to clarify that it is also constrained by max MMPDU size * 10.33.4, 10.35.5/6: VHT sounding feedback is large but, especially after Part B changes, segmented each segment is limited to the maximum number of octets allowed by the VHT beamformer’s maximum MPDU length capability from 10.35.5.3 (Rules for fragmented feedback in VHT sounding protocol sequences). Also Note 1 in Table 9-34 says “NOTE 1—No direct constraint on the maximum MMPDU size; indirectly constrained by the maximum MPDU size (see 9.3.3.1 (Format of (PV0) Management frames)).” Assume that the payload of each segment is an MMPDU, now made explicit.   + PPDU     - From 10.35.5.3, unsegmented or segmented, segments are sent in an A-MPDU, which means a HT or VHT or HE PPDU. The language “allowed by the VHT beamformer’s maximum MPDU length capability” works quite well for each PPDU format (undeclared for HT, declared for VHT and HE), although this “capability” is based on different sub-capabilites (for HT, VHT, etc). Note: AFAIK there is nothing to stop VHT sounding feedback from being sent (unsegmented or segmented) in an HT or HE PPDU **– but that seems to be fine??**   + MMPDU and MMPDU     - So MPDU length is fine, and MMPDU length is fine given VHT and HE are covered by “Table 9-34/NOTE 1—No direct constraint on the maximum MMPDU size; indirectly constrained by the maximum MPDU size (see 9.3.3.1 (Format of (PV0) Management frames)).” * 26.7: HE sounding feedback is segmented again, but now MPDUs up to 11454 octets could be required, and commensurately large MMPDUs.   + PPDU     - Non-TB sounding: same as VHT – unsegmented or segmented; segments are sent in an A-MPDU, which means HT, VHT or HE … This doesn’t seem like it should be allowed, since no one expects 11454 octets for HT!!??     - TB- sounding – uses HE TB PPDU   + MMPDU     - Fine – same as VHT   + MPDU     - Up to 11454 octets, if needed |

Table 9-34—Maximum data unit sizes (in octets) and durations (in microseconds)(#1327)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Non-HT non-VHT non-HE(11ax) non-S1G non-DMG PPDU and non-HT duplicate PPDU | HT PPDU | VHT PPDU | HE PPDU(11ax) |
| MMPDU size | 2304 or higher as identified by NOTE 10 | 2304 or higher as identified by NOTE 11 | See NOTE 1 | See NOTE 1 |
| MPDU size | See NOTE 4 | See NOTE 5 | 3895 or 7991 or 11 454 (see also Table 9-311 (Subfields of the VHT Capabilities Information field) or higher as identified by NOTE 7) | 2.4 GHz band: see NOTE 5.  Otherwise: 3895 or 7991 or 11 454 (see Table 9-311 (Subfields of the VHT Capabilities Information field)and NOTE 7) |
| NOTE 1—No direct constraint on the maximum MMPDU size; indirectly constrained by the maximum MPDU size (see 9.3.3.1 (Format of (PV0) Management frames)).  NOTE 4—No direct constraint on the maximum MPDU size; indirectly constrained by the maximum MSDU, MMPDU or (for HT STAs only) A-MSDU size.  NOTE 5—No direct constraint on the maximum MPDU size; indirectly constrained by the maximum A-MSDU size and (if present) the maximum MMPDU size else the maximum PPDU size.  NOTE 7—The maximum MPDU size might be greater than the size declared as supported by the recipient if the MPDU is an HE Compressed Beamforming/CQI frame.(11ax)  NOTE 10—The maximum MMPDU size might be greater than 2304 octets if the MMPDU is carried in a CSI frame (see 9.6.11.4 (CSI frame format)) or a Compressed Beamforming frame (see 9.6.11.6 (Compressed Beamforming frame format)).  NOTE 11—The maximum MMPDU size might be greater than 2304 octets if the MMPDU carried in a CSI frame (see 9.6.11.4 (CSI frame format)), a Compressed Beamforming frame (see 9.6.11.6 (Compressed Beamforming frame format)) or a HE Compressed Beamforming/CQI frame (see 9.6.31.2 (HE Compressed Beamforming/CQI frame format)). | | | | |

**Table 9-311—Subfields of the VHT Capabilities Information field**

|  |  |  |
| --- | --- | --- |
| **Subfield** | **Definition** | **Encoding** |
| Maximum MPDU Length | Indicates the maximum MPDU length that the STA is capable of receiving (see 10.11 (A-MSDU operation)), excepting that a higher maximum MPDU length might be required for the frames listed in NOTE 7 in Table 9-34 (Maximum data unit sizes (in octets) and durations (in microseconds)). | Set to 0 for 3895 octets.  Set to 1 for 7991 octets.  Set to 2 for 11 454 octets.  The value 3 is reserved |

|  |
| --- |
| ***Note to reader: no change is needed to the draft for 6 GHz since this is defined by xref to the table modified above:***  **9.4.2.262 HE 6 GHz Band Capabilities element**  The Maximum A-MPDU Length Exponent subfield and Maximum MPDU Length subfield are defined in (#2317)Table 9-311 (Subfields of the VHT Capabilities Information field) |

10.35.5.1 General

***Since this definition is widely used and before where it was defined, insert the following as a new last paragraph (copied exactly from the old para in 10.35.5.2***

VHT compressed beamforming feedback comprises the VHT Compressed Beamforming Report information (see Table 9-103 (VHT Compressed Beamforming Report information)) and the MU Exclusive Beamforming Report information (see Table 9-106 (MU Exclusive Beamforming Report information)). Subclause 9.6.22.2 (VHT Compressed Beamforming frame format) specifies how VHT compressed beamforming feedback is converted into a VHT Compressed Beamforming frame, and it also specifies the rules for the presence or absence of the two fields listed here.

10.35.5.2 Rules for VHT sounding protocol sequences