IEEE P802.11
Wireless LANs

|  |
| --- |
| CR for miscellaneous CIDs |
| Date: 2023-06-23 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Yunbo Li | Huawei |  |  | liyunbo@huawei.com |
| Ming Gan |  |  |  |  |
| Yuchen Guo |  |  |  |  |
| Guogang Huang |  |  |  |  |
| Yue Zhao |  |  |  |  |
| Zhenguo Du |  |  |  |  |
| Stephen McCann |  |  |  |  |
| Edward Au |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes comment resolution(s) for the following 3 CID(s) received in LB271 on TGbe D3.2

CIDs: 16293, 18320, 18323

Revisions:

* Rev 0: Initial version of the document.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause**  | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 16293 | Pascal VIGER | 9.2.4.6.4 | 140.10 | QoS Characteristics element provides parameters that describe traffic characteristics (within the SCS procedure), especially the low latency (LL) parameters, so that AP shall be able to create an optimal schedule .Unfortunatly, it is well known that such traffic is never well specified and does not inform the real amount of LL at a given time inside buffer's STA.An updated BSR shall be provided for Latency Sensitive data | An updated BSR Control shall inform the AP scheduler of an amount of data with regards to a timing indication, which provides the expected date for delivery (e.g. UL trigger). This greatly helps the AP scheduling UL RUs accordingly (date and size). | RejectedA proposed resolution for this CID was discussed as part of the comment resolutions in https://mentor.ieee.org/802.11/dcn/22/11-22-1454-02, however the group could not reach consensus on the proposed change. |
| 18320 | Rubayet Shafin | 35.3 | 479.01 | Power saving operation for NSTR Mobile AP MLD is not clear from the current spec. | Please provide clarifying text on STA and AP side behavior on this. | RejectedThis topic was discussed during the previous rounds of comment resolution. However, the group could not reach consensus on this. See doc 11-22/356 for prior discussion on this. |
| 18323 | Rubayet Shafin | 35.3 | 479.01 | 2-links restriction for mobile AP MLD is quite limiting and needs to be generalized. | As in comment | RejectedThis topic was discussed during last round of comment resolution. The group fail to reach consensus on supporting more than 2 links for a NSTR mobile AP MLD in 11be. E.g. see  <https://mentor.ieee.org/802.11/dcn/22/11-22-1793-06-00be-nstr-mobile-ap-miscellaneous-cids.docx>  |

Discussion:

1. **Proposed spec text**

***TGbe editor: Please make the following changes in subclause :***