IEEE P802.11
Wireless LANs

|  |
| --- |
| LB271 CR for 16118 |
| Date: 2023-07-11 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Shawn (Sanghyun) Kim | WILUS Inc. | 216 Hwangsaeul-ro, Seongnam-si, Gyeonggi-do, Korea |  | shawn.kim@wilusgroup.com |
| Greg Geonjung Ko | greg.ko@wilusgroup.com |
| John(Ju-Hyung) Son | john.son@wilusgroup.com |
| Jin Sam Kwak | jinsam.kwak@wilusgroup.com |

This document proposes resolution to the following LB271 CID (changes relative to draft 3.2):

16118

Revisions:

* Rev0: Initial version of the document.
* Rev1: EMLMR delay => EMLMR transition delay, EMLMR Delay subfield => EMLMR Transition Delay subfield

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 16118 | 620 | 45 | 35.8.5.1 | The point at which a non-AP STA in EMLSR mode begins switching back operation is at the end of the frame exchange. Since the end of frame exchange for a non-AP STA in EMLSR mode is TXOP end time + aSIFSTime + aSlotTime + aRxPHYStartDelay, we need to verify whether the 'T' for EMLSR should be EMLSR transition delay + aSIFSTime + aSlotTime + aRxPHYStartDelay. | As in comment | **Reject**This topic was discussed in TGbe group (23/1060r2) and the group could not reach consensus. |