IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for Misc CIDs | | | | |
| Date: 2023-07-08 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Dibakar Das | Intel |  |  | Dibakar.das@intel.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for following CIDs:

16734 15878

Revisions:

* Rev 0: Initial version.

The changes are relative to 11be draft 3.2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Comment | Proposed Change | Resolution |
| 15878 | 35.3.16.8.1 | 560.61 | "As described above" doesn't explain well how to update the timer. During the transmission of interest, is the timer (the "previous MediumSyncDelay") still running? | Add corresponding description. | **Reject.**  The timer is still running which is clear since there is no spec language saying its not. There is only a single instance of the word “update” before this paragraph in this section, so the reference on how to update is unambiguous. |
| 16734 | 35.2.1.2.3 | 477.55 | "shall not  be used by the non-TB PPDU(s) that is transmitted during the time allocated by an associated AP" could be worded better, and this applies to all the PPDUs since they are required to be non-TB above | Change to "shall not be used by PPDU(s) transmitted during the time allocation" | **Accept.** |