|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for CIDs in annex B | | | | |
| Date: 2023-7-10 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Jay Yang | ZTE Corporation |  |  | Yang.zhijie@zte.com.cn |
| Yan Li | ZTE Corporation |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for the following CIDs:

**110,152**

R0: initial the draft

R1: minor change according to the feed back from the group

R2: Incorporate the proposed change from Robert on CID110.

R3: minor change according to the feedback during the call in 1st Aug.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbh D1.0 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbh D1.0 Draft. (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbh Editor: Editing instructions preceded by “TGbh Editor” are instructions to the TGbh editor to modify existing material in the TGbh draft. As a result of adopting the changes, the TGbh editor will execute the instructions rather than copy them to the TGbh Draft.***

|  |  |  |  |
| --- | --- | --- | --- |
| **CID** | **Comment** | **Proposed Change** | **Resolution** |
| 110 | The PICS shows both Device ID & IRM to be both CFCMA:O. My  interpretation is that both protocol capabilities are optional.  Perhaps this was not intentional. | Clarify or fix | Revised--   Device ID and IRM are two separate and optional features,  PICS should reflect the feature set and thus should have two entries, one for each feature.  TGbh editor: Incorporate the proposed change in 1250r3 |
| 152 | Referring to PC34 in the Status for IUT configuration item is not appropriate. | Remove "PC34 AND" from the Status for CFCMA.  Add a new row for PC34 to the table under B.4.4.1 and add Status "CFCMA:M" in the added row. | Rejected--  PC34:O in the IUT configuration follows the writing style in 11az specification(in B.4.3 IUT configuration CFPASN Support for PASN 12.13 PC34:O), no further change on this part. |

**TGbh edit: use the following table to replace the table in B.4.3.1 MAC protocol capabilities, and delete the table in B.4.4 MAC protocol**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **IUT configuration** | **References** | **Status** | **Support** |
| CFDID | Device ID indication | 12.2.11.1 ( Device ID indication) | PC34 AND CFAP:O  PC34 AND CFSTAofAP:O | Yes o No o |
| CFIRM | IRM operation | 12.2.11.2 (IRM operation) | PC34 AND CFAP:O  PC34 AND CFSTAofAP:O | Yes o No o |